**Coordination**

Contract Documents must clearly define and specify responsibilities to furnish rough-in, cable installation, and connections. Tasks shall be performed as follows:

1. Outlet boxes shall be installed by the Electrical Contractor
2. Underground conduits leading into the MDF room shall be installed by the Electrical Contractor
3. Empty raceway shall be installed by Electrical Contractor
4. Punch down blocks shall be installed by the Data Cable Installation Contractor
5. Equipment racks shall be installed by the Telecommunications Contractor
6. Horizontal and riser data cable shall be installed by the Telecommunications Contractor
7. RJ45 jacks shall be installed by the Telecommunications Contractor
8. Patch panels shall be installed by the Telecommunications Contractor
9. RJ34 connectors shall be installed by the Telecommunications Contractor
10. Type F connectors for video coaxial cable shall be installed by the Telecommunications Contractor.