|  |  |  |  |
| --- | --- | --- | --- |
| Reference Number: | 15-C-038 | Release Date: | 20. July 2015 |
| GWM-Number: | E150052 | Revision: | 01 |

# Symptom Description

Tailgate descends.

# Cause

Gas strut at left hand side leaky - slow pressure loss until totally loss of gas pressure / force.

# Scope

Insignia Station Wagon - MY 2009 - 2015

|  |  |  |  |
| --- | --- | --- | --- |
| Model | Plant | From | To |
| Insignia | Ruesselsheim | 9 1 000329 | F 1 036034 |

Only vehicles with power tailgate (RPO code: TB5) marked “open” in GWM have to be reworked.

# Remedy

Replace LH tailgate gas pressure strut.

* See working procedure “Liftgate Strut Replacement (Hatchback and Wagon)”, group “Body Repair / Bolted Exterior Body Panels and Closures”, in the Service Instruction Insignia
* (Document Number **92198872**)

# Parts

|  |  |  |
| --- | --- | --- |
| Qty | Part Name | Part No. |
| 1 | Tail Gate Strut, LH | 39 011 536 |

# Labour Operation Claiming

Labour codes mentioned below will be accepted without any time or mileage limit.

|  |  |  |
| --- | --- | --- |
| Number | Labour Description | Hrs |
| 9101439 | Replace the left side tailgate gas pressure strut | 0.3 |
| 9101440 | Vehicle already reworked | 0 |