|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Product Name:** | |  | | **Batch Number:** |  |
| **Machine #:** |  | | **Checklist Issued By/Date:** | |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Step** | **Activity** | **Initials** | **Date** |
| **1** | Verify all approvals have been obtained |  |  |
| **2** | Verify all calibrations are current |  |  |
| **3** | Turn the compressed air supply to the Blender “**ON**” and verify the pressure is at least 90 psig |  |  |
| **4** | Install the gasket for the access lid opening and install/secure the access lid |  |  |
| **5** | Install the gasket for the drum charging/discharge valve |  |  |
| **6** | Close the discharge valve (two technicians required) |  |  |
| **7** | Check the Drum tray - Lifting/Lowering mechanism |  |  |
| **8** | Check the Blender rotation |  |  |
| **9** | Check the Discharge valve – Open / Close mechanism |  |  |
| **10** | Check that the Light curtain sensor is functioning |  |  |

|  |  |
| --- | --- |
| Comments: |  |
|  | |
|  | |
|  | |

|  |  |  |  |
| --- | --- | --- | --- |
| Supervisor/designee: |  | Date: |  |