Tight tolerances on pitch and dual sided contours for precise termination.

Designed to integrate with today’s High Density type connectors for internal wiring of class 2 circuits in electronic equipment.

UL and CSA approved (cable is printed UL/CSA). Stranded construction for ease of routing and longer flex cycles.

Semi-Rigid PVC (series 23262) designed for today’s new high speed termination machinery, offering tight tolerances and rugged construction. See Part No. 23113-080 for an Ultra ATA compliant cable.

UL Listing: CSA Listing:

2678 AWM I A/B FT-1

UL Voltage Rating: CSA Voltage Rating:

150V 300V

UL Temperature: CSA Temperature:

105° C 105° C

Series No. Conductor Stranding coating Insulation

Conductor Resistance @ 20° C

Capacitance Impedance Prog. Delay

(G-S) (G-S-G) (G-S-G) SE (G-S) SE ns/ft.

Skew ns/ft.

23113 30 AWG

7/38 Tinned

PVC 106 Ohms /Mft. 15.8 pF/ft. 23.3 pF/ft. 75 (Ohms) 110 (Ohms)

1.62 .030 (Max.)

23262 30 AWG

7/38 Tinned

SR-PVC 106 Ohms /Mft. 15.44 pF/ft. 22.5 pF/ft. 75 (Ohms) 110 (Ohms)

1.54 .034 (Max.)

Physical construction description: This Microzip construction uses a 30 AWG stranded tinned conductor. Conductors are then pulled parallel and fully extruded with PVC (23113 Series) or SR-PVC (23262 Series) insulation. A red polarity stripe is added to the first conductor for easy identification. Standard color is Gray.

Part No. HCM Configuration Insulation

No. of Cond.

Width "W" Span "S" Pitch Tolerance

Standard Put-ups 23113-010 A3007-51-10T AWM/CSA PVC 10 0.250" 0.225" ± .005" ± .0016" 100’ 23113-016 A3007-51-16T AWM/CSA PVC 16 0.400" 0.375" ± .005" ± .0016" 100’ 23113-020 A3007-51-20T AWM/CSA PVC 20 0.500" 0.475" ± .005" ± .0016" 100’ 23113-026 A3007-51-26T AWM/CSA PVC 26 0.650" 0.625" ± .005" ± .0016" 100’ 23113-030 A3007-51-30T AWM/CSA PVC 30 0.750" 0.725" ± .005" ± .0016" 100’ 23113-034 A3007-51-34T AWM/CSA PVC 34 0.850" 0.825" ± .005" ± .0016" 100’ 23113-040 A3007-51-40T AWM/CSA PVC 40 1.000" 0.975" ± .005" ± .0016" 100’ 23113-050 A3007-51-50T AWM/CSA PVC 50 1.250" 1.225" ± .005" ± .0016" 100’, 200’ & 400’ 23113-060 A3007-51-60T AWM/CSA PVC 60 1.500" 1.475" ± .005" ± .0016" 100’ 23113-064 A3007-51-64T AWM/CSA PVC 64 1.600" 1.575" ± .005" ± .0016" 100’ 23113-068 A3007-51-68T AWM/CSA PVC 68 1.700" 1.675" ± .005" ± .0016" 100’, 200’ & 400’ 23113-080 A3007-51-80T AWM/CSA PVC 80 2.000" 1.975" ± .005" ± .0016" 100’ 23113-100 A3007-51-100T AWM/CSA PVC 100 2.500" 2.475" ± .007" ± .0020" 100’ 23262-050 B3007-51-50T AWM/CSA SR-PVC 50 1.250" 1.225" ± .005" ± .0016" 400? 23262-068 B3007-51-68T AWM/CSA SR-PVC 68 1.700" 1.675" ± .005" ± .0016" 400’

Other conductor counts available upon request. 10