Tight tolerances on .025" pitch flat ribbon cable. Stranded conductor TPO construction for enhanced performance over PVC.

UL and CSA approved (cable is printed UL/CSA). Compliant for today’s new high speed termination machinery, offering tight tolerances on pitch and span. A low cost alternative to the costly FEP cables.

See Part No. 20009-068 & 20021-068 for SCSI Fast-20/40/80 and 160 compliant cables. See Part No. 23196-080 for an Ultra ATA compliant cable.

UL Listing: 20848 UL Voltage Rating: 30V UL Temperature: 105° C CSA Listing: AWM I A/B FT-1 CSA Voltage Rating: 300V CSA Temperature: 105° C

Series No. Conductor Stranding Coating Insulation

Conductor Resistance @

20° C

Capacitance Impedance

Propagation Delay

(G-S) (G-S-G)

(G-S-G) SE (G-S) SE ns/ft.

Skew ns/ft

23196 30 AWG

7/38 Tinned

Thermo- Plastic Olefin 106 Ohms/Mft

8.8 pF/ft 15.7 pF/ft 77 Ohms 118 Ohms 1.44 .030 (Max.)

20009 31 AWG

7/0.0033" Tinned

Thermo- Plastic Olefin 140 Ohms/Mft

9.43 pF/ft 15.75 pF/ft 90 Ohms 127 Ohms 1.42 .040 (Max.)

20021 32 AWG 7/40 Tinned

Thermo- Plastic Olefin 176 Ohms/Mft 8.84 pF/ft 14.77 pF/ft 90 Ohms 129 Ohms 1.45

.030 (Max.)

Physical construction description: This Microzip cable consists of 30 AWG stranded tinned copper. Each leg of copper is pulled in parallel and fully extruded with HCM?s unique Thermo-Plastic Olefin (TPO). A red polarity stripe is co-extruded into position number one for easy identification. By co-extruding the polarity stripe, HCM assures a permanent marking that will not chip and avoids the use of hazardous ink materials. Standard color is light yellow.

Part No. HCM Configuration Insulation

No. of Cond.

Width "W" Span "S" Pitch Tolerance

Standard Put-ups

23196-026 R3007-51-26T AWM/CSA TPO 26 0.650" 0.625" ±.005" ± .0016" 100’

23196-034 R3007-51-34T AWM/CSA TPO 34 0.850" 0.825" ±.005" ± .0016" 100’

23196-040 R3007-51-40T AWM/CSA TPO 40 1.000"

0.975" ± .005" ± .0016" 100’

23196-050 R3007-51-50T AWM/CSA TPO 50 1.250"

1.225" ± .005" ± .0016" 100’

23196-064 R3007-51-64T AWM/CSA TPO 64 1.600"

1.575" ± .005" ± .0016" 100’

23196-068 R3007-51-68T AWM/CSA TPO 68 1.700"

1.675" ± .005" ± .0016"

100’, 200’ & 400’

23196-080 R3007-51-80T AWM/CSA TPO 80 2.000"

1.975" ± .008" ± .0016" 100’

23196-100 R3007-51-100T AWM/CSA TPO 100 2.500"

2.475" ± .007" ± .0020" 100’

20009-068 R3107-51-68T AWM/CSA TPO 68 1.700"

1.675" ± .005" ± .0016"

100’, 200’ & 400’

20021-068 R3207-55-68T AWM/CSA TPO 68 1.700"

1.675" ± .005" ± .0016" 400’

20021-080 R3207-55-80T AWM/CSA TPO 80 2.000" 1.975" ±.005" ± .0016" 400’

Other conductor counts available upon request.