Discuss this and other technologies with colleagues at the Reader Forum

Analytic Technique for Separation of Cochannel FM Signals

In the absence of noise, two signals can be separated perfectly.

NASA’s Jet Propulsion Laboratory, Pasadena, California

nth sampling interval is given by , where A and B A and B vary slowly, relative to problem is to estimate A, B,

and r

, where

.

For a single sample r(n (n (n (n (n (n (n and the second state represents the solution

. each time step n

the phase samples, an mth-order (where m

The metric for the trellis branch from the kth state at time n lth state at time n is the square of [(the l at time n n on the basis of k at time n

find the correct sequence.

estimation of A and B

This work was done by Jon Hamkins of Caltech for . For further free on-line at www.nasatech.com

NPO-20483

HOME | ABOUT NTB | LINKS CONTACT US | FEEDBACK PRIVACY