1-800-BELDEN-1

High Temperature Instrumentation and Control Cable Unshielded 20 AWG, 1 Pair

Trade Number Industry Stds.

Std. Lgth. (ft.)

Std. Units (lbs.)

AWG (strand) Type

(Nom. D.C.R.) Insul Thick

(Jkt Thick)

Nom. O.D.

Nom. Imp. (ohms)

Vel. of Prop.

Nom. Cap.

Conductors Shields

85220 100500

1000 4.0 13.7 26.9

20 (7x28) TC 0.015 in. 0.02 in.

0.185 in.

Metric

(Meters) 30.5 152.4 304.9

(Kg) 1.82 6.2 12.2

.381 mm

.508 mm

4.699 mm

Description:

Insulation: Tefzel Tinned copper conductors, Tefzel® insulated, conductors cabled, Clear Tefzel jacket. 150°C. 300V (RMS). Passes VW-1 Vertical Wire Flame Test. Color code: Black, Red. Spools and/or UnReel® cartons are one piece, but length may vary +/-10% for spools and +/-5% for UnReel® from length shown. Tefzel is a DuPont trademark. *Capacitance between conductors. **Capacitance between conductors and other conductors connected to shield.

Jacket: Tefzel

Plenum Version(s): n/a

(Select other related products with BACK or PREVIOUS.)

Disclaimer: Great effort is made to ensure the accuracy of the information presented, but errors or omissions may exist. This listing of information is presented as a courtesy and does not ensure that a product with these specifications is available. Specifications and availablility should be confirmed with a call to our sales representatives or to customer service. Have a question? Call us at 1-800-BELDEN-1 or send us a comment. Page displayed 1/25/2000 for category Multi-Conductor Paired.

Return to Belden’s Home Page

Products | Trade Shows | Distributors | Links | Message Center | Financial Info | Search | FAQs

Copyright © 2000 Belden Inc.