A R G O N N E N A T I O N A L L A B O R A T O R Y 41050103-00002

Title:Technical Specification for APS 1 ID Beamline Monochromatic HutchR e v . 0 0 ApprovedDate

Page

11˚ of

˚ ˚ 1 1 ˚ ˚

ANL-242 (3-83)4 . 2 . 6 . 6 Water Pressure and Flow Tests. Only clean, filtered tapwater shall be used for testing. After testing, the water lines shall be dried by blowingthem out with clean, dry, oil free air.4.2.6.6.1 Water lines shall be pressure tested to 200 psi. Noevidence of leakage is permissible.4.2.6.6.2 Water lines shall be flow tested for continuity with 5gpm minimum flow required at 1 psi or less pressure drop per foot of pipe.5.0

PREPARATION FOR DELIVERY5 . 1 Each package shipped shall be identified by the appropriate purchase ordernumber, assembly number and a sequential package identity number if there is morethan one.5 . 2 Any moving components on an assembly must be firmly secured for shipmentin a manner that precludes damage from motion and vibration.5 . 3 Assemblies must be secured for shipment in fashion that protects the assemblyfrom dust, dirt and weather or water damage. The assemblies must be securelyfastened, padded, boxed and/or crated for shipment in a suitable manner for preventionof shipment damage to any assembly and its weather/dust protection and insure theirsafe delivery to the Laboratory.5 . 4 The 1 ID Monochromatic Hutch shall be erected on the experimental floor ofthe Advanced Photon Source at a location to be specified by cognizant APS personnel.Final delivery and acceptance shall be after successful completion of inspection andacceptance testing per section 4.2 above.