A R G O N N E N A T I O N A L L A B O R A T O R Y 41050203-00002

Title:Technical Specification for APS Monochromatic Beam Experimental Stations in Sectors 1, 2 and 3R e v . 0 0 ApprovedDate

Page

15˚ of

˚ ˚ 1 5 ˚ ˚

ANL-242 (3-83)

4 . 2 . 6 . 6 . 1

Water lines shall be pressure tested to 200 psi. Noevidence of leakage is permissible.

4 . 2 . 6 . 6 . 2

Water lines shall be flow tested for continuity with 5gpm minimum flow required at 1 psi or less pressure drop per foot of pipe.

4.2.6.7

Electrical Circuit Tests:Each electrical circuit shall betested for continuity of connection from beginning of the circuit to the end, and foropen circuit line-to-line and line-to-ground.

4.2.6.8

Crane and Hoist Tests: The cranes and hoists shall betested for compliance with the appropriate ANSI/ASME specification as shown inSection 2.6.2 of this specification

5.0

PREPARATION FOR DELIVERY5.1

Package Identification

:Each package shipped shall be identified bythe appropriate purchase order number, assembly number and a sequential packageidentity number if there is more than one.

5.2

Moving Components:

Any moving components on an assemblymust be firmly secured for shipment in a manner that precludes damage from motionand vibration.

5.3

Protection:

Assemblies must be secured for shipment in fashion thatprotects the assembly from dust, dirt and weather or water damage. The assembliesmust be securely fastened, padded, boxed and/or crated for shipment in a suitablemanner for prevention of shipment damage to any assembly and its weather/dustprotection and insure their safe delivery to the Laboratory.

5.4

Erection:

The APS Monochromatic Beam Experimental Stations shallbe erected on the experimental floor of the Advanced Photon Source at a location to bespecified by cognizant APS personnel. Final delivery and acceptance shall be aftersuccessful completion of inspection and acceptance testing per section 4.2 above.