M. Gilchriese

Disk Rings and Assembly

M. G. D. Gilchriese

Lawrence Berkeley National Laboratory

April 2000

M. Gilchriese 2

Disk Ring

¯ Quantities

˘ Preproduction : minimum one

˘ Production : 6 rings for 11 sector disks and

4 rings for 10 sector disks

¯ Important requirements

˘ Locate sectors(placement accuracy) within window of +/- 50 microns(actual locations for each sector will be surveyed after assembly to accuracy <5 microns rms relative to ring mount definitions using optical CMM).

˘ Provide stability of sectors under operating conditions of

¯ < 10 microns rms in plane

¯ < 50 microns rms out-of-plane

˘ Meeting interface requirements(space) for services

¯ Minimize material/cost consistent with meeting above.

3 support points

to support frame.

3 support points

for each sector.

3

History and Status S ummary

¯ Design is responsibility of Hytec, Inc.

¯ First prototype design complete, first prototype fabricated and tested with full complement

of sectors(but not current baseline design - ESLI sectors). This has been supported by DoE

SBIR program. See report also in your notebook.

¯ Second prototype designed, under fabrication. Will also have full complement of

sectors(Hytec design). Also supported by DoE SBIR program. Will have final test results

by July.

¯ Testing shared between Hytec and LBNL.

¯ First prototype did not meet placement accuracy requirements but appears to meet stability

and other requirements.

¯ Design of second prototype modified to meet placement tolerances, to improve

stiffness/stability and better assembly.

¯ Dimensions of both prototypes not the same as current 11 or 9 sector baseline(layout

evolved) but very close(to 11 sector).

¯ Current plan is to proceed from second prototype directly to preproduction for 11 sector

disk ring. Will make at least one additional ring beyond number required for experiment,

equip with baseline sectors and repeat stability test program before launching full

construction(although materials will be ordered). This will provide spare ring(s).

4

First Prototype Disk Ring

¯ BOND TOGETHER AND THEN MACHINE BONDED

ASSEMBLY TO FINISHED DIMENSIONS

¯ RING O.D.420mm

¯ RING I.D. 380mm

¯ DEPTH 11mm

¯ MATERIAL

¯ FACESHEETS:K321 CARBON-CARBON .7mm THK

¯ C CHANNEL:T300 GRAPHITE LAMINATE, 4 PLY

(0/20/-20/0) 60% VOLUME FIBER AND CYANATE

ESTER RESIN

¯ BUSHINGS/WASHERS:CARBON-CARBON BRAKE

MATERIAL

¯ RING MOUNTS:6061-T6 ALUM, BLACK ANODIZE

¯ CONSTUCTION

¯ FACESHEETS: EACH FACESHEET COMPOSED OF

4 PARTS BONDED TOGETHER

¯ C CHANNELS: SHAPE OF CHANNELS CONFORM

TO FACESHEET PROFILE

¯ PROBLEMS:

¯ TWIST INGRAINED IN C CHANNELS DUE TO

LAYUP PATTERN

¯ DRILL BIT WANDERED WHILE MACHINING

SECTOR MOUNTING PATTERN

¯ FINAL WEIGHT: 124gms

0.7 mm thick carbon-carbon face sheets

chosen to match CTE of sectors.

Box-like construction

Mounting insert

T300 close-out

Carbon-carbon inserts

for sector attachment

5

First Prototype Ring Photos

6

Second Prototype Ring

¯ BOND PREMACHINED PARTS TOGETHER USING PRECISE GRAPHITE BOND JIG . C-CHANNELS WILL BE

FABRICATED USING AN AUTOCLAVE PROCESS TO ACHIEVE DESIRED FIBER FRACTION AND A BETTER

FINISHED PRODUCT. BOND JIG WOULD BE INVAR IN PRODUCTION.

¯ RING O.D. 423.34mm

¯ RING I.D. 374.65mm

¯ DEPTH 16.04mm

¯ SECTOR MOUNT PATTERN B.C. DIAMTERS: SAME AS FIRST PROTOTYPE RING

¯ RING MOUNT PATTERN B.C.: SAME AS FIRST PROTOTYPE RING

¯ MATERIAL:

¯ FACESHEETS: HEAT TREATED P30 CARBON-CARBON UNITAPE .4mm THK 8 LAYER 0/45/-45/90/-S)

¯ C CHANNEL: YSH50 WOVEN CLOTH, 4 PLY [0/90/45/-45] s 60% VOL FIBER AND YLA RS-12 CYANATE ESTER

RESIN

¯ BUSHINGS/WASHERS: PEEK MATERIAL

¯ RING MOUNTS: 6061-T6 ALUM, BLACK ANODIZE

¯ CONSTRUCTION:

¯ FACESHEETS: FACESHEETS CONSTRUCTED FROM ONE PIECE

¯ C CHANNELS: 180 ° PROFILE CONFORMS TO OUTER AND INNER DIA OF FACE SHEET

¯ MOUNTING CORNERS: CARBON-CARBON CORNERBLOCK INSERT REPLACES C CHANNEL PROFILE

¯ FINAL BOND ADHESIVE: HYSOL 9396 WITH .003~ GLASS BEAD FILLER

¯ PROBLEMS: TBD

¯ FINAL WEIGHT: TBD

7

First Prototype Disk

12 ESLI Sectors

and support ring.

Complete thermal

and mechanical

prototype

8

First Prototype Disk

¯ Purpose

˘ Gain assembly experience

˘ Test stability under operating conditions

¯ Scope

˘ First prototype disk support ring

˘ 12 sectors from ESLI(of which 2 were damaged during shipment/assembly and

leak)

˘ Dummy heaters on each sector to simulate heat load(up to 60 Watts/sector).

˘ Multiple optical targets on each sector, on ring and other locations.

˘ Temperature and pressure readout via computer

˘ Coolant connections using standard components(not low mass) and coolant is

water/alcohol mix.

¯ Measurement program

˘ Use optical CMM to measure targets under variety of operating conditions

˘ See video tape of measurement process.

9

Target Locations First Prototype Disk

Coordinate system is

defined by targets on

Invar support triangle.

These are remeasured

after measuring other

targets to gauge stability

of measurement.

Targets on ring, on inlet

and outlet(in/out) tubes, at

inner radius of sectors

and outer radius of

sectors(at mounts).

10

Stability Measurements

¯ Preliminary analysis is complete. We

have spent most of time

understanding reliability of

measurements.See note in book and

some plots next pages.

¯ Present here example of motion seen

by comparing room

temperature(average) base state with -

10 o C, 60 Watts state.

¯ Results indicate that stability

requirements can be met.

¯ Intrinsic resolution of device is about

1 - 1.5 microns rms in X and Y and

about 3-5 microns in Z.

X Y Z

RMS (ring) 0.0038 0.0055 0.0073

RMS (in/out) 0.0088 0.0052 0.0111

RMS (sec tor@mount) 0.0023 0.0041 0.0083

RMS (sec tor@innerR) 0.0028 0.0033 0.0091

SP READ (ring) 0.0105 0.0134 0.0180

SP READ (in/out) 0.0206 0.0133 0.0323

SP READ (s ector@m ount) 0.0079 0.0141 0.0320

SP READ (s ector@innerR) 0.0107 0.0134 0.0378

SP READ (invar, final) 0.0041 0.0018 0.0014

AV E (ring) -0.0027 -0.0005 0.0014

AV E (in/out) -0.0005 0.0014 0.0013

AV E (sec tor@mount) -0.0013 0.0002 0.0014

AV E (sec tor@inner R) -0.0010 -0.0012 0.0135

AV E (invar,f inal) -0.0008 -0.0005 -0.0016

AVE is average motion between the two

states. SPREAD is the largest-smallest

motion(including sign). RMS is standard

deviation. Units are mm.

11

SH IF TX avg,in nertargets,vs in let pressure

-0.002

-0.0015

-0.001

-0.0005

0

0.0005

0.001

0.0015

0.002

-5 0 5 10 15 20 25 30

P r ess ur e (p si)

S hiftX (mm)

26 C

20 C

16 C

-10 C

20 C (amb.)

12

X RMS,innertarg ets,vsinletpres.

-0.002

-0.001

0

0.001

0.002

0.003

0.004

-5 0 5 10 15 20 25 30

P r ess ur e (p si) mm

26 C

20 C

16 C

-10 C

20 C (am.,)

13 shiftYavg.in nertargetsvsinletpressure

-0.002

-0.001

0

0.001

0.002

0.003

0.004

0.005

-5 0 5 10 15 20 25 30

P r ess ur e (p si)

S hiftY (mm)

26 C

20 C

16 C

-10 C

20 C (amb.)

14

R MS Y,innertarg ets,vsinletpressure

0

0.0005

0.001

0.0015

0.002

0.0025

0.003

0.0035

0.004

0.0045

-5 0 5 10 15 20 25 30

P r ess ur e (p si) mm

26 C

20 C

16 C

-10 C

20 C (amb.)

15

SHIF T ZAVG INNERR VS INLET PRESSURE

-0.00 5

0

0.005

0.01

0.015

0.02

0.025

-5 0 5 10 15 20 25 30

Pr essu re (p si)

Sh iftZ(mm)

26 C

20 C

16 C

-10 C

20 C (amb.)

16

ZRM S inn er Rvs in le tpr e ss ur e

0

0.00 5

0.01

0.01 5

0.02

0.02 5

-5 0 5 10 15 20 25 30

P re s s ure (p s i) mm

26 C

20 C

16 C

-10 C

20 C (amb.)

17

Measurement Implications and Plan

¯ Stability in-plane appears to be adequate - better than 10 microns rms , although full

temperature range not explored.

¯ Out-of-plane stability is within requirement.

¯ FEA estimates predict(see Hytec note in your book) small motion(max 12 micron

displacement for 40 degree temperature change) but do not include pressure effects.

¯ Measurements will be repeated on 2nd prototype disk

˘ Will use TV holography at Hytec, which has order of magnitude better resolution in out-

of-plane coordinate.

˘ TV holography being adapted to measure in-plane but can also use LBNL optical CMM

again if this fails albeit with poorer but still adequate precision.

˘ Will increase temperature range, and use simple evaporative system(at Hytec but not

LBL) for cooling.

¯ We also applied known loads to coolant connection points and measured deflections.

These deflections during services connection must be controlled monitored during

actual assembly => assembly concept devised to take this into account(services

support frame and motion monitors during assembly will be implemented).

18

Interfaces

¯ Sector mounting

˘ Under control and part of prototype program

¯ Support to frame

˘ This is current critical issue - see next page

¯ Services

˘ This is current critical issue - see next page

¯ Assembly and final assembly

˘ Early conceptual design complete(see Eric´s talk later).

˘ Do we need additional hard points, connections on ring for assembly? Current

answer is no - will incorporate into three supports to frame.

˘ Must monitor/control deflections from attaching services to sectors when on

disk

¯ Survey

˘ Will include optical targets on ring for survey after assembly but expect to use

survey targets on sectors since sector location is critical issue.

˘ Expect to measure locations of all sectors relative to 3 support points using

optical CMM with technique like that used to assess stability.

˘ In addition, will have targets mounted at inner radius of sectors for post-

assembly survey.

19

Critical Issues

¯ Critical Issues

˘ Overall stability of disk will be

affected by design of ring-to-frame

support.

˘ Conceptual design started but no

prototypes for 4-6 months(aim to

have by end September).

˘ Will use existing frame prototype

parts to mockup support(see Eric´s

talk later) and assess stability.

˘ Services interface and strain relief.

Current plan has all of strain relief

in sectors and frame and none in

ring. But this needs to be verified.

Timescale : by June FDR of

sectors.