E949 Circuit Breakers July 12, 1994 revised 3/5/2002

Rack Use Breakers^1,^2 power strip R1 DC Postamps B13,B14,B15,B16,B17 B15 R2 DC Postamps B18,B19,B20,B21,B22 B20 R3 Splitters None R4 RS Phillips fanouts E23A,E24A E24A R5 RS Phillips fanouts B23B,B24B R6 RS Phillips fanouts E25A,E26A R7 RS Phillips fanouts B25B,B26B E25A in R6 R8 Splitters None R9 FASTBUS ADC’s C2,C4, C1-3,C6-8 E25A in R6 R10 FASTBUS TDC’s C4, C5-7,C9-11,C10-12 R11 CCD 1 C14, C13-15,C17-19,C18-20 R12 CCD 2 C16, C21-23,C25-27,C26-28 R13 CCD 3 C22, C29-31,C30-32,C33-35 R14 CCD 4 C24, C34-36,C37-39,C38-40 L1 Splitters None L2^3 BV Discriminators E1,E3,E2 L3 Summers E3,E4 L4 Splitters None L5 TG Amplifiers E5,A6 L6^4 TG Discriminators A7,A8,A10 A6 in L5 L7 Beam logic A9,A10 L8 Beam logic A11,A12 B61 L9 Trigger A13,A14 L10 Trigger FASTBUS A15, B30-32,B31-33,B35-37 L11 Walkway None L12^5 FASTBUS Master, FERA A22,A24,A17-19 B61 L13 TD 1,2,3 A30, A26-28,A29-31,A25-27 L14 TD 4,5,6 A37, A32-34,A33-35,A36-38 A37 L15 TD 7,8,9 A40A, A18-20,A21-23,B67-68 L16 FERA E39,B53,B54,B55,B56 E39 L17 FERA B57,B58,B59,B60 L18 FERA A40B, B51,B52,B61 L19 Alarms B62 L20 Target CCD logic A16 “R15” Moveable Test Rack E2A,D22-24

wall outlets near CCD’s A1A,E2A,E3A,A4A

1CB not in use: E27A,A29,E28A,B28B,E63,B65,D7,D9,D11,D13,D14-16,D22-24 2old CB A(1,2,2A,3,3A,4,5,39), B(23A,24A,25A,26A,27A,28A,63) moved to panel E with the number unchanged, i.e. A1 is now E1, etc.

3L2 CMC2 power moved from breaker E4 to E3 4L6 CMC3 power moved from breaker A8 to A10 5L12 bottom CMC powered by breaker A61 6CB A1A,E2A.E3A.A4A outlets on wall next to CCD racks