EM cal peds

EMCal pedestals vs run number. The shielding was grounded at time shown by the red line.

EM cal peds, cont

EMCal pedestals vs run number. Other noisy channels.

number of hot channels

EMCal’s number of hot channels vs run number.

ped′s rms distributions

Distribution of the RMS values of EMCal peds for selected run numbers.

what is next?

• keep tracking of hot channels • more work on shielding, groundings ...

• place peds (mean and rms) onto MIPP DB via batch ... • apply ped’s on beam events