* * * * * * * * 

READ AND REMOVE THIS OUTLINE GUIDE BEFORE PLACING
THE SPECIFICATION SECTION IN THE CONTRACT

* * * * * * * *

O U T L I N E   G U I D E

DIVISION 9 :FINISHES

SECTION 09542 - FIBERGLASS REINFORCED PLASTIC PANELS

USE:	Furnishing and installing Fiberglass reinforced Plastic Panels.  Typically used for wall covering in restroom and kitchen applications.  Consider as a lower cost option in areas of high moisture and high abuse in lieu of tile.

May not be appropriate in higher end installations where attachment battens and rivets are aesthetically unacceptable.

Panels still require backing for attachment such as plywood or gypsum wallboard.

NOTES TO SPECIFIER:

A.	Options within paragraphs are identified by enclosure in brackets; blank spaces enclosed by brackets [      ] provide for information to be inserted, as appropriate to individual projects.

B.	TO AVOID CONFLICTING REQUIREMENTS AND COSTLY MISTAKES, the specifier must edit (delete, substitute or add to the text).  The remaining paragraphs must be renumbered.

C.	DELETE FOR FINAL COPY: Notes to the Specifier, located between lines of asterisks; all [brackets], underlining, boldface, and italics within the paragraphs; and this page.  (Open Reveal Codes [alt F3] to do this accurately).

D.	To Edit “(Footer B)”: (Corel 8).  ENTIRE FOOTER SHOULD BE BOLDED.  Click in the footer and delete the “Project Name (ftr B)” text and replace it with the Name Of The Project (upper/lower case).  Replace date with current MM/YY (WITHOUT BRACKETS). 

E.	The Guide Specifications are intended to be continuously reviewed and revised.  User’s technical comments are appreciated.  Also, other related or similar specifications that are written “from scratch” that could benefit others, or other questions can be sent to NARSC A/E Group, RS-110 or call (303) 987-6851.

F.	DESIGN NOTES:

1.	DRAWING DATA REQUIRED:

		A.	Indicate panel layout and location of battens if attempting to achieve a particular pattern.

REVISIONS OF THIS SECTION:
CSI format, editorial changes 11/99
Metric: Not Applicable
Technical Update: 12/99 	

SECTION 09542

FIBERGLASS REINFORCED PLASTIC PANELS

PART 1:  GENERAL

1.1	DESCRIPTION
********************************************************
BRIEFLY DESCRIBE, IN GENERAL TERMS, WHAT THE WORK OF THE SECTION INCLUDES.
********************************************************

A.	This section describes the requirements for furnishing and installing fiberglass-reinforced plastic panels according to manufacturer’s recommendations.

B.	Related Work:
***********************************************************
LIST SECTIONS WHERE ITEMS OF WORK THAT MIGHT LOGICALLY BE FURNISHED AND INSTALLED UNDER THIS SECTION, BUT INSTEAD ARE SPECIFIED IN ANOTHER SECTION.  THIS ARTICLE IS RARELY REQUIRED.
***********************************************************

1.2	SUBMITTALS

A.	General:  Submittals shall be according to Section 01330 ‑ Submittal Procedures.

B.	Samples: Submit [two] samples of panels, standard colors, and each type of trim and fastener.

C.	Manufacturer's Literature:  Submit [five] copies of manufacturer's descriptive data for materials to be used on this project.

1.3	QUALITY ASSURANCE

A.	Provide panels and molding only from one manufacturer to ensure warranty and color harmonization of accessories.

B.	Comply with manufacturer’s recommendation for installation. 

1.4	DELIVERY, STORAGE, AND HANDLING

A.	Deliver materials in original packages, bearing brand name and identification of manufacturer.  Store and protect as per manufacturer’s recommendations.  Handle material to prevent damage.  Damaged material will be rejected.  

1.5	PROJECT AND SITE CONDITIONS

A.	Installation shall not begin until building is enclosed, permanent heating and cooling equipment is in operation, and residual moisture from plaster, concrete or terrazzo work has dissipated. 

B.	During installation and for not less than 48-hours before, maintain an ambient temperature and relative humidity within limits required by manufacturer.

C.	Provide ventilation to disperse fumes during application of adhesive as recommended by the adhesive manufacturer.  

PART 2:  PRODUCTS

2.1	MATERIALS
***************************************************************
IN A SEPARATE ARTICLE OR PARAGRAPH, DESCRIBE EACH PRODUCT.  USE ONE OF FOUR METHODS:
1.	DESCRIBE THE PRODUCT IN DETAIL, SPECIFYING THE ESSENTIAL PHYSICAL AND FUNCTIONAL CHARACTERISTICS.  TO ENCOURAGE MAXIMUM PRICE COMPETITION, LIST ONLY ESSENTIAL REQUIREMENTS, AND WHERE POSSIBLE, AVOID SPECIFYING A PRODUCT OR A FEATURE PECULIAR TO ONE MANUFACTURER.
2.	SPECIFY A MANUFACTURER’S PRODUCT OR “APPROVED EQUAL”.  GIVE THE MANUFACTURER’S NAME AND CITY AND STATE.  IF THE COMPANY IS NOT NATIONALLY RECOGNIZED, GIVE THE COMPLETE ADDRESS AND TELEPHONE NUMBER.  INCLUDE COMPLETE CATALOG, MODEL, AND PART NUMBERS, VERIFIED TO ENSURE THAT THE SPECIFIED PRODUCTS ARE CURRENTLY AVAILABLE.
3.	CITE A REFERENCE STANDARD AND IDENTIFY THE EDITION REFERENCED (DATE), STATING THE TYPE, CLASS, OR STYLE, AS APPROPRIATE.  MAKE SURE REFERENCE IS COMPLETE AND ACCURATE TO AVOID UNINTENTIONALLY GIVING THE CONTRACTOR AN OPTION.
4.	OR, IN EITHER PART 2 OR PART 3, SPECIFY THE REQUIRED RESULTS AND THE CRITERIA BY WHICH THE PERFORMANCE CAN BE VERIFIED.
*****************************************************************

A.	Fiberglass Reinforced Panels: Glass fiber laminate consisting of a uniform mat of high strength glass fibers embedded in an organic resin and heat cured to a solid material which is strong and resistant.  Color shall be uniform throughout.  Color shall be [white].

B.	Molding: Division bars, edge trim, and corner trim shall be manufacturer’s standard shapes extruded vinyl pieces; longest length possible to eliminate end joints.  Color [to match panels].

C.	Adhesive: As recommended by manufacturer.

D.	Fasteners: Manufacturer-supplied, non-corroding fasteners to attach panels and trim to substrate.  Color [to match panels].

2.2	MANUFACTURER

**********VERIFY SOURCES**********
******************************************************************
USE THIS ARTICLE ONLY IF ALL ITEMS SPECIFIED ARE BY ONE MANUFACTURER.  IF THIS ARTICLE IS USED, IT IS NOT NECESSARY TO FOLLOW THE MODEL NUMBER WITH THE WORDS “OR APPROVED EQUAL”.
******************************************************************

A.	Glassboard wall panels and accessories as available through Kemlite Company, Joliet, Illinois, 800-435-0080.

B.	Other manufacturer’s products may be used provided they are approved as equal.

PART 3:  EXECUTION

3.1	PREPARATION

A.	Examine backup surfaces to determine that corners are plumb and straight, surfaces are smooth, uniform, clean and free from foreign matter, nails countersunk, joints and cracks filled flush and smooth with the adjoining surface.

B.	Do not begin installation until backup surfaces are in satisfactory condition.  

3.2	APPLICATION

A.	Do all cutting and drilling with carbide tipped saw blades or drill bits, or cut with snips.

B.	Install panels with manufacturer’s recommended gap for panel field and corner joints. 

C.	Fastener holes in the panels must be predrilled 1/8-inch over size.

D.	Using products acceptable to manufacturer, install the panel system in accordance with panel manufacturer’s printed instructions.  Use full panel sheets and lengths of trim to minimize the number of joints.  Adhere panels to substrate with recommended adhesive.  Mechanical fasteners to be concealed by edge molding.  Coordinate the installation of panels with the installation of trim pieces to provide a clean and moisture-resistant system with minimal joints and no seams or fasteners left uncovered by moldings.  No gaps, bows, damaged trim or panels will be accepted.  Cut all molding at 45 degree angle at all directional changes.  Apply silicone sealant in a workmanlike manner and as recommended by manufacturer to achieve a clean, moisture-resistant installation.  Apply 1/8-inch bead of silicone sealant full length of panel base along panel/ceramic tile joint.  Tool joint smooth.  Sealant color [to match panel/trim].

3.3	CLEANING

A.	Remove any adhesive or excessive sealant from panel face using solvent or cleaner recommended by panel manufacturer.

PART 4: MEASUREMENT AND PAYMENT

4.1	METHOD OF MEASUREMENT

************************************************************
WHEN A “LUMP SUM” CONTRACT IS USED, DELETE THE TITLE “PART 4: MEASUREMENT AND PAYMENT” AND BOTH ARTICLES FROM THIS SECTION.  MEASUREMENT AND PAYMENT WILL BE ADDRESSED IN PART 4 OF SECTION 01009 - GENERAL INFORMATION AND REQUIREMENTS OR SECTION 01010 - SUMMARY OF WORK.

WHEN NOT A “LUMP SUM” CONTRACT, SELECT APPLICABLE PHRASES; USE THE “NO MEASUREMENT” PHRASE WHEN NONE OF THE PAY ITEMS IN THIS SECTION ARE INCLUDED IN THE BID SCHEDULE.
**********************************************************

A.	Units: The work described in the section will [not be measured for payment] [be measured and paid for] [on a lump sum basis].

4.2	BASIS OF PAYMENT

**************************************************************
WHEN NOT A “LUMP SUM” CONTRACT, SELECT APPLICABLE PHRASE; USE THE “NO DIRECT PAYMENT” PHRASE WHEN NONE OF THE PAY ITEMS IN THIS SECTION ARE INCLUDED IN THE BID SCHEDULE.

WHEN NOT A “LUMP SUM” CONTRACT AND PAYMENT IS TO BE MADE UNDER THIS SECTION, SELECT APPLICABLE PAY ITEMS.  DO NOT CHANGE PAY ITEM NUMBER.
***************************************************************

A.	Payment: [No direct payment for the work described under this section will be made.  The Contractor shall include consideration for this item in the bid price for other items of the Contract]. [Prices and payment will be full compensation for the work described in this section.  Payment will be made under]:

09542(01)	Fiberglass Reinforced Plastic Panels	Lump Sum

END OF SECTION

FIBERGLASS REINFORCED PLASTIC PANELS
Project Name (ftr B)	[12/99]
09542 -