Checkout Sheet Technician Name: _______________________ TRACER # : _______________________

Fermilab

Particle Physics Division/CDF Upgrade Project

Checkout Procedure for TRigger And Clock + Event Readout Module (TRACER _V2.1)

Theresa M. Shaw Rodney L. Klein 9/28/98

Checkout Sheet

Technician Name: _______________________

TRACER #: _______

Note any test which initially fails and the action taken to repair it:

Name of Failing Test: __________________________________________

Repair Steps: ________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

Name of Failing Test: __________________________________________

Repair Steps: ________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

Name of Failing Test: __________________________________________

Repair Steps: ________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

Name of Failing Test: __________________________________________ Repair Steps: ________________________________________________ _____________________________________________________________ _____________________________________________________________ _____________________________________________________________ _____________________________________________________________ _____________________________________________________________ _____________________________________________________________

Name of Failing Test: __________________________________________ Repair Steps: ________________________________________________ _____________________________________________________________ _____________________________________________________________ _____________________________________________________________ _____________________________________________________________ _____________________________________________________________ _____________________________________________________________

Name of Failing Test: __________________________________________ Repair Steps: ________________________________________________ _____________________________________________________________ _____________________________________________________________ _____________________________________________________________ _____________________________________________________________ _____________________________________________________________ _____________________________________________________________

Name of Failing Test: __________________________________________ Repair Steps: ________________________________________________ _____________________________________________________________ _____________________________________________________________ _____________________________________________________________ _____________________________________________________________ _____________________________________________________________ _____________________________________________________________

Name of Failing Test: __________________________________________

Repair Steps: ________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

Name of Failing Test: __________________________________________

Repair Steps: ________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

Name of Failing Test: __________________________________________

Repair Steps: ________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

Name of Failing Test: __________________________________________

Repair Steps: ________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

_____________________________________________________________

TRACER Pre-Production Module Checkout

______ Visual Board Inspection

Look for rotated ICs, missing components, poor soldering, etc.

______ Check for shorts between power and ground

The BOLD Components MUST be Programmed and Inserted into sockets Do not stuff switch S4

Particle Physics Division/CDF Upgrade ProjectTTACER Checkout Procedure

06/22/98 09:40:51                               Electronics Design System                                     Page: 0001

                                                    Bill of Materials

                                <<<From Job:  J:\TRACER_PROD_V2_1\vbdc\tracer_prod.prj>>>

                                               Fermi National Accelerator

                                              PPD/ET&T/CDF Upgrade Project

------------------------------------------------------------------------------------------------------------------------

 Item  | QTY   | vendor part number               | Description                              | Cost  | REF DESG

------------------------------------------------------------------------------------------------------------------------

     1 |     3 | AD9501JP                         | Dig Prog Delay Gen, JP pkg               | 20.00 | U56-U58

     2 |     1 | AMP 1-520459-3                   | AMP Modular Jack Connector 8 Pos         | 2.25  | J1

     3 |     1 | AMP 3-520459-3                   | AMP Modular Jack Connector 8 Pos         | 2.25  | J2

     4 |     1 | AMP 226968-1 DIGI A1126-ND       | Twinax Bulkhead                          | 24.58 | J6

     5 |     1 | AMP 269050-1                     | AMP Optronic Data Link - RCVR 200Mb/s    | 76.47 | U15

     6 |     1 | AMP 352009-1 PLUS SHIELDS .      | AMP 5x19 Z-PACK 2mm Female Conn w/gnd sh | 25.00 | P0

     7 |     1 | AMP269049-1                      | 200 Mb/s 1300 nm optical transmitter.    | 20.00 | D6

     8 |     1 | AM27S19SAPC                      | 32x8 PROM                                | 1.25  | U35

     9 |     1 | AM29F010-45JC                    | No PDB description available             | 10.45 | U11

    10 |     1 | AM7968-175JC                     | Taxi xmtr                                | 20.00 | U22

    11 |     1 | AM7969-175JC                     | TAXI RCVR                                | 25.00 | U16

    12 |     1 | BOT d_strip                      | Bottom Discharge strip                   | .01   | X2

    13 |     1 | C&K P8121  1160-1890             | Mom. Push button Panel mnt               | 2.48  | S4 - do not stuff

    14 |     3 | CAP_CER_SMT_SPARE_1206           | SMT CAP SPARE                            | 0.168 | C147,C149,C151

    15 |     1 | CY7B991-7JC                      | ROBOCLOCK                                | 21.85 | U42

    16 |     5 | CY7C470-15JC                     | Cypress 8K x 9 FIFO                      | 22.00 | U17,U28,U38,U44

     * |       |                                  |                                          |       | U49

    17 |     5 | CY74FCT16500TTSSOP               | 18-bit Registered Transceivers           | 5.78  | U23,U29,U30,U32

     * |       |                                  |                                          |       | U39

    18 |     1 | CY74FCT16543CTPAC                | No PDB description available             |       | U31

    19 |     5 | CY74FCT162244TTSSOP              | 16-Bit Buffers/Line Drivers              | 3.95  | U18,U27,U37,U43

     * |       |                                  |                                          |       | U48

    20 |     1 | DS26C32ATN RS-422 recvr National | Diff Line RCVR                           | 3.50  | U52

    21 |     1 | DS90C031 National                | Differential Line Driver                 | 2.23  | U9

    22 |     1 | DS90C032 National                | Differential Line Receiver               | 2.23  | U41

    23 |     3 | DS1020                           | Programmable 8-bit Silicon delay line 1n | 22.00 | U61-U63

    24 |     2 | ERIE 8131-100-651-104M 1415-3140 | Bypass Cap .1UF                          | 0.05  | C17,C25

    25 |     1 | ERIE 8131-100-651-153M 1415-3090 | Bypass Cap .015UF                        | 0.07  | C1

    26 |     4 | ERJ-6ENF19.1 Digi P19.1CBK-ND    | 1/10W 1% 19.1 ohm                        | 0.061 | R40,R43,R51,R54

    27 |     8 | ERJ-6ENF51.1 Digi P51.1CBK-ND    | 1/10W 1% 51.1 ohm                        | 0.061 | R41,R42,R44,R45

     * |       |                                  |                                          |       | R52,R53,R55,R56

    28 |     1 | ERJ-8ENF1.00K  Digi P1.00KFBK-ND | 1/8W 1% 1.0K ohm                         | 0.0542| R37

    29 |     3 | ERJ-8ENF8.0K Digi P8.0KFBK       | 1/8W 1% 8.0K ohm                         | 0.0542| R78-R80

    30 |     7 | ERJ-8ENF66.5   Digi P66.5FBK-ND  | 1/8W 1% 66.5 ohm                         | 0.0542| R26,R32,R35,R39

     * |       |                                  |                                          |       | R46,R65,R68

    31 |     2 | ERJ-8ENF82.5   Digi P82.5FBK-ND  | 1/8W 1% 82.5 ohm                         | 0.0542| R70,R71

    32 |     2 | ERJ-8ENF100   Digi P100FBK-ND    | 1/8W 1% 100 ohm                          | 0.0542| R48,R72

    33 |     2 | ERJ-8ENF121   Digi P121FBK-ND    | 1/8W 1% 121 ohm                          | 0.0542| R73,R74

    34 |     2 | ERJ-8ENF158   Digi P158FBK-ND    | 1/8W 1% 158 ohm                          | 0.0542| R29,R30

    35 |     2 | ERJ-8ENF169   Digi P169FBK-ND    | 1/8W 1% 169 ohm                          | 0.0542| R17,R25

    36 |     2 | ERJ-8ENF249  Digi P249FBK-ND     | 1/8W 1% 249 ohm                          | 0.0542| R23,R24

    37 |     2 | ERJ-8ENF267   Digi P267FBK-ND    | 1/8W 1% 267 ohm                          | 0.0542| R28,R34

Particle Physics Division/CDF Upgrade ProjectTTACER Checkout Procedure

06/22/98 09:40:51                               Electronics Design System                                     Page: 0002
                                                    Bill of Materials
                                <<<From Job:  J:\TRACER_PROD_V2_1\vbdc\tracer_prod.prj>>>

                                               Fermi National Accelerator
                                              PPD/ET&T/CDF Upgrade Project

------------------------------------------------------------------------------------------------------------------------
 Item  | QTY   | vendor part number               | Description                              | Cost  | REF DESG
------------------------------------------------------------------------------------------------------------------------

    38 |     2 | ERJ-8ENF394 Digi P394FBK-ND      | 1/8W 1% 394 ohm                          | 0.0542| R49,R50
    39 |    80 | Ground Via                       | Ground-Via                               | .00   | VG1-VG7,VG18,VG19
     * |       |                                  |                                          |       | VG20-VG85,VG89
     * |       |                                  |                                          |       | VG90-VG93
    40 |     3 | HARTING-male                     | VME64 Card Connector                     | 25.00 | P1-P3
    41 |     1 | HIROSE TM5RJ1-66  DIG H9083-ND   | Modular Jack 6pos 6contact               | 2.30  | J3
    42 |     1 | HP HFBR-2412                     | Fiber Optic RCVR                         | 18.15 | U26
    43 |     4 | HP HLMP-1301  1445-0475          | Red LED                                  | 0.24  | D1,D3-D5
    44 |     1 | HP HLMP-1401   1445-0495         | Yellow LED                               | 0.24  | D2
    45 |     1 | IDT 74FCT244DTP                  | 8 bit Tri-state buffer                   | 3.40  | U50
    46 |    17 | KEMET T340B106K015AS             | 10UF 15V Bullet                          | .80   | C56,C57,C59,C61
     * |       |                                  |                                          |       | C104,C132,C137
     * |       |                                  |                                          |       | C157,C161,C167
     * |       |                                  |                                          |       | C181-C183,C206
     * |       |                                  |                                          |       | C208,C211,C212
    47 |     3 | KEMET T354H336K016AS             | 33UF 16V RADIAL Dip                      | .85   | C18,C26,C53
    48 |     2 | LITTLEFUSE 251010 Newark 20F604  | 10 AMP PCB Fuse                          | 0.74  | F1,F2
    49 |     1 | MACH 110-12JC                    | AMD PLD 44 Pin PLCC                      | 7.00  | U25
    50 |     2 | MC10E116                         | QUINT differentail Line Receiver         | 10.00 | U40,U76
    51 |     1 | MC10H350                         | PECL Receiver                            | 10.00 | U51
    52 |     2 | MOTOROLA 1N5908                  | Transient Suppressor 6.0V                | 1.24  | D7,D8
    53 |     3 | PALCE22V10H-7PC                  | Programmable Logic Device                | 5.00  | U10,U34,U47
    54 |    15 | PAN ECS-H1CC106R DIG PCT3106     | SMT CAP 10.0UF                           | 0.9765| C2,C5,C6,C11,C13
     * |       |                                  |                                          |       | C14,C15,C24,C28
     * |       |                                  |                                          |       | C30,C31,C36,C37
     * |       |                                  |                                          |       | C41,C52
    55 |     1 | PAN ECS-H1CY105R DIG PCT3105     | SMT CAP 1.0UF                            | 0.3955| C48
    56 |    11 | PAN ECU-V1H103KBG DIG PCC103BN   | SMT CAP 0.01UF                           | 0.168 | C7,C9,C29,C32,C39
     * |       |                                  |                                          |       | C46,C90,C101,C102
     * |       |                                  |                                          |       | C119,C205
    57 |     5 | PAN ECU-V1H103KBM DIG PCC103BCT  | SMT CAP 0.01UF                           | 0.168 | C19,C50,C51,C92
     * |       |                                  |                                          |       | C93
    58 |   152 | PAN ECU-V1H104KBW DIG PCC104B    | SMT CAP 0.1UF                            | 0.5914| C3,C4,C12,C16,C21
     * |       |                                  |                                          |       | C23,C27,C33,C34
     * |       |                                  |                                          |       | C35,C38,C42,C43
     * |       |                                  |                                          |       | C44,C45,C49,C54
     * |       |                                  |                                          |       | C55,C58,C60,C62
     * |       |                                  |                                          |       | C63-C89,C91,C94
     * |       |                                  |                                          |       | C95-C100,C103
     * |       |                                  |                                          |       | C105-C118,C120
     * |       |                                  |                                          |       | C121-C131,C133
     * |       |                                  |                                          |       | C134-C136,C138

Particle Physics Division/CDF Upgrade ProjectTTACER Checkout Procedure

06/22/98 09:40:51                               Electronics Design System                                     Page: 0003

                                                    Bill of Materials

                                <<<From Job:  J:\TRACER_PROD_V2_1\vbdc\tracer_prod.prj>>>

                                               Fermi National Accelerator

                                              PPD/ET&T/CDF Upgrade Project

------------------------------------------------------------------------------------------------------------------------

 Item  | QTY   | vendor part number               | Description                              | Cost  | REF DESG

------------------------------------------------------------------------------------------------------------------------

     * |       |                                  |                                          |       | C139-C146,C148

     * |       |                                  |                                          |       | C150,C152,C153

     * |       |                                  |                                          |       | C154-C156,C158

     * |       |                                  |                                          |       | C159,C160,C162

     * |       |                                  |                                          |       | C163-C166,C168

     * |       |                                  |                                          |       | C169-C180,C184

     * |       |                                  |                                          |       | C185-C204,C207

     * |       |                                  |                                          |       | C209,C210,C213

     * |       |                                  |                                          |       | C214,C215,C245

    59 |     6 | PAN ECU-V1H561JCX DIG PCC561CGCT | SMT CAP 560pF                            | 0.125 | C8,C10,C20,C22

     * |       |                                  |                                          |       | C40,C47

    60 |    40 | PN32                             | test point                               |       | GP1-GP18,TP18

     * |       |                                  |                                          |       | TP23,TP24,TP31

     * |       |                                  |                                          |       | TP32,TP33,TP40

     * |       |                                  |                                          |       | TP44-TP58

    61 |     5 | RC05-270   1487-0290             | 270 ohm 1/8W 5%                          | 0.19  | R1,R3,R4,R6,R7

    62 |     1 | RC05-820K   1487-0497            | 1/8W 820Kohm 5%                          | 0.18  | R5

    63 |     3 | RC05-1000    1487-0325           | 1000 ohm                                 | 0.18  | R14-R16

    64 |     1 | RC07-1.5M   1487-1125            | 1/4W, 5PCT, THRU                         | 0.14  | R76

    65 |     2 | RC07-1M   1487-1105              | 1/4W, 5PCT, THRU                         | 0.19  | R2,R77

    66 |     1 | RC07-5.6   Digi 5.6QBK-ND        | 1/4W, 5PCT, THRU                         | 0.06  | R75

    67 |     5 | RC07-4700  1487-0825             | 1/4W, 5PCT, THRU                         | 0.08  | R10-R13,R36

    68 |     1 | RN55C-13K                        | 1/8W 1PCT Thru                           | 0.04  | R19

    69 |     3 | RN55C-27K                        | 1/8W 1PCT Thru                           | 0.04  | R20-R22

    70 |     2 | RN55C-84.5                       | 1/8W 1PCT Thru 249 Ohm                   | .04   | R62,R63

    71 |     1 | RN55C-100K                       | 1/8W 1PCT Thru                           | 0.04  | R18

    72 |     1 | RN55C-249   1487-4365            | 1/8W 1PCT Thru 249 Ohm                   | .04   | R61

    73 |    13 | SN74ABTE16245SSOP                | 16 Bit Incident Transceiver              | 5.60  | U1,U7,U8,U21,U33

     * |       |                                  |                                          |       | U45,U46,U54,U59

     * |       |                                  |                                          |       | U60,U65,U66,U75

    74 |     1 | SN74ABTE16246SSOP                | 11 Bit Incident Transceiver              | 7.50  | U14

    75 |     3 | Samtec TSW-12-07-L-D 2pin sip    | 2 pin jumper - mates with SNT-100-BK-G $ | 0.16  | S1-S3

    76 |     8 | Spare-IC 24DIP3                  | Spare 24 pin DIP                         | 0.00  | U67-U74

    77 |    16 | TEST_PIN                         | .025 x .025 square post.                 | .01   | TP2-TP6,TP14,TP19

     * |       |                                  |                                          |       | TP20,TP25,TP30

     * |       |                                  |                                          |       | TP34-TP37,TP42

     * |       |                                  |                                          |       | TP43

    78 |     1 | TIBPAL16L8-5C                    | Programmable Logic Device                | 5.00  | U13

    79 |     1 | TOP d_strip                      | Top Discharge strip                      | .01   | X1

    80 |    28 | VCC Via                          | VCC-Via                                  | .00   | VP1-VP25,VP59

     * |       |                                  |                                          |       | VP60,VP61

    81 |     1 | XC3130A-1PQ100C                  | Xilinx XC3130A Logic Cell Array          | 35.00 | U4

Particle Physics Division/CDF Upgrade ProjectTTACER Checkout Procedure

06/22/98 09:40:51                               Electronics Design System                                     Page: 0004
                                                    Bill of Materials
                                <<<From Job:  J:\TRACER_PROD_V2_1\vbdc\tracer_prod.prj>>>

                                               Fermi National Accelerator
                                              PPD/ET&T/CDF Upgrade Project

------------------------------------------------------------------------------------------------------------------------
 Item  | QTY   | vendor part number               | Description                              | Cost  | REF DESG
------------------------------------------------------------------------------------------------------------------------

    82 |     1 | XC4005EPQ100-3                   | Xilinx FPGA                              | 60.00 | U19
    83 |     1 | XC4013E-3PQ240C                  | Xilinx FPGA                              | 250.00| U6
    84 |     1 | XC17128-PD8C                     | XILINX PROM                              | 13.00 | U20
    85 |     2 | XC17256-PD8C                     | XILINX PROM                              | 13.00 | U3,U12
    86 |     2 | mc10h351l                        | Quad TTL to PECL translator.             | 10.00 | U36,U55
    87 |    15 | res_spare1206                    | 1/8W 1% 1.0K ohm                         | 0.00  | R8,R9,R27,R31,R33
     * |       |                                  |                                          |       | R38,R47,R57,R58
     * |       |                                  |                                          |       | R59,R60,R64,R66
     * |       |                                  |                                          |       | R67,R69
    88 |     1 | 1N5817                           | Scottky Diode                            | .80   | D9
    89 |     1 | 3 pin jump 3SIP60 TSW-12-07-L-D  | 3 pin jumper                             | 0.30  | U24
    90 |     1 | 10x-2-102                        | 10 pin 1K SIP, pin 1 common              | 1.50  | RP1
    91 |     1 | 74F04N                           | hex inverter                             | 0.53  | U53
    92 |     2 | 74F38N                           | Open collector nand                      | 0.53  | U5,U64
    93 |     1 | 74LS14N 1455-8014                | schmitt trigger inverter                 | 0.31  | U77
    94 |     1 | 74LS123N 1455-8123               | Multivibrator                            | 0.35  | U2
    95 |     4 | 2503-5020-UG 3M 20pin Rt Ang HDR | 3M 20 pin right angle header             |       | J7-J10
    96 |     6 | 2743021446 PSC ELECTRONICS       | SMT FERRITE BEAD 10UH                    | 1.30  | L1-L6

Total Parts Used: 573
Total Parts Cost: 1313.17

Begin Checkout Procedures

POWER

______ Check that Power LED D1 (page 1) comes on when board plugged in

______ Check voltage level on both sides of Fuses F1 and F2 (page 1). You should see 5 Volts.

RESET

______ Plug in a Reset Cable from the CDF Reset Module to Tracer Front panel Connector J3.

Issue a reset by issuing command by

1) logging into dorothy

2) type �ld <reset.o�

3) type �timer_on�

4) type �menu�

5) Select �Reset one Crate� option and select appropriate cable # (1-96)

When the Reset is sent, you should see the MVME162 re-boot itself.

Verify Download of FPGAs

______ Look at U12-4 (page 3A). This pin will have a high logic level if the VME_slave FPGA is properly downloaded.

______ Check for a high logic level at pin U3-4 (page 9A). This verifies the download of the TSI

Interface FPGA.

______ Check for a high logic level at pin U20-4 (page 9B). This verifies the download of the Local

Teststand Calibration FPGA.

Begin VMEbus Checkout

______ With only the TRACER module and a VRC (MVME162) in the crate, open the generalized checkout program VASE. Choose the option to MAP the crate.

______ Verify that the result of the crate map is a readout of the TRACER�s ID PROMU35 (page 4)in the correct slot. The ID PROM should be similar to the one below:

0987 001 TRACER_V2 where,

0987 reflects the serial number (changes on board by board basis - should match engraved serial number )

001 is the board type (always the same)

TRACER is the user specified text

VMEbus Register Checkout ______ Going back to VASE, select the TRACER submenu, and then choose the Tracer Checkout Menu option. Choose the Test all Registers option. This will allow you to do an initial test of most TRACER registers automatically. If errors are detected, exit menu and select Register Test Menu option to test individual registers. • ______ Diagnostic Register (inside VMEbus Slave FPGA) • ______ Control Register (inside VMEbus Slave FPGA) • ______ Calibration Register (inside local Teststand Calibration FPGA) • ______ Start Delay Register (inside local Teststand Calibration FPGA) • ______ Calibration Delay Register (inside local Teststand Calibration FPGA) • ______ Halt Delay Register (inside local Teststand Calibration FPGA) • ______ Interrupt Return Vector Register (inside VMEbus Slave FPGA) • ______ TDC Pulses Enable Register (inside VMEbus Slave FPGA) • ______ TDC Calibration Course Delay Register (inside VMEbus Slave FPGA) • ______ TDC Calibration Fine Delay Register (page 3A U23, U39) • ______ TDC Calibration Pulse Width Register (page 3A U29, U30) • ______ TBUS Register (page 14) • ______ Transition Port Read/Write Register (inside VMEbus Slave FPGA) • ______ Transition Port Address Register (inside VMEbus Slave FPGA) • ______ Event FIFO Data (U30, U37, U41, U46 page 7) • ______ Event FIFO Status Check • ______ Word Count Register (inside VMEbus Slave FPGA) • ______ Event Header Register (inside VMEbus Slave FPGA) • ______ A�s Pattern Register (insideVMEbus Slave FPGA) • ______ 5�s Pattern Register (insideVMEbus Slave FPGA) ______ Run looping test, Test all Registers in Loop Mode , for 100 loops.

Verify Flash RAM Registers

A 1 Megabit (131,072 x 8-Bit) AMD AM29F010 Flash Memory has been incorporated on the TRACER

(see page 13). The purpose of this Flash Memory is to serve as a storage device for any TRACER or crate level constants.

Like all Flash RAM, a specific algorithm must be used when erasing or programming the contents.

Two examples below describe how to set up the erase and the write alogorithms to these devices. For additional information on these devices, please refer to AMD�s data sheet.

To erase the Flash RAM write 0xAA 0000 to addr  0xYY61 5554(YY is Geo. Address)
write 0x55 0000 to  0xYY60 AAA8
write 0x80 0000 to  0xYY61 5554
write 0xAA 0000 to 0xYY61 5554
write 0x55 0000 to 0xYY60 AAA8
write 0x10 0000 to 0xYY61 5554

To write the Flash RAM write 0xAA 0000 to addr 0xYY61 5554
write 0x55 0000 to  0xYY60 AAA8
write 0xA0 0000 to  0xYY61 5554
write desired data to desired adrress

______ Using the Test Flash RAM option in the TRACER Checkout menu within VASE, verify that the

FLASH RAM can be loaded with data, verified and erased.

Module Select Light

______ As the board is addressed over VMEbus, the yellow Module Select light, D2 (page 3) should come on. Verify that it does, and that it is off when the module is not addressed.

Externally Applied Pulse

______ Use the PECL pulse generator box to drive a pulse over a Twinax cable to the Twinax Connector on the front panel of the TRACER (J6 page 5). This pulse should be received by U76 and is driven off the module with U40. Verify this is the case by looking (with o-scope) at front panel connector J7 pin 13 (page 11). This pin is being driven by a differential receiver which is looking at the backplane.

Logic Analyzer Port - On the TRACER

Tracer Front Panel Ports J will provide ports for easy access to the CDF backplane trigger and clock signals. These ports will bring TTL level signals to four 20 pin right angle box headers on the front panel.

The ports can be used by a wide range of oscilloscopes or logic analyzers, but are specifically designed for ease of use with HP logic analyzers and the HP Terminator Adapter.

Hewlett Packard Pinout on Terminator Adapter (HP part number 01650-63203)

Pin Signal Pin Signal

20 GND 19 D0

18 D1 17 D2

16 D3 15 D4

14 D5 13 D6

12 D7 11 D8

10 D9 9 D10

8 D11 7 D12

6 D13 5 D14

4 D15 3 CLK1

2 CLK2 1 +5V

Create a setup disk for the HP Logic Analyzer, so that all the BOLD

Italicised signals are available for viewing when required by the tests which follow.

CDF Signals are connected to the Port as follows: Port J7 - POD 1 Pin Signal Pin Signal 20 GND 19 CDF_TDC_CAL0* 18 CDF_RowA1 17 CDF_TDC_CAL1* 16 CDF_RowA2 15 CDF_TDC_CAL2* 14 CDF_RowA3 13 CDF_TDC_CALIB 12 CDF_RowA4 11 No Connect 10 CDF_RowA5 9 CDF_TDC_DONE 8 CDF_CLOCK 7 CDF_RowC7 6 No Connect 5 CDF_RowC8 4 CDF_RowA8 3 CDF_CLOCK 2 No Connect 1 No Connect Port J8 - POD 2 Pin Signal Pin Signal 20 GND 19 CDF_RowC9 18 CDF_BC* 17 CDF_RowC10 16 CDF_B0* 15 CDF_RowC11 14 CDF_RowA11 13 CDF_GLIVE* 12 CDF_L1A* 11 CDF_L1_CALIB* 10 CDF_L1R* 9 RSVD_L1W2* 8 CDF_L2B0* 7 CDF_STOP* 6 CDF_L2B1* 5 CDF_TEST* 4 CDF_HALT* 3 CDF_CLOCK 2 No Connect 1 No Connect Port J9 - POD 3 Pin Signal Pin Signal 20 GND 19 CDF_RUN* 18 CDF_RowA17 17 CDF_RL0* 16 CDF_RECOVER* 15 CDF_RL1* 14 CDF_RowA19 13 CDF_RL2* 12 CDF_ABORT* 11 CDF_CALIB3* 10 CDF_CALIB0* 9 CDF_CALIB4* 8 CDF_RowA22 7 CDF_CALIB5* 6 CDF_CALIB1* 5 CDF_CALIB6* 4 CDF_CALIB2* 3 CDF_CLOCK 2 No Connect 1 No Connect Port J10 - POD 4 Pin Signal Pin Signal 20 GND 19 CDF_CALEN* 18 CDF_RowA25 17 CDF_RowC26 16 CDF_ERROR* 15 CDF_L2R* 14 CDF_L2A* 13 CDF_L2A_EN* 12 CDF_L2BD0* 11 CDF_EVID0* 10 CDF_RowA29 9 CDF_EVID1* 8 CDF_L2BD1* 7 CDF_EVID2* 6 CDF_RSVD0* 5 CDF_EVID3* 4 CDF_RSVD1* 3 CDF_CLOCK 2 No Connect 1 No Connect

Master Clock Interface

______ For this test, the TESTCLK module must be used.

Prior to inserting the TESTCLK, make sure that the TESTCLK jumpers S13 and S14 are removed .

______ Now, from VASE, select the TESTCLK submenu. Go to the TSIE submenu and turn on the Cable clock driver.

Now connect the Clock Cable between TESTCLK and TRACER front panel connector J2 page 5.

With an o-scope or Logic Analyzer, view the four clock signals on the following front panel connector.

CDF_CLOCK

CDF_BC*

CDF_B0*

CDF_ABORT*

Trigger on CDF_B0*, and verify the pattern looks as pictured below.

______ Change the scale of the clock signals and put the Logic Analyzer in �Accumulate On� mode.

Verify that the clock signals are not drifting.

TSI Interface

______ The TSI (Trigger System Interface) interface will now be tested. To do this, the TESTCLK will again be used. The Clock cable (J2 page5) must be connected between the TESTCLK and

TRACER as well as the Fiber Optic Cable (U15 page 9). Within VASE: Tracer Checkout Menu, select the TSI Interface Test option. The program enables the Cable Clock, and sets TSIE start wait condition on the Testclk.

______ Prior to starting test, set the Logic Analyzer to trigger off STOP* going low.

The TSI Interface Test software will:

• Enable the Cable Clock at the TESTCLK.

• Set the �Enable CDF Trigger Signals to backplane� bit in the Tracer�s Control Register

• Load the TESTCLK TSIE FIFO and Enables the transmission of the tsi trigger file �toggle_all.tsi�.

______ Trigger on STOP going low, and you should see the following patterns:

Automatic Testing of Trigger Sum bits Using CBSS Module This test will use the CBSS module to verify what you have visually observed above. This test requires that you have a TESTCLK, CBSS and the TRACER under test installed in the crate. ______ Assert CDF_ERROR* on the backplane by using special Error generator module. ______ Now within Vase and the TRACER Checkout Menu, select the TRACER -> CBSS Trigger Test The test will:

• Setup the TESTCLK so that the cable clock is on and the clock cable is installed between the TESTCLK and the TRACER.

• Set the Wait for B0 bit on the TESTCLK. • On the CBBS board, clear the FIFOs and make sure the Enable VME access bit is low. • Have the TESTCLK send the file �CBSS_test.tsi� in looping mode. • Check to verify that the FIFOs on the CBSS have filled • Enable VME access in the CBSS Control Register • Verify that the contents of the FIFO matches a known comparison file

___ Next, run the Tracer -> CBSS Trigger Test in Loop Mode for at least 100 loops.

Test of the Start Scan Register

The Start Scan Register receives its information from the Level 2 word sent from the TSI. To perform the next level of testing, you will send TSI patterns from the TESTCLK to set Start Scan Register bits.

______Within VASE: Tracer Checkout Menu, select the TSI - Start Scan Test . The Clock cable J2 page5) must be connected between the TESTCLK and TRACER as well as the Fiber Optic Cable

(U15 page 9).

The test program performs the following tests:

• Check that the test enables Testclk Cable Clock. And sets the TSIE Start Wait condition.

• Set the DONE bit in the DONE register.

• Load the TSIE file START_SCAN.tsi

Read the Start Scan Register and verify that the Start Scan bit is set. All other bits (besides the

CDF_TDC_DONE) should be low.

• Set the DONE bit in the DONE register.

• Load the TSIE file EVID0.tsi

Read the Start Scan Register and verify that the Event ID 0 bit is set. All other bits (besides the

CDF_TDC_DONE) should be low.

• Load the TSIE file EVID1.tsi

Read the Start Scan Register and verify that the Event ID 1 bit is set. All other bits (besides the

CDF_TDC_DONE) should be low.

• Load the TSIE file EVID2.tsi

Read the Start Scan Register and verify that the Event ID 2 bit is set. All other bits (besides the

CDF_TDC_DONE) should be low.

• Load the TSIE file EVID3.tsi

Read the Start Scan Register and verify that the Event ID 3 bit is set. All other bits (besides the

CDF_TDC_DONE) should be low.

• Load the TSIE file L2B0.tsi

Read the Start Scan Register and verify that the L2 Decision Buffer Address 0 bit is set. All other bits

(besides the CDF_TDC_DONE and Start Scan) should be low.

• Load the TSIE file L2B1.tsi

Read the Start Scan Register and verify that the L2 Decision Buffer Address 1 bit is set. All other bits

(besides the CDF_TDC_DONE and Start Scan) should be low.

• Load the TSIE file RL0.tsi

Read the Start Scan Register and verify that the Readout List 0 bit is set. All other bits (besides the

CDF_TDC_DONE and Start Scan) should be low.

• Load the TSIE file RL1.tsi

Read the Start Scan Register and verify that the Readout List 1 bit is set. All other bits (besides the

CDF_TDC_DONE and Start Scan) should be low.

• Load the TSIE file RL2.tsi Read the Start Scan Register and verify that the Readout List 2 bit is set. All other bits (besides the CDF_TDC_DONE and Start Scan) should be low.

• Load the TSIE file CAL0.tsi Read the Start Scan Register and verify that the Calibration bit 0 bit is set. All other bits (besides the CDF_TDC_DONE and Start Scan) should be low.

• Load the TSIE file CAL1.tsi Read the Start Scan Register and verify that the Calibration bit 1 bit is set. All other bits (besides the CDF_TDC_DONE and Start Scan) should be low.

• Load the TSIE file CAL2.tsi Read the Start Scan Register and verify that the Calibration bit 2 bit is set. All other bits (besides the CDF_TDC_DONE and Start Scan) should be low.

• Load the TSIE file CAL3.tsi Read the Start Scan Register and verify that the Calibration bit 3 bit is set. All other bits (besides the CDF_TDC_DONE and Start Scan) should be low.

• Load the TSIE file CAL4.tsi Read the Start Scan Register and verify that the Calibration bit 4 bit is set. All other bits (besides the CDF_TDC_DONE and Start Scan) should be low.

• Load the TSIE file CAL5.tsi Read the Start Scan Register and verify that the Calibration bit 5 bit is set. All other bits (besides the CDF_TDC_DONE and Start Scan) should be low.

• Load the TSIE file CAL6.tsi Read the Start Scan Register and verify that the Calibration bit 6 bit is set. All other bits (besides the CDF_TDC_DONE and Start Scan) should be low.

___ Next, run the TSI - Start Scan Test Loop for at least 100 loops.

Test of the Done bit in the DONE Register

The Done bit is set over VMEbus and reset whenever a Start Scan is received from the TSI.

______ From the VASE: Tracer Checkout Menu, select the TSI - Done Test option and verify the following:

• Test will verify that it can set the DONE bit.

______ Verify the DONE LED (D3 on page 10)turns on.

• Test loads the TSIE file START_SCAN.tsi.

• Test verifies that the DONE bit in the Done Register has been reset.

______ Verify the DONE LED (D3 on page 10)turns off.

• Test verifies that the Start Scan bit in the Start Scan Register has been set.

• Test will now again write the DONE bit and verify it has been set.

• Verify that the above step has reset the Start Scan bit in the Start Scan Register.

______ Next, run the TSI - Done Test Loop Mode for at least 100 loops.

TSI Diagnostic FIFO

It is possible for the TSI to turn on the input to the TSI Diagnostic FIFO by sending the �TEST� bit in the TSI Control Word. When �TEST� is sent, the FIFO is flushed and the next 8K data words received from the TSI to be clocked into a FIFO. In its this operating mode, once the FIFO is full, no further data recording will be done. In order to repeat the test, the original �TEST� state must be cleared by toggling the �resettsi test� bit in the Control Register.

______ From the VASE: Tracer Checkout Menu, select Testclk - Tracer TSI Diagnostic FIFO TEST Mode Test option.

The test will perform the following:

• Turns on the Cable Clock at the TESTCLK.

• Clears any possible ERROR state by toggling the �Reset TSI Taxi Error� bit (high then low) in the Control Register.

• Sets the �Enable CDF Trigger Signals tobackplane� bit in the Control Register

• Sets the TSI �TEST� bit low by downloading the following tsie pattern to TESTCLK and sending it across the optical link.

H000 "L1 word - nothing active H003 "Control word - clear TEST H000 "L1 word - nothing active

• Begins by toggling (high and then low) the �Reset TSI Diagnostic FIFO TEST mode� bit.

• Resets the TSI Diagnostic FIFO by toggling the �Reset TSI Diagnostic FIFO� bit.

• Verifies the TSI Diagnostic FIFO is empty by checking the FIFO status in the Control register.

• Downloads a tsie pattern to the TESTCLK which will turn on the �TEST� mode and then send across random data.

The first active lines of this file should be

H000 "L1 word - nothing active H013 "Control word - set TEST H000 "L1 word - nothing active H003 "Control word - clear TEST H000 "L1 word - nothing active �. To be followed by 8K of random data in the range of H000 to H1FF.

• The TSI Diagnostic FIFO should fill up. Verifies this by checking the FIFO status in the Control register.

• Resets the TEST mode state by toggling (high and then low) the �Reset TSI Diagnostic FIFO TEST mode� bit. This will prevent the FIFO from continuing to fill as we read it out.

• Reads out the FIFO information and compare it to what was downloaded.

___ Next, run the Loop Mode - Testclk -> Tracer TSI Diagnostic FIFO TEST Mode Test at least

100 loops.

______ Also, while CDF_ERROR* is asserted, observe the ERROR Front Panel LED (D4 on page 10).

The LED should be on.

______ Check the ERROR mask by setting the �Mask CDF_ERROR� bit in the Control register. The

ERROR LED should go off.

______ Now reset the �Mask CDF_ERROR� bit in the Control register. The ERROR LED should come on again.

______ Now clear the CDF_ERROR* signal being asserted by the small circuit card.

______ Clear the ERROR state by toggling the �Reset TSI Taxi Error� bit (high then low) in the Control

Register.

______ The ERROR LED (D4) should turn off.

______ Now TSI Diagnostic FIFO read and write activity should begin again. Observe the activity on the

READ* pin (U17-18 on page 10) and WRITE* pin (U17-2). Both should contain a train of pulses.

TSI Return Cable The TSI Return Cable is a copper link which returns the signals DONE, ERROR, and BUSY to the TSI. The state of these signals is also visible by looking at the Front Panel LEDs (page 10). DONE Previously observed and checked. ERROR Previously observed and checked. BUSY BUSY will be set to a logic high state in two possible ways.

The default TSI Busy uses the status of the EVENT FIFO Flags. Bit 0 of the Control Register should be low. The Event Status Level that the busy operates off can be programmed with bits (3:1) of the Control Register. By default, TSI BUSY will turn on when the Event FIFO becomes greater than half full. ______ From VASE: Tracer Checkout Menu, select Busy Test. The test will perform the following: • Set bit 0 of the Control Register low. • Set Control Register bits (1) low (2) high (3) high • Reset the Event FIFO _____ Verify the BUSY LED is OFF • Partially fill the EVENT FIFO to more than half full by writing 4,100 words into it. _____ Verify the BUSY LED is ON • Reset the Event FIFO. _____ Verify the BUSY LED is OFF. • Set Control Register bits (1) high (2) low (3) low ______ Verify the BUSY LED is ON.

Secondly, Busy can be set when the VME buffer space in the VME Readout Buffer (VRB) is approaching full.

• To do this, set the Select the TAXI-Test Busy as the source for the TSI Busy. Do this by setting bit 0 of the Control Register high.

You can simulate this state with the Taxi Test module. Transmit a Busy condition over a Fiber Optic

Cable plugged into U26 (page 8) on the front panel. In the Taxi-Test Menu select the RX # Control

Menu and enable the BUSY SET bit.

______ The BUSY LED should turn on, and

• VRB Busy bit in the Control Register should be set.

Local Teststand Calibration

Calorimetry

The Tracer has the capability of driving the following lines for doing a teststand calibration: VME_DTACK* CDF_L1A* CDF_L1R* CDF_L2B0* CDF_L2B1* CDF_HALT* CDF_RECOVER* CDF_CALEN* CDF_CALIB0* CDF_CALIB1* CDF_CALIB2* CDF_CALIB3* CDF_CALIB4* CDF_CALIB5* CDF_CALIB6* CDF_RL0* CDF_RL1* CDF_RL2* CDF_TDC_CAL0* CDF_TDC_CAL1* CDF_TDC_CAL2* CDF_CLOCK

A typical Calibration sequence will look as follows:

(Make sure that the rising edge of CDF_CLOCK validates all the gated trigger signals shown below.)

Particle Physics Division/CDF Upgrade ProjectTTACER Checkout Procedure

3

CDF_L1A*

CDF_HALT*

CDF_RECOVER*

CDF_CALEN*

CDF_L1R*

CDF_L2B(1:0)*

...

... ... ... ...

... ... ...

...

0 1 2

VMEbus

DTACK*

set by Start

Delay Register

set by lower

16 bits of the

Calibration Delay

Register

set by upper

16 bits of the

Calibration Delay

Register set by Halt

Delay Register

CDF_CALx*

CDF_RLx*

The following sequence is involved in the Local Teststand Calorimetry Calibration:

• Issue a Calibration command by writing to the TRACER Calibration Register.

• Tracer will wait programmed time, determined by the TRACER Start Delay Register.

• Tracer will issue Halt - Reset - Run sequence.

• Tracer will wait programmed time, determined by the TRACER Calibration Enable Delay Register.

• Tracer will issue Calibration Enable.

• Tracer will issue four successive L1 Accepts at a programmed number of crossings (set in the Calibration Delay Register) after calibration enable. These L1 Accepts will occur a programmed number of CDF_CLOCK cycles after the CDF_CALEN* pulse. The successive L1 Accepts will fill buffers 0, 1, 2 and 3 in that order.

• Tracer will wait a programmed delay, determined by the TRACER Halt Delay Register.

• Tracer will issue Halt (if halt mode enabled).

• Tracer will set a bit in a register to indicate process is done.

______ From VASE: Tracer Checkout Menu, select Teststand Calibration Test. Verify the following pictures with a Logic Analyzer.

The test performs the following: (NOTE: timing mentioned in each step is not observable until you get to the step which writes to the Calibration Register.)

• Turns on the Cable Clock at the TESTCLK.

• Sets the �Enable CDF Trigger Signals tobackplane� bit in the Control Register

• Sets the �CDF Trigger Signal Source� to �1� to select the Local CalibrationSequencer.

This is set in the Tracer�s Control Register.

• Writes to the Start Delay Register. Each count equals 132ns, and a typical value to be set is 1ms, for a count of 1D97(hex). This value controls how long the Tracer waits to begin the Calibration sequence following a write to the Calibration Register. You can measure this with the Logic analyzer by looking at the time difference between the VME DTACK* line from the write to the Calibration Register to the assertion of CDF_HALT*

• Writes two values to the Calibration Delay Register. The lower 16 bits (example 1 sets this to 4 hex, example 2 sets this to 13 hex) represents how many clock cycles to wait before issuing CDF_CALEN* following the Halt-Recover-Run sequence. You can measure this with the Logic analyzer by looking at the time difference between the signal CDF_HALT* to the assertion of CDF_CALEN*

The upper 16 bits (example 1 sets this to 8 hex, example 2 sets this to 29 hex) control the number of CDF_CLOCK cycles after CDF_CALEN* until the sequence of four

CDF_L1As occur. Typically, this value will be set to 29(hex). You can measure this with the Logic analyzer by looking at the time difference between the signal CDF_CALEN* to the assertion of CDF_L1A*

• Writes to the Halt Delay Register. This is an eight bit register which controls the number of CDF_CLOCK cycles (examples set this to 03 hex) following the L1As until

CDF_HALT* is issued (assuming the �Enable Halt Mode� bit is set in the Calibration

Register). You can measure this with the Logic analyzer by looking at the time difference between the signal CDF_L1A* to the assertion of CDF_HALT*

• Writes to the Calibration Register. Writing to this register will begin the sequence. The

�Local Calibration Enable� bit must be set, along with a value for Calibration Enables

(6:0). You should observe CDF_CAL(6:0)* backplane lines which match the value you gave it. (Example enables CDF_CAL0*, CDF_CAL1* and Halt Mode).

• When the sequence is done, reads the Calibration Done Register and verifies that the

�Teststand Calibration Done� bit has been set. (This bit is cleared at the beginning of each Local Teststand Calibration sequence.)

Example 1) start delay = 1D97 (~1ms) calen delay = 4 (note CALEN* occurs 4+1 cycles after HALT*) l1 delay = 8 (note L1A* occurs 8 cycles after CALEN*) halt delay = 3 (note HALT* occurs 3+1 cycles after last L1A*)

Example 2) start delay = 1D97 (~1ms) calen delay = 13 hex (note CALEN* occurs 13+1 hex cycles after HALT*) l1 delay = 29 hex (note L1A* occurs 29+1 hex cycles after CALEN*) halt delay = 3 (note HALT* occurs 3+1 cycles after last L1A*)

Zoom in on timing between HALT* and CALEN*. Note timing matches predicted delay of

2.5us.

Zoom in on timing between CALEN* and L1A*. Note number of crossings and timing matches predicted delay of 5.4us.

TDC Calibration Pulses

It is also possible to trigger the TDC Calibration pulses trig(0) trig(1) trig(2)

CDF_TDC_CAL0*

CDF_TDC_CAL1*

CDF_TDC_CAL2* from control of the local teststand calibration used for the calorimetry.

______ In order to trigger the CDF_TDC_CAL(2:0)* pulses it is necessary to select from the

VASE: Tracer checkout Menu, TDC Calibration Test. Verify the following pictures with a Logic analyzer.

The test will perform the following:

• Writes to the TDC Calibration Pulses Enable Register and enable the pulse or pulses which you want to test.Example enables all three pulses.

• Writes to the TDC Calibration Course Delay Register. This register will allow you to set the number of CDF_CLOCK cycles which occur prior to firing the TDC trigger pulses trig(2:0) (page 9). Example sets course delays of 3, 4 and 5 for CDF_TDC_CAL0*,

CDF_TDC_CAL1*, and CDF_TDC_CAL2*. Note that the true delay is always the programmed number plus one.

• These trigger pulses, trig(2:0), now go to rest of the TDC calibration pulse logic. It is necessary to write to the TDC Calibration Fine Delay register (Example sets all Fine

Delay values to 0 , 80 and FF hex).

• Sets the TDC Calibration Width Delay Register (Example sets all values to 7 hex) to have further control over the pulse width and timing.

Note the delay of 82 ns between TRIG0 and TDC_CAL0*. This is the inherent delay of the programmable pulse generator.

Note the delay of 210 ns between TRIG1 and TDC_CAL1*. This is the sum of the inherent delay (~82ns) plus half scale of the full range (~265ns).

Note the delay of 346 ns between TRIG2 and TDC_CAL2*. This is the sum of the inherent delay

(~82ns) plus full scale of the full range (~256ns).

Event Data FIFO The TRACER has an optical data link to the VRB. This link uses the TAXIchip (AM7968-175JC) protocol and AMP optical driver (AMP 269049-1). It operates at two times the CDF_CLK. An 8K by 32 bit Event FIFO feeds this data link. It is possible to fill this Event FIFO in two ways. One way is to simply do a VMEbus write into the FIFO. If the VRC is used to do zero suppression and data formatting, this method would be used. The VRC would first read in raw event data, do the formatting and then write the formatted data to the Event FIFO.

A sequencer on the TRACER detects when data is present in the FIFO, serialize the data through the use of a TAXIchip, and transmit it upstairs to the Readout Memory (VRB) module via an optical link. The data can be transmitted to the VRB at a rate of up to one byte every 66 ns (twice the CDF clock). A Taxi Sync signal is sent up at least every 5 bytes; thus, a data rate of 4 Bytes/(5 x66ns), or 12.1 MB/s is achievable out of the crate. ______ Connect dual optical cable between Tracer�s Event data and Busy Ports to the Taxi-Tester Data and Busy Ports.

______ From VASE: Tracer Checkout Menu, select Tracer -> Taxi-Test Test . The test will perform the following: • Make sure the Testclk is driving the Cable Clock to the TRACER. • Make sure that the �Event Data Taxi Enable� in the Tracer�s Control Register is set low. • Load the Tracer�s Event Data FIFO with Sequential Data. The FIFO flags should indicate a high state.

• Enable the Taxi-Tester Module so that it is ready to accept data. (Enable receive mode, clear the FIFO, reset the flags, wordcount, and enable BUSY).

• Now, set the �Event Data Taxi Enable� in the Tracer�s Control Register. • Data will flow from Tracer to Taxi-Tester until the FIFO on Taxi-Tester becomes almost full. • At this point the Taxi-Tester will send BUSY. Verify that you see the Front Panel WAIT LED turn on.

• In order to clear the WAIT state, read out the FIF0 on the Taxi-Tester until its status is empty - you should observe the sequential data.

• You should see the Event FIFO status flags indicate Empty as well when you read them. • Now (leaving the �Event Data Taxi Enable� bit set in the Tracer�s Control Register), fill the Event FIFO with random data.

• Data will flow from Tracer to Taxi-Tester. Repeat the readout of the Taxi-Tester FIFO until it is empty.

• You should also see the Event FIFO status flags indicate Empty when you read them. • Now look at the data in the Taxi-Tester FIFO. It should be identical to what was sent.

Spy Mode Test of VMEbus Reads

A second method for getting event data to the VRB would involve using the TRACER’s Spy capability.

The TRACER will have the capability to spy on the data as the VMEbus Readout Controller (VRC) reads it out. During event readout, the TRACER has the ability to clock data into the Event FIFO. The data which gets clocked into the event FIFO includes any VMEbus reads of data in the L2 Buffer Space (specified in

CDF/DOC/TRIGGER/CDFR/2288), and any write to the Done Register which sets the EOB marker. This

Spy mode would be used only if there is no need for the VRC to do data formatting.

______ Connect dual optical cable between Tracer�s Event data and Busy Ports to the Taxi-Tester Data and Busy Ports

______ From VASE: Tracer Checkout menu, select Tracer -> Taxi-Test in Spy Mode and verify the following:

The test will perform the following:

• Make sure the Testclk is driving the Cable Clock to the TRACER.

• Make sure that the �Event Data Taxi Enable� in the Tracer�s Control Register is set low.

• Set the �Spy Mode Enable� bit in the Tracer�s Control Register.

• Now fill the Event FIFO with sequential data read from some other memory module on the

VMEbus - a possible source is the ADMEM�s Diagnostic FIFO.

• Readout the Tracer�s Event FIFO and verify the match between it and the source.

• Now repeat the fill of the Event FIFO with sequential data read from the other memory module on the VMEbus.

• This time transmit the data to the Taxi-Tester by:

• Enable the Taxi-Tester Module so that it is ready to accept data. (Enable receive mode, clear the

FIFO, reset the flags, wordcount, and enable BUSY).

• Now, set the �Event Data Taxi Enable� in the Tracer�s Control Register.

• Data will flow from Tracer to Taxi-Tester until the FIFO on Taxi-Tester becomes almost full.

• At this point the Taxi-Tester will send BUSY. Verify that you see the Front Panel WAIT LED turn on.

• In order to clear the WAIT state, read out the FIF0 on the Taxi-Tester until its status is empty - you should observe the sequential data.

• You should see the Event FIFO status flags indicate Empty as well when you read them.

• Make sure that the Violation Flag on the Taxi-Tester remains low.

Spy Mode Test of VMEbus Reads of Tracer�s Event Space Registers

• Make sure the Event FIFO is empty - this can be done by toggling software reset or toggling the �Event Data Taxi Enable� bit.

Reads of the Tracer�s �Event Space� registers should be captured by the Event FIFO in Spy mode. These registers include:

Word Count Register Event Header Register TSI TAXI Violation Counter Register A�s Pattern Register 5�s Pattern Register

• With �Spy Mode� enabled and the �Event Data Taxi Enable� bit set low, readout the above registers.

• Now readout the Event FIFO. The contents of the Event FIFO should match exactly with the contents of the registers just read out. Verify this.

Spy Mode Test of VMEbus write to the Tracer�s Done Register and setting of EOB (End of Block)

It is possible to append set an End of Block (EOB) marker on the transmitted data stream. This is done by writing to the EOB bit in the Done register. Whenever a logic high is written to this bit, the equivalent of a

33 bit word will be clocked into the Event FIFO. The MSB will be set high and will indicate the EOB.

This EOB bit will be passed to the TaxiChip as the 9th data bit, which can then be decoded as EOB by the

VRB.

______ Connect dual optical cable between Tracer�s Event data and Busy Ports to the Taxi-Tester Data and Busy Ports.

______ From VASE: Tracer Checkout menu, select Tracer -> Taxi-Test Spy - EOB Test .

The test will perform the following:

• Make sure the Testclk is driving the Cable Clock to the TRACER.

• Make sure that the �Event Data Taxi Enable� in the Tracer�s Control Register is set low.

• Make sure the Event FIFO is empty - this can be done by toggling software reset or toggling the �Event

Data Taxi Enable� bit.

• Set the �Spy Mode Enable� bit in the Tracer�s Control Register.

• Write to the Tracer�s DONE register. Bit 31 must be set in order to cause an EOB.

The EOB marker cannot be read on the Tracer - it is set only as the data goes to the TAXI link.

• Enable the Taxi-Tester Module so that it is ready to accept data. (Enable receive mode, clear the FIFO, reset the flags, wordcount, and enable BUSY).

• Now, set the �Event Data Taxi Enable� in the Tracer�s Control Register.

• One word of data will flow from Tracer to Taxi-Tester.

• Readout the contents of the Taxi-Tester FIFO. There should be on word (four bytes).

• On the fourth byte which is read out, you should see that the ninth bit has been set. This is the EOB marker which we wrote to the Tracer�s Done Register.

______ Run the Tracer -> Taxi-Test Loop Mode Test Sequential Data for at least 100 loops.

______ Run the Tracer -> Taxi-Test Loop Mode Test Random Data for at least 100 loops.

______ Run the Loop Mode Test of Tracer -> Taxi-Test in Spy Mode for at least 100 loops.

______ Run the Tracer -> Taxi-Test in Spy EOB Loop Test for at least 100 loops.

Test Interrupt functionality The Clock cable must be connected between the TESTCLK and TRACER as well as the Fiber Optic Cable (U15 page 9). ______ Within VASE: Tracer Checkout Menu, select Interrupt Test. The test performs the following: • Enables the Cable Clock and TSIE Start Wait condition on Testclk. • Enables the Interrupt mode on the TRACER by setting the �Interrupt Mode Enable� bit in the Tracer�s Control Register.

• Sets the �Enable CDF Trigger Signals tobackplane� bit in the Control Register • Connect the Interrupt Handler by doing an RLOGIN to the MVME162 and executing the �inter� routine. This routine will generate an interrupt return vector which must be loaded into the lower 8 bits of the Tracer�s Interrupt return vector.

• Load the Tracer�s Interrupt return Vector at the prompt. • The test loads the TSIE file START_SCAN.tsi Reads the Start Scan Register and verifies that the Start Scan bit is set. All other bits (besides the CDF_TDC_DONE) should be low.

• The setting of the Start Scan bit should generate an interrupt which prints a message to the screen the Interrupt Handler is running on.

Tracer Transition Module Port

The Tracer has a Transition Module Port on it. In order to use this port, one must first write a address to the

Transition Port Address Register. The transition module register is then accessible by reading or writing to the Transition Port Read/Write Register.

______ From VASE: Tracer Checkout Menu, select Transition Card Test

The test will perform the following:

• Writes a unique pattern to each register.

• Reads out each register and compares data.

• Rotates a 1 through a field of 0�s in each register.

• Rotates a 0 through a field of 1�s in each register.

48

Particle Physics Division/CDF Upgrade ProjectTTACER Checkout Procedure

49

PC

V R C

T R A C E R

T E S T C L K

V R C

R E S E T

A D M E M

T A X I F I F O

Clock Cable TSI Trigger

Event Data Out

Event Data Readout

TRACER CHECKOUT CRATE

CDF RESET Crate

Reset