ac/dc

208V

DV DD

DV DD2

AV DD

GND

Cont rol

&

Link

0V

Vcc

Module

Pow er

Suppl ies

Figure 2- Ve rsion w ith low volt age bus Vcc. The li nk ground has t o be connected t o 0v.

The load is connected to graound at t he Port C ard. The rack and c rate are c onnec ted t o the AC m ains safet y ground.

Laye rs

Junc tion

Box Port C ard