Recognition of tagging jets from qq->qqH, M_H=135 GeV in HF with HF Trigger Tower Selection of tagging jets with cut on max. HF Trigger Tower (2x2 HF towers)

1-3 % of false jets is OK for off-line => E_t^{thr} =18 - 20 GeV what E_t^{thr} on HF triger towers is acceptable for L1 e + 3j ? Next plot - efficiency curve for HF tower threshold 18 GeV