Conducting shell stabilization of n=1 tilt mode in oblate FRC

MHD simulations, E=0.6

1e-07

1e-05

0.001

0.1

0 1 2 3 4 5 tA

|V |^1_2

(a)

(b)

(a) without conducting shell

(b) with close fitting conducting shell

t=0.

t=4t (a) A

[Belova,99]