... and a state of the art detector

ffl High bandwidth DAQ, 500 MHz digitization, state-of-the-art detectors. ffl Proven background rejection to 10^{�11} (parts per trillion). ffl Final E787 sensitivity will reach the SM level (ˇ 10^{�10}).