Stainless SteelCopperEB Weld3 . 3 . 4

Leak Check.Weldments shall be leak checked prior to assembly.Leak checking procedure is defined in specification 410201-00095 (see paragraph 3.3.1above).3.3.5

Fasteners. All bolts and screws in vacuum or used in ConFlat typevacuum flanges shall be silver plated. All screws used in blind tapped holes shall bevented.3 . 4

Assembly and Workmanship.3.4.1 The parts shall be free of burrs and sharp edges, and free of dents,gouges and scratches.3.4.2 The parts shall be clean and free of dirt, oil and grease with theexception of the appropriate lubrication on moving bearing surfaces. Bearing surfacesshall be lubricated as required by the assembly drawing.3.4.3 All assemblies shall be leak checked. Leak checking procedure isdefined in specification 410201-00095 (see paragraph 3.3.1 above).

A R G O N N E N A T I O N A L L A B O R A T O R Y 4102020101-00015

Title:Technical Specification for BM Front EndFixed Mask And Photon ShuttersR e v . 0 0 ApprovedDate

Page

11˚ of

˚ ˚ 1 1 ˚ ˚

ANL-242 (3-83)5 . 4 Assemblies must be secured for shipment in fashion that protects the assemblyfrom dust, dirt and weather or water damage. The assemblies must be securelyfastened, padded, boxed and/or crated for shipment in a suitable manner for preventionof shipment damage to any assembly and its weather/dust protection and insure theirsafe delivery to the Laboratory.