A R G O N N E N A T I O N A L L A B O R A T O R Y 410201-00101

Title:Technical Specification For Lead CollimatorsAnd Ratchet Wall ShieldingR e v . 0 1 ApprovedDate

Page

11˚ of

˚ ˚ 1 1 ˚ ˚

ANL-242 (3-83)5 . 0

PREPARATION FOR DELIVERY5 . 1

Package Identification:Each assembly shipped shall be identified bythe appropriate purchase order number, assembly number and a sequential identity orserial number.5 . 2

Moving Components: Any moving components on an assemblymust be firmly secured for shipment in a manner that precludes damage from motionand vibration. The contractor shall advise ANL prior to shipment on the intendedmeans of securing the tungsten blocks for shipment. If removal of the blocks isintended, the removal and handling of the blocks must be compatible with specification410201-00095 (see 5.3 below), and the contractor must make arrangements with ANLfor the installation of the blocks into the shutter-collimator assembly at ANL.5 . 3

Vacuum components: Vacuum components must be prepared forshipment in accordance with specification 410201-00095,

Vacuum Requirements Of

Ultra High Vacuum Devices For Beamlines.5 . 4

Protection: Assemblies must be secured for shipment in fashion thatprotects the assembly from dust, dirt and weather or water damage. The assembliesmust be securely fastened, padded, boxed and/or crated for shipment in a suitablemanner for prevention of shipment damage to any assembly and its weather/dustprotection and insure their safe delivery to the Laboratory.