* * * * * * * * * *

READ AND REMOVE THIS PAGE BEFORE PLACING
THE SPECIFICATION SECTION IN THE CONTRACT
			
* * * * * * * * * *

DIVISION 1:  GENERAL REQUIREMENTS

SECTION 01009 ‑ GENERAL INFORMATION AND REQUIREMENTS

Use:	Guidance relating to labor, equipment, supplies, and materials, [except for specified Government‑furnished property].

NOTES TO SPECIFIER:

	A.	Options within paragraphs are identified by enclosure in brackets; blank spaces enclosed by brackets [_____] provide for information to be inserted, as appropriate, to individual projects.

	B.	TO AVOID CONFLICTING REQUIREMENTS AND COSTLY MISTAKES, the specifier must edit (delete, substitute or add to the text).  The remaining paragraphs must be renumbered.

	C.	DELETE FOR FINAL COPY: Notes to the Specifier, located between lines of asterisks; all [brackets], underlining, boldface, and italics, within the paragraphs; and this page.  (Open Reveal Codes [alt F3] to do this accurately.)

	D.	To Edit “(Footer B)”: (Corel 8).  ENTIRE FOOTER SHOULD BE BOLDED.  Click in the footer and delete the “Project Name (ftr B)” text and replace it with the Name of the Project (upper and lower case).  Replace date with current MM/YY (WITHOUT BRACKETS).

	E.	The Guide Specifications are intended to be continuously reviewed and revised.  User’s technical comments are appreciated.  Also, other related or similar specification that are written “from scratch” that could benefit others, or other questions can be sent to NSTC A/E Group, ST 110, or call (303) 987-6868.

DRAWING DATA REQUIRED:  Use the following standard drawings as appropriate:

REVISIONS OF THIS SECTION:
CSI format, editorial changes: 11/01
Reference Standards:  7/96
Metric:  
Technical, Products update:  7/96

													

SECTION 01009

GENERAL INFORMATION AND REQUIREMENTS

PART 1:  GENERAL

1.1	SUMMARY

*******************************************************************************
INSERT A BRIEF SYNOPSIS OF THE WORK TO BE PERFORMED, (E.G. CONSTRUCT APPROXIMATELY 15 MILES OF BARBED WIRE FENCE; REPAIR 16 STOCKWATER RESERVOIRS; CHAIN AND SEED APPROXIMATELY 2,000 ACRES OF RANGELAND).
*******************************************************************************

A.	Description of Work:  Furnishing labor, equipment, supplies, and materials, [except for specified Government‑furnished property,] to [                   ].

B.	Location:  Work under this Contract is located in [            ] County, [            ].  [The work site is at the [________________.]] [The work locations are shown on the drawings.]

C.	Work Data Sheet:  Designates the type and quantity of work required at each project location, and dimensions required for typical drawings.

1.2	REFERENCES

*******************************************************************************
EDIT OUT UNNEEDED AND ADD ANY REFERENCES NOT LISTED.  MAKE SURE ALL REFERENCES CITED IN THE TECHNICAL SECTIONS ARE INCLUDED AS THIS IS THE ONLY PLACE THEY SHOULD BE SHOWN IN FULL TEXT INCLUDING PUBLICATION DATE.
*******************************************************************************

A.	Referenced Specifications/Standards with Abbreviations and/or Acronyms:  Wherever the following acronyms are used in these specifications or on the drawings, they are to be construed the same as the respective expressions represented.  Copies of the referenced specifications/standards referred to herein may be procured by the Contractor, from the following:

	AA		Aluminum Association, Inc.
				900 19th Street, N.W., Suite 300
				Washington, DC  20006

	AA	30-86			Aluminum Structures Construction Manual
	AA 45-80				Designation System for Aluminum Finishes

	AABC	Associated Air Balance Council
				1518 K Street, N.W.
				Washington, DC  20005

	AABC‑1982			National Standards for Total System Balance

	AAMA	American Architectural Manufacturers' Association
				1540 E Dundee Rd., Suite 310
				Palatine IL  60067

	AAMA 1601.1			Voluntary Thickness Acrylic Plastic Skylight Domes			
				AAMA 302.8			Aluminum Prime Windows
	AAMA SG‑1‑76			Dense Rubber‑like Compression Gasket Materials

	AAN		American Association of Nurserymen
	1250 Eye St., NW, Suite 500
	Washington, DC  20005

	AASHTO	American Association of State Highway and Transportation Officials
	444 North Capitol Street, N.W., Suite 249
	Washington, DC  20001

	AASHTO HBI 83 88		Standard Specifications for Highway Bridges
	AASHTO M 17‑88		Mineral Filler for Bituminous Paving Mixtures
	AASHTO M 20‑70		Penetration Graded Asphalt Cement (R1993)
	AASHTO M 29‑88		Fine Aggregate for Bituminous Paving Mixtures
	AASHTO M 36/M 36M 91	Corrugated Steel Pipe, Metallic‑Coated, for Sewers and Drains
	AASHTO M 43‑88		Sizes of Aggregate for Road and Bridge Construction
	AASHTO M 45‑92		Aggregate for Masonry Mortar
	AASHTO M 81‑92		Cut‑Back Asphalt (Rapid‑Curing Type) 
	AASHTO M 82‑75		Cut‑Back Asphalt (Medium‑Curing Type) (R1993)
	AASHTO M 85‑93		Portland Cement
	AASHTO M 86/86M-93		Concrete Sewer, Storm Drain, and Culvert Pipe
	AASHTO M 133-86		Preservatives and Pressure Treatment Process for Timber (R1993)
	AASHTO M 140‑88		Emulsified Asphalt (R1993)
	AASHTO M 143‑86		Sodium Chloride (R1993)
	AASHTO M 144‑86		Calcium Chloride(R1993)
	AASHTO M 147‑65		Materials for Aggregate and Soil Aggregate Subbase, Base and Surface Courses (R1993)
	AASHTO M 156‑89		Requirements for Mixing Plants for Hot‑Mixed, Hot‑Laid Bituminous Mixtures (R1993)
	AASHTO M 168-84		Wood Products (R1993)
	AASHTO M 170/170M 93	Reinforced Concrete Culvert, Storm Drain and Sewer Pipe
	AASHTO M 182 91		Burlap Cloth Made from Jute or Kenaf
	AASHTO M 190‑88		Bituminous Coated Corrugated Metal Culvert Pipe and Pipe Arches 
	AASHTO M 196/196M-92	Corrugated Aluminum Pipe for Sewers and Drains
	AASHTO M 197/M 197M-88	Aluminum Alloy Sheet for Corrugated Aluminum Pipe
	AASHTO M 198‑75		Joints for Circular Concrete Sewer and Culvert Pipe Using Flexible Water Tight Gaskets (R1993)
	AASHTO M 208-87		Cationic Emulsified Asphalt
	AASHTO M 218‑87		Steel Sheet, Zinc Coated (Galvanized) for Corrugated Steel Pipe
	AASHTO M 226‑80		Viscosity Graded Asphalt Cement (R1993)
	AASHTO M 232-84		Zinc Coating (Hot-Dip) on Iron and Steel Hardware (R1993)
	AASHTO M 240‑92		Blended Hydraulic Cement
	AASHTO M 247‑81		Glass Beads Used in Traffic Paint (R1993)
	AASHTO M 248‑91		Ready‑Mixed White and Yellow Traffic Paints
	AASHTO M 249‑79		White and Yellow Reflective Thermoplastic Striping Material (Solid Form) ® 1986)
	AASHTO M 252-93		Corrugated Polyethylene Drainage Tubing
	AASHTO M 268-94		Retroreflective Sheeting for Traffic Control
	AASHTO M 294-93		Corrugated Polyethylene Pipe, 12 to 36 Inch Diameter
	AASHTO M 304-91		Poly (Vinyl Chloride) (PVC) Profile Wall Drain Pipe and Fittings Based on Controlled Inside Dia.
	AASHTO T 11-91		Method of Test for Materials Finer Than 75 Micrometer (No.200) Sieve in Mineral Aggregate by Washing
	AASHTO T 26-79		Method of Test for Quality of Water to Be Used in Concrete (R1993)
	AASHTO T 27-93		Method of Test for Sieve Analysis of Fine and Coarse Aggregates
	AASHTO T 85-91		Test of Specific Gravity and Absorption of Course Aggregate
	AASHTO T 90-92		Method for Determining the Plastic Limit and Plasticity Index of Soils
	AASHTO T 96-92		Method of Test for Resistance to Degradation of Small Size Coarse Aggregate by Abrasion & Impact in the LA Machine
	AASHTO T 99-93		Method of Test for the Moisture‑Density Relations of Soils Using a 5.5 lb (2.5 kg) Rammer & a 12-inch (305 mm) Drop
	AASHTO T 103-91		Method of Test for Soundness of Aggregate by Freezing & Thawing
	AASHTO T 104-92		Method of Test for Soundness of Aggregate by Use of Sodium Sulfate or Magnesium Sulfate
	AASHTO T 134-92		Method of Test for Moisture Density Relations of Soil‑Cement Mixtures
	AASHTO T 164-93		Method of Test for Quantitative Extraction of Bitumen from Bituminous Paving Mixtures
	AASHTO T 180-93		Method of Test for Moisture Density Relations of Soils Using a 10-lb (4.54 kg) Rammer and 18-inch (457 mm) Drop
	AASHTO T 182-84		Method of Test for Coating and Stripping of Bitumen-Aggregate Mixtures (R1993)
	AASHTO T 191-93		Method of Test for Density of Soil in Place by the Sand Cone Method
	AASHTO T 205-86		Method of Test for Density of Soil In‑Place by the Rubber-Balloon Method (R1993)
	AASHTO T 211-90		Method of Test for Determination for Cement Content in Cement Treated Aggregate by the Method of Titration (R1993)
	AASHTO T 217-87		Method of Test for Determination of Moisture in Soils by Means of a Calcium Carbide Gas Pressure Moisture Tester (R1993)
	AASHTO T 224-86		Method of Test for Correction for Coarse Particles in the Soil Compaction Test (R1993)
	AASHTO T 230-68		Method of Test for Determining Degree of Pavement Compaction of Bituminous Aggregate Mixtures (R1993)
	AASHTO T 238-86		Method of Test for Density of Soil and Soil-Aggregate in Place Nuclear Methods (Shallow Depth) (R1993)
	AASHTO T 239-91		Method of Test for Moisture Content of Soil and Soil Aggregate in Place by Nuclear Methods (Shallow Depth)
	AASHTO T 248-89		Method of Tests for Reducing Field Samples of Aggregate to Testing Size

	AATCC	American Association of Textile Chemists and Colorists
	P.O. Box 12215
	Research Triangle Park, NC  27709-2215

	AATCC 8-95			Colorfastness to Crocking: 	
	AATCC  				Crockmeter Method
	AATCC 16-93			Colorfastness to Light
	AATCC 134-91			Electrostatic Propensity of Carpets

	ACI		American Concrete Institute
	P.O. Box 19150
				Detroit, MI  48219

	ACI 211.1-91			Standard Practice for Selecting Proportions for Normal, Heavyweight, and Mass Concrete
	ACI 301-89			Structural Concrete for Buildings
	ACI 304R-89			Guide for Measuring, Mixing, Transporting, and Placing Concrete
	ACI 305R-91			Hot Weather Concreting
	ACI 306R-88			Cold Weather Concreting
	ACI 315-92			Details and Detailing of Concrete Reinforcement
	ACI 318/318R-95		Building Code Requirements for Reinforced Concrete
	ACI 347R-94			Guide to Formwork for Concrete
	ACI 503.1-92			Bonding Hardened Concrete, Steel, Wood, Brick, to Hardened Concrete with a Multi-Component Epoxy Adhesive
	ACI 503.2-92			Bonding Plastic Concrete to Hardened Concrete with a Multi-Component Epoxy Adhesive
	ACI 506R-90			Guide to Shotcrete (R1995)
	ACI 506.2-90			Materials, Proportioning, and Application of Shotcrete
	ACI 506.3R-91			Guide to Certification of Concrete Nozzelmen

	ADAAG	Architectural and Transportation Barriers Compliance Board
	1331 F Street, NW, Suite 1000
	Washington DC  20004-1111

	ADC		Air Diffusion Council
	111 E. Wacker Dr., Suite 200
	Chicago IL  60601

	ADC 1062 R4-77		Certification, Rating and Test Manual

	AGA		American Gas Association
	8501 East Pleasant Valley Road
	Cleveland, OH  44131

	AGA Z 21.10.1-93		Gas Water Heaters Volume I Storage Water Heaters with Input Ratings of 75,000 Btu per hour or less
	AGA Z 21.10.3-93		Gas Water Heaters Volume III Storage, with Input Ratings Above 75,000 Btu per hour, Circulating and Insatantaneous Water Heaters
		AGA Z 21.12-90		Draft Hoods
				AGA Z 83.6A-90		Gas-Fired Infrared Heaters

	AI		Asphalt Institute
	PO Box 14052
	Lexington KY  40512-4052

	AI MS-2-93			Mix Design Methods for Asphalt Concrete and other Hot-Mix Types

	AIA		The American Institute of Architects
	1735 New York Ave., NW
	Washington, DC  20006

	AIHA	American Industrial Hygiene Association
	2700 Prosperity Ave., Suite 250
	Fairfax, VA  22031

	AISC	American Institute of Steel Construction
				1 E Wacker Dr., Suite 3100
				Chicago, IL  60601

	AISC M 016-89			Manual of Steel Construction Allowable Stress Design
	AISC M 017-92			Manual of Steel Construction, Vol.II-Connections
	AISC S 302-86			Code of Standard Practice for Steel Buildings and Bridges

	AISI	American Iron and Steel Institute
	1101 17th St.NW, Suite 1300
				Washington, DC  20036

	AISI SG 503-76		Design & Fabricating of Cold-Formed Steel Structurals
	AISI SG 673-86		Cold formed Steel Design Manual

	AITC	American Institute of Timber Construction
				11818 S.E. Mill Plain Blvd., Suite 407
	Vancouver, WA  98684
	AITC GLTI			Glued Laminated Timbers for Industrial, Commercial, and Institutional Buildings
	AITC PWR				Panelized Wood Roof System for Construction and Industrial Building Standard for 2 inches Nominal Thickness Lumber Roof Decking for Structural
	AITC TMC				Timber Construction Manual
AITC 109-90			Treating Standard for Structural Glued Laminated Timber
	AITC 110-84			Standard Appearance Grades for Structural Glued Laminated Timber
	AITC 111-79			Recommended Practice for Protection of Structural Glued Laminated Timber During Transit, Storage, and Erection
	AITC 200-92			Inspection Manual

	ALSC	American Lumber Standards Committee
	PO Box 210
	Germantown, MD  20875

	AMCA	Air Movement and Control Association
				30 West University Drive
				Arlington Heights, IL  60004

	AMCA 210-85			Laboratory Methods of Testing Fans for Rating
	AMCA 300-85			Reverberant Rom Method for Sound Testing of Fans (R1987)
	AMCA 301-90			Methods of Calculating Fan Sound Ratings from Laboratory Test Data
	AMCA 500-89			Test Methods for Louvers, Dampers, and Shutters

	ANSI	American National Standards Institute
				11 W 42nd St.
				New York, NY  10036

	ANSI A 17.1-93		Safety Code for Elevators and Escalators
	ANSI A 39.1-95		Safety Requirements for Window Cleaning
	ANSI A 108.1-92		Installation of Ceramic Tile a Collection
	ANSI A 112.19.1M-87	Enameled Cast Iron Plumbing Fixtures
	ANSI A 112.19.2M-90	Vitreous China Plumbing Fixtures
	ANSI A 112.19.3M-87	Stainless Steel Plumbing Fixtures (Designed for Residential Use)
	ANSI A 112.19.4M-94	Porcelain Enameled Formed Steel Plumbing Fixtures
	ANSI A 112.19.5-79		Trim for Water-Closet Bowls, Tanks, and Urinals (Dimensional Standards) (R1990)
	ANSI A 112.21.1M-91	Floor Drains
	ANSI A 112.21 2M-83	Roof Drains
	ANSI A 115.1-90		Preparation of Mortise Locks in 1-3/8 Inch and  1-3/4 Inch Standard Steel Doors and Frames
	ANSI A 118.9-90		Test Methods and Specifications for Cementitious Backer Units
	ANSI A 135.4-95		Basic Hardboard
	ANSI A 156.1-88		Butts and Hinges
	ANSI A 156.2-89		Bored and Preassembled Locks & Hatches
	ANSI A 156.3-94		Exit Devices
	ANSI A 156.4-92		Door Controls
	ANSI A 156.5-92		Auxiliary Locks & Associated Products
	ANSI A 156.6-94		Architectural Door Trim
	ANSI A 156.7-88		Template Hinge Dimensions
	ANSI A 156.8-94		Door Controls-Overhead Stops and Holders
	ANSI A 156.14-91		Sliding & Folding Door Hardware
	ANSI A 156.16-89		Auxiliary Hardware
	ANSI A 156.18-93		Materials and Finishes
	ANSI A 156.21-89		Thresholds
	ANSI B 1.20.1-83		Pipe Threads, General Purpose (Inch)
	ANSI B 16.1-89		Cast Iron Pipe Flanges and Flanged Fittings
	ANSI B 16.3-92		Malleable Iron Threaded Fittings
	ANSI B 16.11-91		Forged Fittings, socket Welding and Threaded
	ANSI B 16.12-91		Cast Iron Threaded Drainage Fittings
	ANSI B 16.15-85		Cast Bronze Threaded Fittings
	ANSI B 16.18-84		Cast Copper Alloy Solder Joint Pressure Fittings
	ANSI B 16.22-89		Wrought Copper and Copper alloy Solder Joint Pressure Fittings
	ANSI B 16.23-92		Cast Copper Alloy Solder Joint Drainage Fittings
	ANSI B 16.24-91		Cast Copper Alloy Pipe Flanges and Flanged Fittings
	ANSI B 16.25-92		Buttwelding Ends
	ANSI B 16.26-88		Cast Copper Alloy Fittings for Flared Copper Tubes
	ANSI B 16.29-94		Wrought Copper and Wrought Alloy Solder Joint Drainage Fittings
	ANSI B 16.39-86		Malleable Iron Threaded Pipe Unions (R1994)
	ANSI B 16.5-88		Pipe Flanges and Flanged Fittings
	ANSI B 16.9-93		Factory-Made Wrought Steel Buttwelding Fittings
	ANSI B 18.6.1-81		Wood Screws (Inch Series) (R1991)
	ANSI B 31.1-95		Power Piping
	ANSI B 31.3-93		Chemical Plant and Petroleum Refinery Piping
	ANSI B 31.4-92		Liquid Transportation Systems for Hydrocarbons, Liquid Petroleum Gas, Anhydrous Ammonia and Alcohols
	ANSI B 31.5-92		Refrigeration Piping
	ANSI B 36.10M-85		Welded and Seamless Wrought Steel Pipe (R1995)
	ANSI B 40.1-91		Gauges-Pressure Indicating Dial Type-Elastic Element
	ANSI B 153.1-90		Automotive Lifts-safety Requirements for Construction, Care and Use
	ANSI C 2-93			National Electrical Safety Code
	ANSI C 57.12.00-93		General Requirements for Liquid-Immersed Distribution, Power, and Regulating Transformers
	ANSI C 57.12.20-88		Transformers-Overhead Type Distribution Transformers 500 kVA & smaller
	ANSI C 57.12.25-90		Transformers-Pad mounted, Compartmental-Type, Self-Cooled, Single-Phase Distribution Transformers with Separable Insulated High-Voltage Connectors
	ANSI C 57.12.50-81		Ventilated Dry-Type Distribution Transformers (R1989)
	ANSI C 62.2-87		Application of Gapped Silicon-Carbide Surge Arresters for AC Systems (R1994)
	ANSI C 62.32-81		Low-Voltage Air Gap Surge-Protective Devices (R1994)
	ANSI C 62.61-85		Gas Tube  Surge Arresters on Wire Line Telephone Circuits
	ANSI O 5.1-92			Wood Poles - Specifications and Dimensions
	ANSI O 5.3-95			Wood Products-Solid Sawn-Wood Crossarms and Braces
	ANSI Y 32.9-72		Graphic Symbols for Electrical Wiring and Layout Diagrams Used in Architecture and Building Construction (1989)
	ANSI Z 60.1-90		Nursery Stock
	ANSI Z 88.2-92		Respiratory Protection
	ANSI Z 97.1-84		Safety Glazing Materials Used in Buildings (R1994)
	ANSI Z 124.1-87		Plastic Bathtub Units
	ANSI Z 124.2-87		Plastic Shower Receptors & Shower Stalls
	ANSI Z 133.1-94		Tree Care Operations
	ANSI Z 358.1-90		Emergency Eyewash and Shower Equipment

	AOAC	Association of Official and Analytical Chemists
	2200 Wilson Blvd., Suite 400
	Arlington, VA  22201-3301

	AOAC-90				Official Methods of Analysis of the AOAC 15th Edition

	APA		American Plywood Association
			P.O. Box 11700
				Tacoma, WA  98411

	APA B 840			303 Siding Manufacturing Specifications
	APA E 30				Residential and Commercial
	APA E 445			Performance Standards & Policies for Structural-USE Panels
	APA RR 135-C			Test Methods and Performance Requirements for Floor and Roof Sheathing
	APA TN M335			Finishing Plywood 303 Siding for Protection and Appearance
	APA V 345			Concrete Forming

	API		American Petroleum Institute
				1220 L Street, N.W.
				Washington, DC  20005

	API RP 5A5-93			Recommended Practice for Field Inspection of New Casing, Tubing, and Plain-End Drill Pipe 
	API STD 650-93		Welded Steel Tanks for Oil Storage (R1994)

	ARI		Air Conditioning and Refrigeration Institute
				1501 Wilson Boulevard, Suite 600
				Arlington, VA  22209-2403

	ARI 210/240-89		Unitary Air-Conditioning and Air-Source Heat Pump Equipment
	ARI 270-84			Sound Rating of Outdoor Unitary Equipment
	ARI 310-90			Packaged Terminal Air-Conditioners
	ARI 320-93			Water-Source Heat Pumps
	ARI 380-90			Packaged Terminal Heat Pumps
	ARI 410-91			Forced-Circulation Air-Cooling and Air-Heating Coils
	ARI 430-89			Central-Station Air- Handling Units
	ARI 590-92			Positive Displacement Compressor
	ARI 610-89			Central System Humidifiers for Residential Applications
	ARI 670-90			Fans and Blowers
		ARI 880-89			Air Terminals
	ARI 1010-84			Drinking-Fountains and Self-Contained, Mechanically-Refrigerated Drinking Water Coolers

	ARMA	Asphalt Roofing Manufacturers' Association
			6288 Montrose Road
				Rockville, MD  20852

	ASA		Acoustical Society of America
				500 Sunnyside Blvd.
				Woodbury NY  11797

	ASC		Adhesive and Sealant Council
	1600 North Wilson Blvd., Suite 910
	Arlington, VA  22209

	ASHC	American Society of Hardware Consultants
				7711 Old Springhouse Road
				McLean, VA  22102‑3474

	ASHRAE	American Society of Heating, Refrigerating and Air Conditioning Engineers
				1791 Tullie Circle, N.E.
				Atlanta, GA  30329

	ASHRAE 15-94			Safety Code for Mechanical Refrigeration
	ASHRAE 30-95			Methods of Testing Liquid Chilling Packages
	ASHRAE 37-88			Methods of Testing Rating Unitary Air-Conditioning and Heat Pump Equipment
	ASHRAE 51-85			Laboratory Methods of Testing Fans for Rating
	ASHRAE 52.1-92		Gravimetric and Dust-Spot Procedures for Testing Air-Cleaning Devices Used in General Ventilation for removing Particulate Matter
	ASHRAE 79-84			Methods of Testing for Rating Room Fan-Coil Air Conditioners (R1991)
	ASHRAE 90A-80			Energy Conservation in New Building Design
	ASHRAE 1989			Handbook of Fundamentals, 1991 Additions and Corrections

	ASME	American Society of Mechanical Engineers
	345 East 47th Street
	New York, NY  10017

	ASME A 112.1.2-91		Air Gaps in Plumbing Systems
	ASME A 112.18.1M-94	Plumbing Fixture Fittings
	ASME A 112.21.1M-91	Floor Drains
	ASME B 1.20.1-83		Pipe Threads, General Purpose (Inch) (R1992)
	ASME B 1.20.7-91		Hose Coupling Screw Threads (Inch)
	ASME B 16.5-88		Pipe Flanges and Flanged Fittings
	ASME B 16.9-93		Factory-Made Wrought Steel Buttwelding Fittings
	ASME B 16.21-92		Nonmetallic Flat Gaskets for Pipe Flanges
	ASME B 16.22-89		Wrought Copper and Copper Alloy Solder Joint Pressure Fittings
	ASME B 16.24-91		Cast Copper Alloy Pipe Flanges & Flanged Fittings
	ASME B 16.30-92		Malleable Iron Threaded Fittings
	ASME B 16.5-88		Pipe Flanges and Flanged Fittings
	ASME B 16.9-93		Factory Made Wrought Steel Buttwelding Fittings
	ASME B 16.39-86		Malleable Iron Threaded Pipe Unions (R1994)
	ASME B 18.2.1-81		Square and Hex Bolts and Screws Inch Series (R1992)
	ASME CSD-1-95			Controls and Safety Devices for Automatically Fired Boilers
	ASME PTC 25.3-88		Safety and Relief Valves
	ASME SEC VIII Division 1-95	Rules for Construction of Pressure Vessels
	ASME SEC IX-95		Qualifications Standard for Welding and Brazing Procedures

	ASND	American Society for Nondestructive Testing, Inc.
	11711 Arlingate Ln.
	Columbus, OH  43228

	ASPA	American Sod Producers Association
		1855A Hicks Road
	Rolling Meadows, IL  60008

	ASSE	American Society of Sanitary Engineering
	P.O. Box 40362
	Bay Village, OH  44140

	ASSE 1011-93			Performance Requirements for Hose Connection Vacuum Breakers
	ASSE 1013-93			Performance Requirements for Reduced Pressure Principle backflow Preventers
	ASSE 1015-93			Performance Requirements for Double Check Backflow Preventers
	ASSE 1020-89			Performance Requirements for Pressure Vacuum Breaker Assembly (Recommended for Outdoor Usage)
	ASSE 1047-93			Performance Requirements for Reduced Pressure Detector Backflow Preventer
	ASSE 1048-93			Performance Requirements for Double Check Detector Assembly Backflow Preventer

	ASTM	American Society for Testing and Materials
  			100 Barr Harbor Dr.
				West Conshohocken PA  19428-2959

	ASTM A 6/6M REV C-95	Rolled Structural Steel Bars, Plates, Shapes, and Sheet Piling
	ASTM A 36/A 36M-94		Carbon Structural Steel
	ASTM A 307-90			Carbon Steel Bolts and Studs, 60 000 PSI Tensile Strength
	ASTM A 47M-90			Ferritic Malleable Iron Castings (Metric)
	ASTM A 47-90			Ferritic Malleable Iron Castings
	ASTM A 48M-94			Gray Iron Castings
	ASTM A 48 REV A-94		Gray Iron Castings
	ASTM A 53 REV A-95		Pipe, Steel, Black and Hot-Dipped, Zinc-Coated, Welded and Seamless
	ASTM A 74-94			Cast Iron Soil Pipe and Fitting
	ASTM A 82-95			Steel Wire, Plain, for Concrete Reinforcement
	ASTM A 90/A 90M-95		Test Method for Weight of Coating on Iron and Steel Articles with Zinc or Zinc-Alloy Coatings
	ASTM A 106 REV A-94	Seamless Carbon Steel Pipe for High-Temperature Service
	ASTM A 116-88			Zinc-Coated (Galvanized) Steel Woven Wire Fence Fabric
	ASTM A 121 REV A-92	Zinc-Coated (Galvanized) Steel Barbed Wire
	ASTM A 123 REV A-89	Zinc (Hot-Dip Galvanized) Coatings on Iron and Steel Products
	ASTM A 126-93			Gray Iron Castings for Valves, flanges, and Pipe fittings
	ASTM A 135-93			Electric-Resistance-Welded Steel Pipe
	ASTM A 153/A 153M-95	Zinc coating (Hot-Dip) on Iron and Steel Hardware
	ASTM A 167 REV A-94	Stainless and Heat-Resisting Chromium Nickel Steel Plate, Sheet, and Strip
	ASTM A 181/A 181M-95	Carbon Steel Forgings for General Purpose Piping
	ASTM A 183-83 (R90)	Carbon Steel Track Bolts and Nuts
	ASTM A 185-94			Steel Welded Wire Fabric, Plain, for Concrete Reinforcement
	ASTM A 197-87			Cupola Malleable Iron
	ASTM A 227/A 227M-93	Steel Wire, Cold-Drawn for Mechanical Springs
	ASTM A 229/A 229M-93	Steel Wire, Oil-Tempered for Mechanical Springs
	ASTM A 234/A 234M-95	Piping Fittings of Wrought Carbon Steel and Alloy Steel for Moderate and Elevated Temperatures
	ASTM A 242/A 242M-93	High-Strength Low-Alloy Structural Steel
	ASTM A 307-94			Carbon Steel Bolts and Studs, 60,000 psi Tensile Strength
	ASTM A 325M-93		Structural Bolts, Steel, Heat Treated, 120/105 ksi Minimum Tensile Strength (Metric)
	ASTM A 325-94			Structural Bolts, Steel. Heat treated 120/105 ksi Minimum Tensile Strength High-Strength
	ASTM A 328/A 328M REV A-93		Steel Sheet Piling
	ASTM A 361/361M-94		Steel Sheet, Zinc-Coated (Galvanized) by the Hot Dip Process for Roofing and Siding
	ASTM A 377-95			Standard Index of Specifications for Ductile-Iron Pressure Pipe
	ASTM A 390-95			Zinc-Coated (Galvanized) Steel Poultry Fence Fabric (Hexagonal and Straight Line)
	ASTM A 392 REV B-91	Zinc-Coated Steel Chain Link Fence Fabric
	ASTM A 416/A 416M REV A-94		Steel Strand, Uncoated Seven-Wire for Prestressed Concrete (E1-1995)
	ASTM A 428-89			Test Method for Weight of Coating on Aluminum-Coated Iron or Steel Articles
	ASTM A 446/446 M-93	Steel Sheet, Zinc-Coated (galvanized) by the Hot Dip Process
	ASTM A 478-REV A-95	Chromium Nickel Stainless Steel Weaving and Knitting Wire
	ASTM A 490-93			Heat-Treated Steel Structural Bolts 
	ASTM A 499-89			Steel Bars and Shapes, Carbon Rolled From "T" Rails
	ASTM A 500-93			Cold-Formed Welded and Seamless Carbon Steel Structural Tubing in Rounds and Shapes
	ASTM A 501-93			Hot-Formed Welded and Seamless Carbon Steel Structural Tubing
	ASTM A 506-93			Steel, Sheet and Strip, Alloy, Hot-Rolled and Cold-Rolled
	ASTM A 525M REV A-91	Sheet Steel, Zinc-Coated (Galvanized) by Hot-Dip Process
	ASTM A 525-93			Sheet Steel, Zinc-Coated (Galvanized) by the Hot-Dip Process
	ASTM A 526/A 526 M-90	Steel Sheet, Zinc-Coated (Galvanized) by Hot-Dip Process, Commercial Quality
	ASTM A 527/A 527M-90	Steel Sheet, Zinc-Coated (Galvanized) by Hot-Dip Process, Lock-Forming Quality
	ASTM A529/A529 M-94	High-Strength Carbon-Manganese Steel of Structural Quality
	ASTM A 536-84			Ductile Iron Castings
	ASTM A 563M-93		Carbon and Alloy Steel Nuts (Metric)
	ASTM A 563-94			Carbon and Alloy Steel Nuts
	ASTM A 569/569M REV A-91	Steel, Carbon, (0.15 Maximum, Percent) Hot-Rolled Sheet and Strip Commercial Quality (R1993)
	ASTM A 570/570 M-95	Steel, Sheet and Strip, Carbon, Hot-Rolled Structural Quality
	ASTM A 572/A 572M REV C-94	High-Strength Low-Alloy Columbium-Vanadium Structural Steels
	ASTM A 575-89			Steel Bars, Carbon, Merchant Quality, M Grades
	ASTM A 584-92			Aluminum-Coated Steel Woven Wire Fence Fabric
	ASTM A 585-92			Aluminum Coated Steel Barbed Wire
	ASTM A 588/A 588M-94	High-Strength Low-Alloy Structural Steel with 50 ksi (345 MPa) Minimum Yield
	ASTM A 589-95			Seamless and Welded Carbon Steel Water-Well Pipe
	ASTM A 591/A591M-89	Steel Sheet, Electrolytic zinc-coated, for Light Coating Mass Applications (R1994)
	ASTM A 607 REV A-92	Steel, Sheet and Strip, High-Strength, Low-Alloy Columbium or Vanadium
	ASTM A 615/A 615M REV B-95	Deformed and Plain Billet Steel Bars for Concrete Reinforcement
	ASTM A 641M-91		Zinc-Coated (Galvanized) Carbon Steel Wire (Metric)
	ASTM A 641-92			Zinc-Coated (Galvanized) Carbon Steel Wire
	ASTM A 645/645M-87		Pressure Vessel Plates, Five Percent Nickel Alloy Steel, Specially Heat Treated (R1991)
	ASTM A 659/A659 M-92	Steel, Carbon Hot-Rolled Sheet and Strip, Commercial Quality (R1993)
	ASTM A 666 REV A-94	Austenitic Stainless Steel Sheet, Strip, Plate and Flat Bar
	ASTM A 674-95			Polyethylene Encasement for Ductile Iron Pipe for Water or Other Liquids
	ASTM A 690/A 690M-94	High-Strength Low-Alloy Steel H-Piles and Sheet Piling for Use in Marine Environments
	ASTM A 702-89			Steel Fence Posts and Assemblies,  Hot Wrought (R1994)
	ASTM A 733-93			Welded and Seamless Carbon Steel and Austenitic Stainless Steel Pipe Nipples
	ASTM A 775/A 775M REV D-94		Epoxy Coated Reinforcing Steel bars (E1-1995)
	ASTM A 786/A 786M-93	Rolled Steel Floor Plates
	ASTM A 809-91			Aluminum-Coated Carbon Steel Wire
	ASTM A 817-94			Metallic-Coated Steel wire for Chain Link Fence Fabric
	ASTM A 824-92			Metallic-Coated Steel Carcelled Tension Wire for Use with Chain Link Fence
	ASTM A 854/A 854M-94	Metallic-Coated Steel Smooth High-Tensile Fence and Trellis Wire
	ASTM A 875/A 875M-95	Steel Sheet, Zinc-5% Aluminum Alloy-Coated by Hot-Dip Process
	ASTM A 888-95			Hubless Cast Iron Soil Pipe and Fittings
				ASTM B 32 REV B-95		Solder Material
				ASTM B 61-93			Steam or Valve Bronze Castings
	ASTM B 62-93			Composition Bronze or Ounce Metal Castings
				ASTM B 75-95			Seamless Copper Tube
	ASTM B 85-95			Aluminum-Alloy Die Castings
	ASTM B 88M-89			Seamless Copper Water tube (Metric)
	ASTM B 88 REV A-95		Seamless Copper Water Tube
	ASTM B 111M-93		Copper and Copper and Copper-Alloy Seamless Condenser Tubes and Ferrule Stock (Metric)
	ASTM B 111-95			Copper and Copper-Alloy Seamless Condenser Tubes and Ferrule Stock
	ASTM B 117-95			Operating Salt Spray (Fog) Apparatus
	ASTM B  137-95		Test Method for Measurement of coating per Unit Area on Anodically Coated Aluminum
	ASTM B 209-95			Aluminum and Aluminum-Alloy Sheet and Plate
	ASTM B 211M-95		Aluminum and Aluminum-Alloy Bar, Rod, and wire (Metric)
	ASTM B 211 REV A-95	Aluminum and Aluminum-Alloy Bar, Rod, and Wire
	ASTM B 221M REV A-95	Aluminum and Aluminum-Alloy Extruded Bars, Rods, Wire, Shapes, and Tubes (Metric)
	ASTM B 221-95			Aluminum and Aluminum-Alloy Extruded Bars, Rods, Wire, Shapes, and Tubes
	ASTM B 280-95			Seamless Copper Tube for Air Conditioning and Refrigeration Field Services
	ASTM B 306-95			Copper Drainage Tube (DWV)
	ASTM B 370-92			Copper Sheet and Strip for Building Construction
	ASTM B 395M-95		U-Bend Seamless Copper and Copper-Alloy Heat Exchanger and Condenser Tubes (Metric)
	ASTM B 395-95			U-Bend Seamless Copper and copper-Alloy Heat Exchanger and Condenser Tubes
	ASTM B 429-95			Aluminum Alloy Extruded Structural Pipe and Tube
	ASTM B 543M-91		Welded Copper and Copper-Alloy Heat Exchanger Tube (Metric)
	ASTM B 543-91			Welded Copper and Copper-Alloy Heat Exchanger Tube
	ASTM B 584 REV B-93	Copper Alloy Sand Castings for General Applications
	ASTM B 633-85			Electrodeposited Coatings of Zinc on Iron and Steel (R1994)
	ASTM B 687-93			High Strength Non-headed Steel Bolts and Studs
	ASTM B 699-86			Coatings of Cadmium Vacuum Deposited on Iron and Steel (R1993)
	ASTM C 11-95			Terminology Relating to Gypsum and Related Building Materials and Systems
	ASTM C 12-95			Installing Vitrified Clay Pipe Lines
	ASTM C 14M-95			Concrete Sewer, Storm Drain, and Culvert Pipe (Metric)
	ASTM C 14-95			Concrete Sewer, Storm Drain, and Culvert Pipe
	ASTM C 28-92			Gypsum Plasters
	ASTM C 29/C 29M REV A-91	Test Method for Unit Weight and Voids in Aggregate
	ASTM C 31-91			Making and Curing Concrete Test Specimens in the Field
	ASTM C 33-93			Concrete Aggregate
	ASTM C 35-95			Inorganic Aggregates for Use in Gypsum Plaster
	ASTM C 36 REV A-95		Gypsum Wallboard
	ASTM C 37-92			Gypsum Lath
	ASTM C 39-94			Test Method for Compressive Strength of Cylindrical Concrete Specimens
	ASTM C 42-94			Test Method for Obtaining and Testing Drilled Cores and Sawed Beams of Concrete
	ASTM C 59-91			Gypsum Casting and Molding Plaster
	ASTM C 61-95			Gypsum Keene's Cement
	ASTM C 76-89			Reinforced Concrete Culvert,  Storm Drain, and Sewer Pipe
	ASTM C 88-90			Test Method for Soundness of Aggregate by use of Sodium Sulfate or Magnesium Sulfate
	ASTM C 90-95			Loadbearing Concrete Masonry Units
	ASTM C 91-REV B-95		Masonry Cement
	ASTM C 94-94			Ready-Mixed Concrete
	ASTM C 97-90			Test Method for Absorption and Bulk Specific Gravity of Dimension Stone (R1994)
	ASTM C 99-87			Test Method for Modulus of Rupture of Dimension Stone (R1993)
	ASTM C 109/C 109M-95	Test Method for Compressive Strength of Hydraulic Cement Mortars
	ASTM C 117-95			Test Method for Materials Finer Than 75-Micrometers (No. 200) Sieve in Mineral Aggregate
	ASTM C 119 REV A-95	Standard Terminology Relating to Dimension Stone
	ASTM C 127-88			Test Method for Specific Gravity and Absorption of Coarse Aggregate (R1993)
	ASTM C 128-93			Test Method for Specific Gravity and Absorption of Fine Aggregate
	ASTM C 129-95			Nonloadbearing Concrete Masonry Units
	ASTM C 131-89			Test Method for Resistance to Degradation of Small-Size Coarse Aggregates by Abrasion & Impact in the LA Machine
	ASTM C 136 REV A-95	Test Method for Sieve Analysis of Fine and Coarse Aggregates
	ASTM C 140 REV A-95	Test Methods of Sampling and Testing Concrete Masonry Units
	ASTM C 143 REV A-90	Test Methods for Slump of Hydraulic Cement Concrete
	ASTM C 144-93			Aggregate for Masonry Mortar
	ASTM C 150-95			Portland Cement
	ASTM C 165-95			Test Method for Measuring Compressive Properties of Thermal Insulations
	ASTM C 167-93			Test Methods for Thickness and Density of Blanket or Batt Thermal Insulations
	ASTM C 168-90			Standard Terminology Relating to Thermal Insulating Materials
	ASTM C 170-90			Test Method for Compressive Strength of Dimension Stone (R1994)
	ASTM C 171-95			Sheet Materials for Curing Concrete
	ASTM C 172-90			Sampling Freshly Mixed Concrete
	ASTM C 177-85			Test Method for Steady State Heat Flux Measurements and Thermal Transmission Properties by 
	ASTM C 183 REV A-95	Sampling and the Acceptance of Hydraulic Cement
	ASTM C 188-85			Test Method for Density of Hydraulic Cement
	ASTM C 195-95			Mineral Fiber Thermal Insulating Cement
	ASTM C 196-93			Expanded or Exfoliated Vermiculite Thermal Insulating Cement
	ASTM C 203-92			Test Method for Breaking Load and Flexural Properties of Block-Type Thermal Insulation
	ASTM C 206-84			Finishing Hydrated Lime (R1992)
	ASTM C 207-91			Hydrated Lime for Masonry Purposes (R1992)
	ASTM C 209-92			Test Methods for Cellulosic Fiber Insulating Board
	ASTM C 216 REV A-95	Facing Brick (Solid Masonry Units Made from Clay or Shale)
	ASTM C 231 REV B-91	Test Method for Air Content of Freshly Mixed Concrete by the Pressure Method
	ASTM C 240-91			Test Methods of Testing Cellular glass Insulation Block
	ASTM C 260-95			Air-Entraining Admixtures for  Concrete
	ASTM C 270 REV A-95	Mortar for Unit Masonry
	ASTM C 272-91			Test Method for Water Absorption of Core Materials for Structural Sandwich Constructions
	ASTM C 303-90			Test Method for Density of Performed Block-Type Thermal Insulation
	ASTM C 309-95			Liquid Membrane-Forming Compounds for Curing  Concrete
	ASTM C 311 REV B-94	Test Methods for Sampling and Testing Fly Ash or Natural Pozzolans for Use as a Mineral Admixture in Portland Cement Concrete
	ASTM C 330-89			Lightweight Aggregates for Structural Concrete
	ASTM C 387-87			Packaged, Dry, combined Materials for Mortar and Concrete (R1995)
	ASTM C 404-95			Aggregates for Masonry Grout
	ASTM C 423 REV A-90	Test Method for Sound Absorption and Sound Absorption Coefficients by the Reverberation Method
	ASTM C 425-95			Compression Joints for Vitrified Clay Pipe and Fittings
	ASTM C 443-94			Joints for Circular Concrete Sewer and Culvert Pipe Using Rubber Gaskets
	ASTM C 449/C 449M-95	Mineral Fiber Hydraulic-Setting Thermal Insulating and Finishing Cement
	ASTM C 472-93			Test Method for Physical Testing of Gypsum, Gypsum Plasters and Gypsum Concrete
	ASTM C 475-94			Joint Compound and Joint Tape for Finishing Gypsum Board
	ASTM C 476-95			Grout for Masonry
	ASTM C 478/478M REV A-95	Precast Reinforced Concrete Manhole Sections
	ASTM C 494-92			Chemical Admixtures for Concrete
	ASTM C 518-91			Test Method for Steady State Heat Flux Measurements and Thermal Transmission
	ASTM C 533-95			Calcium Silicate Block and Pipe Thermal Insulation
	ASTM C 534-94			Preformed Flexible Elastomeric Cellular Thermal Insulation in Sheet and Tubular Form
	ASTM C 547-95			Mineral Fiber-Preformed Pipe Insulation
	ASTM C 552-91			Cellular Glass Thermal Insulation
	ASTM C 553-92			Mineral Fiber Blanket Thermal Insulation
	ASTM C 557 REV A-93	Adhesive for Fastening Gypsum Wallboard to Wood Framing
	ASTM C 564 REV A-95	Rubber Gaskets for Cast Iron Soil Pipe and Fitting
	ASTM C 578-95			Rigid, Cellular Polystyrene Thermal Insulation
	ASTM C 579-91			Test Method for Compressive Strength of Chemical Resistant Mortars, Grouts, Monolithic Surfacings and Polymer Concretes
	ASTM C 580-93			Test Method for Flexural Strength and Modulus of Elasticity of Chemical-Resistant Mortars, Grouts, Monolithic Surfacings and Polymer Concrete
	ASTM C 595 REV A-94	Blended Hydraulic Cements 
	ASTM C 595M REV A-95	Blended Hydraulic Cements (Metric)
	ASTM C 602 REV A-95	Agricultural Liming Materials
	ASTM C 603-90			Test Method for Extrusion Rate and Application Life of Elastomeric Sealants
	ASTM C 612-93			Mineral Fiber Block and Board Thermal Insulation
	ASTM C 618-95			Fly Ash and Raw or Calcined Natural Pozzolan for Use as a Mineral Admixture in Portland Cement Concrete
	ASTM C 630-95			Water-Resistant Gypsum Backing Board

ASTM C 635-95			Manufacture, Performance and Testing of Metal Suspension Systems for Acoustical Tile and Lay-In Panels
	ASTM C 639-95			Test Method for Rheological (Flow) Properties of Elastomeric Sealants
	ASTM C 645 REV A-95	Nonload Bearing (Axial) Steel Studs, Runners (track), and Rigid Furring Channels for Screw Application of Gypsum Board
	ASTM C 647-95			Properties and Tests of Mastice and Coating Finishes for Thermal Insulation
	ASTM C 653-92			Determination of the Thermal Resistance of Low-Density Blanket-Type Mineral Fiber Insulation
	ASTM C 661-93			Test Method for Indentation Hardness of Elastomeric-Type Sealants by Means of a Durometer
	ASTM C 665-94			Mineral-Fiber Blanket Thermal Insulation for Light Frame Construction and Manufactured Housing
	ASTM C 666-92			Test Method for Resistance of Concrete to Rapid Freezing and Thawing
	ASTM C 679-87			Test Method for Tack-Free Time of Elastomeric Sealants (R1992)
	ASTM C 700-95			Vitrified Clay Pipe, Extra Strength, Standard Strength, and Perforated
	ASTM C 719-93			Test Method for Adhesion and Cohesion of Elastomeric Joint Sealants Under Cyclic Movement
	ASTM C 728-91			Perlite Thermal Insulation Board
	ASTM C 744 REV A-95	Prefaced Concrete and Calcium Silicate Masonry Units
	ASTM C 790-90			Standard Guide for Use of Latex Sealants
	ASTM C 792-93			Test Method for Effects of Heat Aging on Weight Loss, Cracking, and Chalking of Elastomeric Sealants
	ASTM C 794-93			Test Method for Adhesion-in-Peel of Elastomeric Joint Sealants
	ASTM C 834-95			Latex Sealants
	ASTM C 916-85			Adhesives for Duct Thermal Insulation (R1990)
	ASTM C 920-s95		Elastomeric Joint Sealants
	ASTM C 1002-93		Steel Drill Screws for the Application of Gypsum board or Metal Plaster Bases
	ASTM C 1071-91		Thermal and Acoustical Insulation  (Glass Fiber, Duct Lining Material)
	ASTM C 1136-95		Flexible, Low Permeance Vapor Retarders for Thermal Insulation
	ASTM D 4-86			Test Method for Bitumen Content (R1993)
	ASTM D 5-94			Test Method for Penetration of Bituminous Materials
	ASTM D 6-95			Test Method for Loss on Heating of Oil and Asphaltic Compound
	ASTM D 25-91			Round Timber Piles
	ASTM D 36-95			Test Method for Softening Point of Bitumen (Ring-and-Ball Apparatus)
	ASTM D 41-94			Asphalt Primer Used in Roofing, Dampproofing, and Waterproofing
	ASTM D 43-94			Coal Tar Primer Used in Roofing, Dampproofing and Waterproofing
	ASTM D 70-82			Test Method for Specific Gravity and Density of Semi-Solid Bituminous Materials (R1990)
	ASTM D 75-87			Sampling Aggregate
	ASTM D 92-90			Test Method for Flash and Fire Points by Cleveland Open Cup
	ASTM D 98-95			Calcium Chloride
	ASTM D 113-86			Test Method for Ductility of Bituminous Materials (1992)
	ASTM D 225-86			Asphalt Shingles (Organic Felt) Surfaced with Mineral Granules (R1994)
	ASTM D 226-94			Asphalt Saturated Organic Felt Used in Roofing and Waterproofing
	ASTM D 242-95			Mineral Filler for Bituminous Paving Mixture
	ASTM D 245-93			Establishing Structural grades and Related Allowable Properties for Visually Graded Lumber
	ASTM D 249-89			Asphalt Roll Roofing (Organic Felt) Surfaced with Mineral Granules
	ASTM D 297-93			Test Methods for Rubber Products-Chemical Analysis
	ASTM D 312-95			Asphalt Used in Roofing
	ASTM D 396-92			Fuel Oils
	ASTM D 412-92			Test Methods for Vulcanized Rubber and Thermoplastic Rubbers and Elastometers
	ASTM D 413-82			Test Methods for Rubber Property--Adhesion to Flexible Substrate (R1993)
	ASTM D 418-93			Test Methods for Testing Pile Yarn Floor Covering Construction
	ASTM D 449-89			Asphalt Used in Dampproofing and Waterproofing (R1994)
	ASTM D 450-91			Coal-Tar Pitch Used in Roofing, Dampproofing, and Waterproofing
	ASTM D 471-95			Test Method for Rubber Property-Effect of Liquids
	ASTM D 478-86			Zinc Yellow (Zinc Chromate) Pigments (R1991)
	ASTM D 518-86			Test Method for Rubber Deterioration - Surface Cracking (R1991)
	ASTM D 543-87			Test Method for Resistance of Plastics to Chemical Reagents
	ASTM D 546-94			Test Method for Sieve Analysis of Mineral Filler for Road and Paving Materials
	ASTM D 570-95			Test Method for Water Absorption of Plastics
	ASTM D 573-88			Test Method for Rubber-Deterioration in an Air Oven (R1994)
	ASTM D 624-91			Test Method for Tear Strength of Conventional Vulcanized Rubber and Thermoplastic Elastometers
	ASTM D 638 REV B-94	Test Method for Tensile Properties of Plastics
	ASTM D 692 REV A-94	Coarse Aggregate for Bituminous Paving Mixtures
	ASTM D 696-91			Test Method for Coefficient of Linear Thermal Expansion of Plastics
	ASTM D 746-79			Test Method for Brittleness Temperature of Plastics and Elastomers by Impact (R1987)
	ASTM D 747-93			Test Method for Apparent Bending Modulus of Plastics by Means of a Cantilever Beam
	ASTM D 751-95			Test Method for Coated Fabrics
	ASTM D 790-92			Test Method for Flexural Properties of Unreinforced and Reinforced Plastics and Electrical Insulating Materials
	ASTM D 792-91			Test Methods for Density and Specific Gravity (Relative Density) of Oplastics by Displacement
	ASTM D 854-92			Test Method for Specific Gravity of Soils
	ASTM D 882 REV A-95	Test Method for Tensile Properties of Thin Plastic Sheeting
	ASTM D 906 REV A-94	Test Method for Strength Properties of Adhesives in Plywood Type Construction in Shear by Tension Loading
	ASTM D 946-82			Penetration-Graded Asphalt Cement for Use in Pavement (R1993)
	ASTM D 977-91			Emulsified Asphalt
	ASTM D 979-89			Standard Practice for Sampling Bituminous Paving Mixtures
	ASTM D 994-94			Preformed Expansion Joint Filler for Concrete (Bituminous Type)
	ASTM D 995 REV B-95	Mixing Plants for Hot-Mixed, Hot-Laid Bituminous Paving Mixture
	ASTM D 1004 REV A-94	Test Method for Initial Tear Resistance of Plastic Film and Sheeting
	ASTM D 1037-95		Test Method for Evaluating Properties of wood-Base Fiber and Particle Panel Materials
	ASTM D 1038-83		Terminology Relating to Veneer and Plywood (R1993)
	ASTM D 1073-94		Fine Aggregate for Bituminous Paving Mixtures
	ASTM D 1075-94		Test Method for Effect of Water on Cohesion of Compacted Bituminous Mixtures
	ASTM D 1117-80		Methods of Testing Nonwoven Fabrics
	ASTM D 1143-81		Test Method for Piles Under Static Axial Compressive Load (R1994)
	ASTM D 1149-91		Test Method for Rubber Deterioration-Surface Ozone Cracking in a Chamber
	ASTM D 1188-89		Test Method for Bulk Specific Gravity and Density of Compacted Bituminous Mixtures
	ASTM D 1190-94		Concrete Joint Sealer, Hot Applied Elastic Type
	ASTM D 1203-94		Test Methods for Volatile Loss From Plastics Using Activated Carbon Methods
	ASTM D 1204-94		Test Method for Linear Dimensional Changes of Nonrigid thermoplastic Sheeting or Film
	ASTM D 1248-84		Polyethylene Plastics Molding and Extrusion Materials (R1989)
	ASTM D 1335-67		Method of Test for Tuft Bind of Pile Floor Coverings (R1972)
	ASTM D 1461-85		Test Method for Moisture or Volatile Distillates in Bituminous Paving Mixtures
	ASTM D 1494-92		Test Method for Diffuse Light transmission Factor of Reinforced Plastic Panels
	ASTM D 1559-89		Test Method for Resistance to Plastic Flow of Bituminous Mixture
	ASTM D 1593-92		Nonrigid Vinyl Chloride Plastic Sheeting
	ASTM D 1598-86		Test Method for Time-to-failure of Plastic Pipe Under Constant Internal Pressure (R1991)
	ASTM D 1599-88		Test Method for Short-Time Hydraulic Failure Pressure of Plastic Pipe, Tubing, and Fittings
	ASTM D 1621-94		Test Method for Compressive Properties of Rigid Cellular Plastics
	ASTM D 1622-93		Test Method for Apparent Density of Rigid Cellular Plastics
	ASTM D 1623-78		Test Method for Tensile Adhesion Properties of Rigid Cellular Plastics (R1995)
	ASTM D 1683 REV A-90	Test Method for Failure in Sewn Seams of Woven Fabrics
	ASTM D 1760 REV A-95	Pressure Treatment of Timber Products
	ASTM D 1761-88		Test Methods for Mechanical fasteners in Wood (R1995)
	ASTM D 1784-92		Rigid Poly (Vinyl Chloride) (PVC) Compounds and Chlorinated Poly (Vinyl Chloride) (CPVC) Compounds
	ASTM D 1785-94		Poly (Vinyl Chloride) (PVC) Plastic Pipe, Schedules 40, 80, and 120
	ASTM D 1790-94		Test Method for Brittleness Temperature of Plastic Sheeting by Impact (E1-1995)
	ASTM D 1863-93		Mineral Aggregate Used on Built-Up roofs
	ASTM D 1876-95		Test Method for Peel Resistance of Adhesives (T-Peel Test)
	ASTM D 1929 REV A-91	Test Method for Ignition Properties of Plastics
	ASTM D 2041-95		Test Method for Theoretical Maximum Specific Gravity and Density of Bituminous Paving Mixtures
	ASTM D 2092-95		Preparation of Zinc-Coated (Galvanized) Steel Surfaces for Painting
	ASTM D 2103-92		Polyethylene Film and Sheeting
	ASTM D 2104-93		Polyethylene (PE) Plastic Pipe, Schedule 40
	ASTM D 2126-94		Test Method for Response of Rigid Cellular Plastics to Thermal and Humid Aging
	ASTM D 2136-94		Test Method for Coated Fabrics--Low Temperature Bend Test
	ASTM D 2172-95		Test Methods for Quantitive Extraction of Bitumen from Bituminous Paving Mixtures
	ASTM D 2178-89		Asphalt Glass felt Used in Roofing and Waterproofing
	ASTM D 2200-95		Pictorial Surface Preparation Standards for Painting Steel Surfaces
	ASTM D 2235 REV A-93	Solvent Cement for Acrylonitrile-Butadiene-Styrene (ABS) Plastic Pipe aand Fittings
	ASTM D 2239-94		Polyethylene (PE) Plastic Pipe (SIDR-PR) Based on Controlled Inside Diameter
	ASTM D 2240-95		Test Method for Rubber Property - Durometer Hardness
	ASTM D 2241-94		Poly (Vinyl Chloride) (PVC) Pressure-Rated  Pipe (SDR Series)
	ASTM D 2244-93		Test Method for Calculation of Color Differences from Instrumentally Measured Color Coordinates
	ASTM D 2282-94		Acrylonitrile-Butadiene-Styrene (ABS) Plastic Pipe (SDR-PR)
	ASTM D 2488-93		Standard Practice for Description and Identification of Soils (Visual-Manual Method)
	ASTM D 2310-91		Machine-Made "Fiberglass" Pipe
	ASTM D 2321-89		Standard Practice for Underground Installation of Thermoplastic Pipe
	ASTM D 2464-94		Threaded Poly (Vinyl Chloride) (PVC) Plastic Pipe Fittings, Schedule 80
	ASTM D 2466 REV A-94	Poly (Vinyl Chloride) (PVC) Plastic Pipe Fittings, Schedule 40
	ASTM D 2467-94		Socket-Type Poly (Vinyl Chloride) (PVC) Plastic Pipe Fittings, Schedule 80
	ASTM D 2487-93		Classification Of soils for Engineering Purposes
	ASTM D 2513 REV A-95	Thermoplastic Gas Pressure Pipe, Tubing, and Fittings
	ASTM D 2517-94		Reinforced Epoxy Resin Gas Pressure Pipe and Fittings
	ASTM D 2564-93		Solvent cements for Poly (Vinyl Chloride) (PVC) Plastic Piping Systems
	ASTM D 2582-93		Test Method for Puncture Propogation Tear Resistance of Plastic Film and Thin Sheeting
	ASTM D 2583-93		Test Method for Indentation Hardness of Rigid Plastics by Means of a Barcol Impressor
	ASTM D 2609-93		Plastic Insert Fittings for Polyethylene (PE) Plastic Pipe
	ASTM D 2628-91		Preformed Polychloroprene Elastomeric Joint Seals for Concrete Pavements
	ASTM D 2661-95		Acrylonitrile-Butadiene-Styrene (ABS) Schedule 40 Plastic Drain, Waste, and Vent Pipe and Fittings
	ASTM D 2662-95		Polybutylene (PB) Plastic Pipe (SIDR PR) Based on Controlled Inside Diameter
	ASTM D 2665 REV A-94	Poly (Vinyl Chloride) (PVC) Plastic Drain, Waste and Vent Pipe and Fittings
	ASTM D 2666-95		Polybutylene (PB) Plastic Tubing
	ASTM D 2672-95		Joints for IPS PVC Pipe Using Solvent Cement
	ASTM D 2726-95		Test Method for Bulk Specific Gravity and Density of Compacted Bituminous Mixtures
	ASTM D 2729-93		Poly (Vinyl Chloride) (PVC) Sewer Pipe and Fittings
	ASTM D 2737-93		Polyethylene (PE) Plastic Tubing
	ASTM D 2751-93		Acrylonitrile-Butadiene-Styrene (ABS) Sewer Pipe and Fittings
	ASTM D 2774-94		Underground Installation of Thermoplastic Pressure Piping
	ASTM D 2794-93		Test Method for Resistance of Organic Coatings to the Effect of Rapid Reformation (Impact)
	ASTM D 2822-91		Asphalt Roof Cement
	ASTM D 2824-94		Aluminum Pigmented Asphalt Roof Coatings
	ASTM D 2842-94		Test Method for Water Absorption of rigid Cellular Plastics
	ASTM D 2846/D 2846M REV A-95	Chlorinated Poly (Vinyl Chloride) (CPVC) Plastic Hot-and Cold-Water Distribution Systems
	ASTM D 2852-93		Styrene Rubber Plastic Drain Pipe and Fittings
	ASTM D 2855-93		Making Solvent Cemented Joints with Poly (Vinyl Chloride) (PVC) Pipe and Fittings
	ASTM D 2859 REV A-93	Test Method for Flammability of Finished Textile Floor Covering Materials
	ASTM D 2950-91		Test Method for Density of Bituminous Concrete in Place by Nuclear Methods
	ASTM D 2974-87		Test Method for Moisture, Ash, and Organic Matter of Peat and Other Organic Soils (R1995)
	ASTM D 3018-90		Class A Asphalt Shingles Surfaced with Mineral Granules (R1994)
	ASTM D 3034-94		Type PSM Poly (Vinyl Chloride) (PVC) Sewer Pipe and Fittings
	ASTM D 3035-93		Polyethylene (PE) Plastic Pipe (DR-PR) Based on Controlled Outside Diameter
	ASTM D 3038-93		Test Method for Drop Shatter Test for Coke
	ASTM D 3139-95		Joints for Plastic Pressure Pipes Using Flexible Elastomeric Seals
	ASTM D 3161-95		Test Method for Wind-Resistance of Asphalt Shingles
	ASTM D 3299-88		Filament Wound Glass-Fiber-Reinforced Thermostat Resin Chemical Resistant Tanks
	ASTM D 3309-95		Polybutylene (PB) Plastic Hot and Cold Water Distribution Systems
	ASTM D 3350-93		Polyethylene Plastics Pipe and Fittings Materials
	ASTM D 3381-92		Viscosity-Graded Asphalt Cement for Use in Pavement Construction
	ASTM D 3462 REV A-93	Asphalt Shingles Made from Glass felt and Surfaced with Mineral Granules
	ASTM D 3786-87		Test Method for Hydraulic Bursting Strength of Knitted Goods and Nonwoven Fabrics
	ASTM D 3884-92		Test Method for Abrasion Resistance of Textile Fabrics
	ASTM D 4021-92		Glass-Fiber Reinforced Polyester Underground Petroleum Storage Tanks
	ASTM D 4097-88		Contact Molded, Glass-Fiber-Reinforced Thermoset Resin Chemical Resistant Tanks
	ASTM D 4138-94		Test Method for Measurement of Dry Film Thickness of Protective Coating Systems by Destructive Means
	ASTM D 4355-92		Test Method for Deterioration of Geotextiles from Exposure to UV Light and Water
	ASTM D 4383-95		Plowable, Raised, Retroreflective Pavement Markers
	ASTM D 4491-92		Test Methods for Water Permeability of Geotextiles by Permitivity
	ASTM D 4533-91		Test Method for Trapezoid tearing Strength of Geotextiles
	ASTM D 4632-91		Test Method for Grab Breaking Load and Elongation of Geotextiles
	ASTM D 4751-95		Test Method for Determining Apparent Opening Size of a Geotextile
	ASTM D 4759-88		Standard Practice for Determining the Specification Conformance of Geosynthetics (1992)
	ASTM D 4833-88		Test Method for Index Puncture Resistance of Geotextiles, Geomembranes, and Related Products
	ASTM D 4873-95		Guide for Identification, Storage, and Handling of Geosynthetic Rolls
	ASTM D 5268-92		Topsoil Used for Landscaping Purposes
	ASTM E 84 REV A-95		Test Method for Surface Burning Characteristics of Building Materials
	ASTM E 96-95			Test Methods for Water Vapor transmission of Materials
	ASTM E 108-95			Test Methods for Fire tests of Roof Coverings
	ASTM E 119 REV A-95	Test Methods for Fire Tests of Building Construction and Materials
	ASTM E 283-91			Test Method for Determining the rate of Air Leakage Through Exterior Windows, Curtain Walls, and Doors
	ASTM E 330-90			Test Method for Structural Performance of Exterior Windows, Curtain Walls, and Doors
	ASTM E 331-93			Test Method for Water Penetration of Exterior Windows, Curtain Walls, and Doors
	ASTM E 447 REV B-92	Test Methods for compressive Strength of Masonry Prisms
	ASTM E 542-94			Standard Practice for Calibration of Volumetric Apparatus
	ASTM E 605-93			Test Methods for Thickness and Density of Sprayed Fire-Resistive Material Applied to Structural Members
	ASTM E 648 REV A-95	Test Method for Critical Radiant Flux of Floor Covering Systems Using a Radiant Heat Energy Source
	ASTM E 699-79			Standard Criteria for Evaluation of Agencies Involved in Testing, Quality Assurance, and Evaluating Building Components in Accordance With Test Methods Promulgated by ASTM Committee E-6 (R1991)
	ASTM E 795-93			Practices for Mounting Test Specimens During Sound Absorption Tests
	ASTM E 1155-87		Test Method for Determining Floor Flatness and Levelness Using the F-Number System
	ASTM F 142-93			Test Method for Indentation of Resilient Floor Tiles (McBurney Test)
	ASTM F 386-93			Test Method for Thickness of Resilient Flooring Materials Having Flat Surfaces
	ASTM F 402-93			Safe Handling of solvent Cements, Primers, and Cleaners Used for Joining Thermoplastic Pipe and Fittings
	ASTM F 405-93			Corrugated Polyethylene (PE) Tubing and Fittings
	ASTM F 477-95			Elastomeric Seals (Gaskets) for Joining Plastic Pipe
	ASTM F 480-94			Thermoplastic Well Casing Pipe and Couplings Made in Standard Dimensions Ratios
	ASTM F 567-93			Installation of Chain Link Fence
	ASTM F 626 REV A-94	Fence Fittings
	ASTM F 656-93			Primers for Use in Solvent Cement Joints  (Vinyl Chloride (PVC) Plastic Pipe and Fittings
	ASTM F 668-95			Poly (Vinyl Chloride) (PVC) Coated Steel Chain-Link Fence Fabric
	ASTM F 708-92			Design and Installation of Rigid Pipe Hangers
	ASTM F 789-95			Type PS-46 Poly (Vinyl Chloride) (PVC) Plastic Gravity Flow Sewer Pipe and Fittings
	ASTM F 883-90			Performance Specification for Padlocks
	ASTM F 894-95			Polyethylene (PE) Large Diameter Profile Wall Sewer and Drain Pipe
	ASTM F 900-94			Industrial and Commercial Swing Gates
	ASTM F 934-94			Standard Colors for Polymer-Coated Chain Link Fence Material
	ASTM F 969-92			Construction of Chain-Link Tennis Court Fence
	ASTM F 1043-95		Strength and Protective Coatings on Metal Industrial Chain Link Fence Framework
	ASTM F 1083-93		Pipe, Steel, Hot Dipped Zinc Coated (Galvanized) Welded, for Fence Structures
	ASTM F 1183-88		Aluminum Alloy Chain Link Fence Fabric (R1992)
	ASTM F 1184-94		Industrial and Commercial Horizontal Slide Gates
	ASTM F 1234-93		Protective Coatings on Steel Framework for Fences

	AWCMA	American Window Covering Manufacturers Association
	355 Lexington Ave.
	New York, NY  10017

	AWI		Architectural Woodwork Institute
	PO Box 1550
				Centreville VA  22020

	AWPA	American Wood Preservers' Association
				P.O. Box 286
				Woodstock MD  21163

	AWPA C 1-95			All Timber Products, Pressure Treatment
	AWPA C 2-95			Lumber, Timbers, Bridge Ties and Mine Ties, Pressure Treatment
	AWPA C 3-95			Piles, Pressure Treatment
	AWPA C 4-95			Poles, Pressure Treatment
	AWPA C 5-95			Fence Posts, Pressure Treatment
	AWPA C 7-92			Incised (Red, White, and Yellow Cedar) Pole Butts, Thermal Treatment
	AWPA C 8-92			Poles, (Red Cedar and Alaska Yellow Cedar), Full Length Thermal Treatment
	AWPA C 9-95			Plywood, Pressure Treatment
	AWPA C 10-91			Poles, (Lodgepole Pine), Full Length Thermal Treatment
	AWPA C 11-90			Blocks for Floors and Platforms, Pressure Treatment
	AWPA C 12-90			Poles, (Western Larch), Full Length Thermal Treatment
	AWPA C 14-94			Wood for Highway Construction, Pressure Treatment
	AWPA C 18-95			Material in Marine Construction, Pressure Treatment
	AWPA C 23-94			Pole Building Construction, Pressure Treatment
	AWPA C 27-93			Plywood, Fire Retardant Pressure Treatment
	AWPA M 4-95			Care of Pressure Treated Wood Products
	AWPA M 18-95			Quality Control Procedures for Permanent Wood Foundation Material
	AWPA P 1/P13-95		Creosote 
	AWPA P 2-95			Creosote Solutions
	AWPA P 3-94			Creosote-Petroleum Oil Solution
	AWPA P 5-95			Waterborne Preservatives
	AWPA P 8-95			Oil-Borne Preservatives
	AWPA P 9-92			Solvents for Organic Preservative Systems

	AWS		American Welding Society, Inc.
				550 Lejeune Rd. NW
				Miami, FL  33126

	AWS A 5.1-91			Carbon Steel Electrodes for Shielded Metal Arc Welding
	AWS A 5.8-92			Filler Metals for Brazing
	AWS B 1.10-86			Guide for Nondestructive Inspection of Welds
	AWS D 1.1-94			Structural Welding Code Steel
	AWS D 1.3-89			Structural Welding Code Sheet Steel
	AWS D 1.5-95			Bridge Welding Code
	AWS D 10.11-87		Recommended Practices for Root Pass Welding of Pipe Without Backing (R1992)
	AWS D 10.12-89		Recommended Practices and Procedures for Welding Low Carbon Steel Pipe
	AWS WI CH 4-80		Ethical and Essential Requirements for the Welding Inspector
	AWS WI CH 16-80		Nondestructive Testing

	AWWA	American Water Works Association
				6666 West Quincy Avenue
				Denver, CO  80235

	AWWA B 300-92			Hypochlorites
	AWWA B 301-92			Liquid Chlorine
	AWWA C 104/A 21.4-90	Cement-Mortar Lining for Ductile-Iron Pipe and Fittings for Water
	AWWA C 105/A 21.5-93	Polyethylene Encasement for Ductile-Iron Pipe Systems
	AWWA C 110/A 21.10-93	Ductile-Iron and Gray-Iron Fittings
	AWWA C 111/A 21.11-90	Rubber-Gasket Joints for Ductile-Iron Pressure Pipe and Fittings
	AWWA C 115/A 21.15-94	Flanged Ductile Iron or Gray Iron Threaded Flanges
	AWWA C 151/A 21.51-91	Ductile-Iron Pipe, Centrifugally Cast, for Water or Other Liquids
	AWWA C 153/A 21.53-94	Ductile-Iron Compact Fittings
	AWWA C 200-91			Steel Water Pipe
	AWWA C 203-91			Coal-Tar Protective Coatings and Linings for Steel Water Pipelines-Enamel and Tape-Hot Applied
	AWWA C 205-89			Cement-Mortar Protective Lining and Coating for Steel Water Pipe
	AWWA C 206-91			Field Welding of Steel Water Pipe
	AWWA C 207-94			Steel Pipe Flanges for Waterworks Service, Sizes
	AWWA C 208-83			Dimensions for Fabricated Steel Water Pipe Fittings (R1989)
	AWWA C 209-90			Cold Applied Tape Coatings for the Exterior of Steel Water Pipelines
	AWWA C 214-89			Tape Coating Systems for the Exterior of Steel Water Pipelines
	AWWA C 500-93			Metal Seated Gate Valves for Water Supply Service
	AWWA C 502-94			Dry Barrel Fire Hydrants
	AWWA C 503-88			Wet-Barrel Fire Hydrants
	AWWA C 508-93			Swing-Check Valves for Waterworks Service
	AWWA C 510-92			Double Check Valve Backflow Prevention Assembly
	AWWA C 511-92			Reduced Pressure Principle Backflow Prevention Assembly
	AWWA C 600-93			Installation of Ductile-Iron Water Mains and Their Appurtenances
	AWWA C 606-87			Grooved and Shouldered Joints
	AWWA C 651-92			Disinfecting Water Mains
	AWWA C 700-90			Cold Water Meters Displacement Type, Bronze Main Case
	AWWA C 701-88			Cold-Water Meters-Turbine Type for Customer Service
	AWWA C 702-92			Cold-Water Meters-Compound Type
	AWWA C 703-86			Cold-Water Meters-Fire Service Type
	AWWA C 704-92			Propeller Type Meters for Waterworks Applications
	AWWA C 710-90			Cold Water Meters Displacement Type, Plastic Main Case
	AWWA C 800-89			Underground Service Line Valves and Fittings
	AWWA C 900-89			Polyvinyl Chloride (PVC) Pressure Pipe
	AWWA C 901-88			Polyethylene (PE) Pressure Pipe and Tubing
	AWWA C 902-88			Polybutylene (PB) Pressure Pipe and Tubing
	AWWA C 905-88			Polyvinyl Chloride (PVC) Water Transmission Pipe, Nominal Diameters
	AWWA D 100-84			Welded Steel Tanks for Water Storage
	AWWA D 120-84			Thermosetting Fiberglass-Reinforced Plastic Tanks (R1989)
	AWWA M 6-86			Water Meters-Selection, Installation, Testing, and Maintenance
	AWWA M 11-89			Steel Pipe-A Guide for Design and Installation
	AWWA M 14-90			Recommended Practice for Backflow Prevention and Cross-Connection Control
	AWWA M-17-89			Installation, Field Testing, and Maintenance of Fire Hydrants
	AWWA M 22-75			Sizing Water Service Lines and Meters
	AWWA M 23-80			PVC Pipe Design and Installation
	AWWA M 31-89			Distribution System Requirements for Fire Protection

		BHMA	Builders Hardware Manufacturers Association
				355 Lexington Ave.
				New York, NY  10017

	BIA		Brick Institute of America
				11490 Commerce Park Drive, Suite 300
				Reston, VA  22091

	BIA 8A REV-88			Portland Cement-Lime Mortar for Brick Masonry

	CDA		Copper Development Association, Inc.
				P.O. Box 1840
		Greenwich, CT  06836‑1840

	CDA 404/0			Copper Tube Handbook

	CE		Corps of Engineers
	(US Department of the Army)
	Chief of Engineers--Referral
	Washington, DC  20314

CED 	Civil Engineering Data
Corps of Engineers
PO Box 631
Vicksburg MS  39180

CED TR HL-80-12-80		Utilization of Filter Fabric for Streambank Protection Applications

CFR		Code of Federal Regulations (Available from the Government Printing Office)
N. Capitol St. between G and H St., NW
Washington, DC  20402

16 CFR Part 1201		Safety Standard for Architectural Glazing Materials
29 CFR 1910			Occupational Safety and Health Standards
40 CFR Part 61 Subpart M	National Emission Standards for Hazardous Air Pollutants

CGA		Compressed Gas Association
1725 Jefferson Davis Hwy, Suite 1004
Arlington VA  22202

CISCA	Ceiling and Interior Systems Construction Association
579 W. North Ave., Suite 301
Elmhurst IL  60126

CISPI	Cast Iron Soil Pipe Institute
5959 Shallowford Road, Suite 419
Chattanooga, TN  37421

CISPI 301-90			Hubless Cast Iron Soil Pipe and Fittings for Sanitary and Storm Drain, Waste, and Vent Piping Applications
CISPI 310-90			Coupling for Use in Connection with Hubless Cast Iron Soil Pipe and Fittings for Sanitary and Storm Drain, Waste, and Vent Piping Applications

CLFMI	Chain Link Fence Manufacturers Institute
1776 Massachusetts Avenue N.W., Suite 500
			Washington, DC  20036

CPSC	Consumer Products Safety Commission
5401 Westbard Ave.
Bethesda, MD 20207

CRA		California Redwood Association
405 Enfrente Drive, Suite 200
Novato, CA  94949

CRI		Carpet and Rug Institute
	P.O. Box 2048
	Dalton, GA 30722

CRSI	Concrete Reinforcing Steel Institute
933 North Plum Grove Road
Schaumburg, IL  60173

CRSI DA 4-90			Manual of Standard Practice

CS		Commercial Standards
U.S. Department of Commerce
			Government Printing Office
			Washington, DC 20402

CTI		Ceramic Tile Institute of America
	12061 West Jefferson Blvd.
	Culver City, CA 90230

DHI		Door and Hardware Institute
			14170 Newbrook Dr.
			Chantilly VA  22021

DHI 1990				Recommended Locations for Architectural Hardware for Standard Steel Doors and Frames
	DOC		Department of Commerce
	14th St. and Constitution Ave., NW
	Washington, DC 20230

	DOT		Department of Transportation
		400 Seventh St., SW
		Washington, DC 20590

	EIA		Electronic Industries Association
	2500 Wilson Blvd.
	Arlington VA  22201-3834

	EIA TIA 568-A-95		Commercial Building Telecommunications Cabling Standards
	EIA TIA 569-90		Commercial Building Standard for Telecommunications Pathways and Spaces
	EIA TIA 5700-91		Residential and Light Commercial Telecommunications Wiring Standard

	EIMA	EIFS Industry Manufacturers Assoc.
		2759 State Road 580, Suite 112
		Clearwater, FL 34621

	EPA		Environmental Protection Agency
		401 M St., SW
		Washington, DC 20460

	FAA		Federal Aviation Administration
			(U.S. Department of Transportation)
			800 Independence Ave., SW
			Washington, DC 20590

	FCC		Federal Communications Commission
			1919 M St., NW
			Washington, DC 20554

	FGMA	Flat Glass Marketing Association
				White Lakes Professional Building
				3310 SW Harrison Street
				Topeka, KS  66611

	FHA		Federal Housing Administration
		U.S. Department of Housing and Urban Development
		451 Seventh St., SW
		Washington, DC 20201

	FHDA	Fir and Hemlock Door Association
		1500 Yeon Building
				Portland, OR  97204

	FM		Factory Mutual Engineering and Research Corp.
				P.O. Box 9102
				Norwood, MA  02062

	FP		Standard Specifications for Construction of Roads and Bridgeson Federal Highway Projects
				Government Printing Office
				Washington, DC  20402

	FS		Federal Standard
			General Services Administration
	Specifications Branch
	Room 6039, GSA Building
	7th and D Streets, S.W.
			Washington, DC  20407

	Fed. Spec.	Federal Specification (from GSA)
	Specifications Unit (WFSIS)
	Room 6039
	7th and D Streets, S.W.
				Washington, DC  20407

	Fed. Spec. A-A-1192 A	Bracket, Pipe
	Fed. Spec. A-A-1909	Fertilizer, Mixed,  Commercial
	Fed. Spec. A-A-2671	Seeds, Agricultural
	Fed. Spec. A-A-2862	Head, Sprinkler, (Underground Connected)
	Fed. Spec. FF-S-760 A (2)	Strap, Retaining (Metal for Conduit, Pipe, and Cable)
	Fed. Spec. FTM-601		Rubber, Sampling and Testing
	Fed. Spec. HH-I-1030 B	Insulation, Thermal (Mineral Fiber, for Pneumatic or Poured Applications)
	Fed. Spec. L-C-530 C	Coating, Pipe, Thermoplastic Resin
	Fed. Spec. L-P-535 E	Plastic Sheet (Sheeting):  Plastic Strip:  Poly (Vinyl Chloride) and Poly (Vinyl Chloride-Vinyl Acetate)
	Fed. Spec. L-T-1512 A	Tape, Pressure Sensitive Adhesive, Pipe Wrapping
	Fed. Spec. L-T-80 B	Tape, Pressure Sensitive Adhesive (Aluminum Backed)
	Fed. Spec. O-F-506 C	Flux, Soldering; Paste and Liquid
	Fed. Spec. OO-A-373 C	Air Conditioners, Single Package Type
	Fed. Spec. OO-A-374 B	Air Conditioners with Remote Condensing Units or Remote Air-Cooled and Water-Cooled Condenser Units, Unitary 
	Fed. Spec. QQ-S-571 E	Solder, Electronic 96 to 485 Deg. C
	Fed. Spec. RR-F-621 E	Frames, Covers, Gratings, Steps, Sump and Catch Basin,  Manhole
	Fed. Spec. RR-H 1070 B	Holder, Garbage Can
	Fed. Spec. TT-C-555 B(1) 	Coating Texture (For Interior and Exterior Masonry Surfaces)
	Fed. Spec. TT-C-595 (2)		Colors; For Ready-Mixed Paints
	Fed. Spec. TT-E-489 J	Enamel, Alkyd, Gloss Low VOC Content
	Fed. Spec. TT-E-490 RE (4)	Enamel, silicone Alkyd Copolymer, Semigloss (For Exterior and Interior Non-Residential Use)
	Fed. Spec. TT-E-506 K (1)	Enamel, Alkyd, Gloss, White and Tints (for Interior Use)
	Fed. Spec. TT-E-529 G	Enamel, Alkyd, Semi-Gloss Low VOC Content
	Fed. Spec. TT-E-545 C	Primer (Enamel, Undercoat, Alkyd, Odorless, Interior, Flat, Tints and White)
	Fed. Spec. TT F-336 E	Filler, Wood Paste
	Fed. Spec. TT-F-1098 D	Filler, Block, solvent-Thinned for Porous Surfaces (Concrete Block, Cinder Block, Stucco, etc.)
	Fed. Spec. TT-P-19 D (1)	Paint, Latex (Acrylic Emulsion, Exterior Wood, and Masonry)
	Fed. Spec. TT-P-25 F (1)	Primer coating, Exterior (Low VOC Undercoat For Wood, Ready-Mixed, White and Tints)
	Fed. Spec. TT-P-29 K	Paint, Latex
	Fed. Spec. TT-P-37 C	Paint, Alkyd-Resin, Exterior Trim, Deep Colors
	Fed. Spec. TT-P-641 G (1)	Primer Coating, Zinc Dust-Zinc Oxide (For Galvanized Surfaces)
	Fed. Spec. TT-P-645 B	Primer, Paint, Zinc-Molybdate, Alkyd Type
	Fed. Spec. TT-P-650 D	Primer Coating, Latex-Baase, Interior White (For Gypsum Wallboard)
	Fed. Spec. TT-P-664 D	Primer Coating, Alkyd, Corrosion-Inhibiting, Lead and Chromate Free, Compliant
	Fed. Spec. TT-P-81 E	Paint, Oil-Alkyd, Ready-mixed Exterior, Medium Shades
	Fed. Spec. TT-S-176 E (1)	Sealer, Surface, Varnish Type, floor, Wood and Cork
	Fed. Spec. TT-S-708 A (2)	Stain Oil: Semi-Transparent, Wood, Exterior
	Fed. Spec. TT-S-711 C	Stain, Oil Type, Wood, Interior
	Fed. Spec. TT-V-121 H	Varnish, Spar, Water-Resisting
	Fed. Spec. TT-V-85 C	Varnish, Oil, (Low Sheen, Brush, or Spray Application)
	Fed. Spec. UU-B-790 A	Building Paper, Vegetable Fiber: (Kraft, Waterproofed and Fire Resistant)
	Fed. Spec. W-P-115 C	Panel, Power Distribution
	Fed. Spec. WW-P-401 F	Pipe and Pipe Fittings, Cast Iron, Soil
	Fed. Spec. WW-P-460 D	Pipe Fittings; Brass or Bronze (Threaded) 125 and 250 pound
	Fed. Spec. WW-U-516 B	Unions, Brass or Bronze, threaded Pipe Connections, and Solder-Joint Tube Connections
	Fed. Spec. WW-V-54 D	Valve, gate, Bronze (125, 150, and 200 pound, screwed)

	FSSB*	Federal Supply Service Bureau
	470 E L'Enfant Plaza SW
			Washington, DC  20407

	FMERC 4880-72			Building Corner Fire Test Procedures

	GA		Gypsum Association
	810 First Street N.E., Suite 510
	Washington, DC  20002

	GAL		Gas Appliance Laboratory
	3133 East Olympic Boulevard
	Los Angeles, CA  90023

	GANA	Glass Association of North America (also FGMA)
	3310 SW Harrison St.
	Topeka KS  66611-2279

	GANA/FGMA-1990		Glazing Manual
	GANA/FGMA-1990		Sealing Manual
	GANA/FGMA-1992		Fabrication, Erection & Glazing Manual

	GSA		General Services Administration
			F St. and 18th St., NW
			Washington, DC 20405

Federal Specifications, Federal Standards, Federal Supply Schedules, and catalogs may be obtained at Business Service Centers of Regional Offices of the General Services Administration.  (Washington, DC; Boston, MA; New York, NY; Philadelphia, PA; Atlanta, GA; Chicago, IL; Kansas City, MO; Fort Worth, TX; Denver, CO; San Francisco, CA; and Auburn, WA.)

	HMA		Hardwood Manufacturers Association
	400 Penn Center Blvd.
	Pittsburgh PA  15235

	HPVA	Hardwood Plywood & Veneer Association
	P.O. Box 2789
	Reston, VA  22090

	IAPMO	International Association of Plumbing and Mechanical Officials
	20001 Walnut Drive S
	Walnut, CA  91789

	ICEA	Insulated Cable Engineers' Association, Inc.
				P.O. Box 440
			South Yarmouth, MA  02664

	IEEE	Institute of Electrical and Electronics Engineers
				345 East 47th Street
				New York, NY  10017

	IEEE 112-91			Test Procedure for Polyphase Induction Motors and Generators

	IESNA	Illuminating Engineering Society of North America
			120 Wall Street
				New York, NY  10005

	ISA
	ISA RP 75.06-81		Control Valve Manifold designs, Recommended Practice

	IFI		Industrial Fasteners Institute
				1505 East Ohio Building
				Cleveland, OH  44114

	LPI		Lightning Protection Institute
		3365 N. Arlington Heights Rd., Suite J
		Arlington Heights, IL 60004

	MBMA	Metal Building Manufacturers Association
				1230 Keith Building
				Cleveland, OH  44115

	MBMA				Fact Book (Annual) Manual (Includes 1990 Suppl)

	MFMA	Maple Flooring Manufacturers' Association, Inc.
	60 Revere Drive, Suite 500
	Northbrook, IL  60062
	Mil. Spec.	Military Specifications
	Naval Publications and Forms Center
	5801 Tabor Avenue
	Philadelphia, PA  19120

	DOD Spec. C-24176 B	Cement, Epoxy, Metal Repair and Hull Smoothing (Metric)
	DOD Spec. P-15328 D	Primer (Wash) Pretreatment (Formula No. 117 for Metals)
	Mil. Spec. A-24179 A	Adhesive, Flexible Unicellular-Plastic Thermal
	Mil. Spec. A-3316 C	Adhesive, Fire-Resistant, Thermal Insulation
	Mil. Spec. A-907 E		Antiseize Thread Compound, High Temperature
	Mil. Spec. A-A-50502	Air- Conditioner, (Unitary Heat Pump)
	Mil. Spec. A-A-50541	Valves, Tank float, Angle and Globe Pattern
	Mil. Spec. B-17452 E	Boilers, Steam and Hot Water
	Mil. Spec. B-18796 F	Burners, Single:  Oil, gas and Gas Oil Combination for Packaged Boilers
	Mil. Spec. B-18897 F	Boilers Steam and Hot Water
	Mil. Spec. B-19564	B	Bedding Compound, Thermal Insulation Pipe Covering
	Mil. Spec. C-19565 C	Coating Compounds, thermal Insulation, Fire and Water-Resistant, Vapor Barrier
	Mil. Spec. C-4556		Coating Kit, Epoxy, for Interior of Steel Fuel Tanks
	Mil. Spec. G-17713 D	Gages, Liquid Level Measuring, Tank
	Mil. Spec. GG-M-2802	Meters, Fluid Quantity, Volumetric
	Mil. Spec. I-2781 F	Insulation, Pipe, Thermal
	Mil. Spec. P-16077 D	Pumps, Centrifugal, Water Circulating Electric-Motor-Driven
	Mil. Spec. P-17552 F	Pump Units, Centrifugal, Water, Horizontal
	Mil. Spec. P-17608	D	Pump, Rotary, Power Driven, Viscous Liquids
	Mil. Spec. P-23236 B	Paint Coating Systems, Fuel and Salt Water Ballast Tanks
	Mil. Spec. R-6855 E	Rubber, Synthetic, Sheets, Strips
	Mil. Spec. T-22361		Thread Compound, Antisieze, Zinc Dust-Petrolatum
	Mil. Spec. T-462 E		Tanks, Liquid Storage, Metal: Fuel-Oil, Horizontal
	Mil. Spec. T-5544 C	Thread Compound, Antiseize, Graaphite-Petrolatum
	Mil. Spec. V-12003 F	Valves, Plug: Cast Iron or Steel, Manually Operated
	Mil. Spec. V-18433 C	Valves, Temperature-Regulating (Thermostatically Controlled)
	Mil. Spec. V-18436 F	Valves, Check: Bronze, Cast-Iron and Steel Body
	Mil. Spec. V-19902 C	Caps, Vent, Fuel Storage Tank
	Mil. Spec. WW-S-2739	Strainer, Sediment, Pipeline, Water, Air, Gas, Oil or Steam
	Mil. Std. 101 B		Color Code for Pipelines and Compressed Gas Cylinders 

	ML/SFA	Metal Lath/Steel Framing Association
				(See NAAMM) 
	MSS		Manufacturer's Standardization Society of the Valve and Fittings Industry, Inc.
	127 Park Street, N.E.
	Vienna, VA  22180

	MSS SP 58-93			Pipe Hangers and Supports-Material, Design and Manufacture
	MSS SP 69-91			Pipe Hangers and Supports - Selection and Applications
	MSS SP 70-90			Cast Iron Gate Valves, Flanged and Threaded Ends
	MSS SP 80-87			Bronze Gate, Globe, Angle and Check Valves

	MUTCD	Manual on Uniform Traffic Control Devices for Streets and Highways
			Superintendent of Documents
				Government Printing Office
				Washington, DC  20402

	NAAMM	National Association of Architectural Metal Manufacturers
			600 South Federal Street, Suite 400
				Chicago, IL  60605

	NAAMM AMP 500-505-88	Metal Finishes Manual

	NACE	National Association of Corrosion Engineers
				1440 South Creek Drive
				Houston, TX  77084

	NACE RP 0169-92		Control of External Corrosion on Underground or Submerged Metallic Piping Systems

	NAPA	National Asphalt Pavement Assoc.
		NAPA Building
		5100 Forbes Blvd.
			Lanham, MD 20706-4413

	NBFU	National Board of Fire Underwriters
				85 John Street.
				New York, NY  10038
		              or
			465 California Street
				San Francisco, CA  94104

	NCMA	National Concrete Masonry Association
				2302 Horse Pen Rd.
				Herndon, VA  22071

NECA	National Electrical Contractors Association
				3 Bethesda Metro Ctr., Suite 1100
				Bethesda, MD  20814

	NECA 				Standard of Installation

	NEMA	National Electrical Manufacturers Association
		2101 L Street, N.W., Suite 300
				Washington, DC  20037

	NEMA 250-91			Enclosures for Electrical Equipment (1,000 Volts Maximum)
	NEMA DC 10-83			Residential Controls-Temperature Limit Controls for Electric Baseboard Heaters (R1989)
	NEMA DC 13-79			Line Voltage Integrally Mounted Thermostats for Electric Heaters (R1991)
	NEMA ICS 1-93			Industrial Control and Systems General Requirements
	NEMA ICS 2-93			Industrial Control and Systems Controllers, Contractors, and Overload Relays
	NEMA KS 1-90			Enclosed and Miscellaneous Distribution Equipment Switches
	NEMA LA 1-92			Surge Arresters
	NEMA LD 3.1-91		Performance Application, Fabrication, and Installation of High Pressure Decorative Laminates
	NEMA MG 1-93			Motors and Generators
	NEMA RN 1089			Polyvinyl-Chloride (PVC) Externally Coated Galvanized Rigid Steel Conduit and Intermediate Metal Conduit
	NEMA TC 2-90			Electrical Plastic Tubing (EPT) and Conduit (EPC-40 and EPC-80)
	NEMA WD 6-88			Wiring Devices, Dimensional Requirements

	NFPA	National Fire Protection Association
				1 Batterymarch Park
			Quincy, MA  02269

	NFPA 10-94			Portable Fire Extinguishers
	NFPA 12A-92			Halon 1301 Fire Extinguishing Systems
	NFPA 13-94			Installation of Sprinkler Systems
	NFPA 14-93			Installation of Standpipe and Hose Systems
	NFPA 24-95			Installation of Private Fire Service Mains and Their Appurtenances
	NFPA 26-88			Recommended Practice for Supervision of Valves Controlling Water Supplies for Fire Protection
	NFPA 30-93			Flammable and Combustible Liquids Code
	NFPA 31-92			Installation of Oil Burning Equipment
	NFPA 49-94			Hazardous Chemicals Data
	NFPA 54-92			National Fuel Gas Code
	NFPA 70-96			National Electrical Code
	NFPA 72-93			National Fire Alarm Code
	NFPA 80-95			Standard for Fire Doors and Fire Windows
	NFPA 80 A-93			Recommended Practice for Protection of Buildings from Exterior Fire Exposure
	NFPA 90 A-93			Installation of Air Conditioning and Ventilating Systems
	NFPA 90 B-93			Installation of Warm-Air Heating and Air-Conditioning Systems
	NFPA 91-95			Exhaust Systems for Conveying of Materials
	NFPA 101-94			Code for Safety to Life from Fire in Buildings and Structures
	NFPA 211-92			Chimneys, Fireplaces, Vents, and Solid Fuel Burning Appliances
	NFPA 255-87			Methods of Test Surface Burning Characteristics of Building Materials
	NFPA 258-94			Research Test Method for Determining Smoke Generation of Solid Materials
	NFPA 325-94			Guide to Fire Hazard Properties of Flammable Liquids, Gases, and Volatile Solids
	NFPA 495-92			Explosive Materials Code
	NFPA 704-90			Standard System for the Identification of the Fire Hazards of Materials
	NFPA 1961-92			Fire Hose
	NFPA 1963-93			Fire Hose Connections

	NHLA	National Hardwood Lumber Assoc.
		PO Box 34518
		Memphis, TN 38184-0518

	NIST	National Institute of Standards and Technology
		US Department of Commerce
		Gaithersburg, MD 20899

	NPA		National Particleboard Association
	18928 Premiere Court
	Gaithersburg, MD  20879

	NPCA	National Paint and Coatings Association
	1500 Rhode Island Avenue, N.W.
				Washington, D.C.  20005

	NRCA	National Roofing Contractors Association
	10255 W Higgins Rd., Suite 600
	Rosemont IL  60018

	NRCA ITEM M L102		Roofing and Waterproofing Manual, 3rd ed.

	NSF		National Sanitation Foundation
	3475 Plymouth Rd.
		Ann Arbor, MI  48105

	NSF 7-90				Food Service Refrigerators and Storage Freezers
	NSF 14-90			Plastic Piping Components and Related Materials
	NSF 21-85			Thermoplastic Refuse Containers

	NTMA	National Terrazzo and Mosaic Association, Inc.
		3166 Des Plaines Avenue, Suite 132
				Des Plaines, IL  60018

	NWWDA	National Wood Window and Door Association 
				1400 East Toughy Avenue, Suite G‑54
				Des Plaines, IL  60018

	NWWDA I.S.1-87		Series for Wood Flush Doors
	NWWDA I.S.2-87		Wood Window Units
	NWWDA I.S.4-81		Water-Repellant Preservative Non-Presure Treatment for Millwork

	OSHA	Occupational Safety and Health Administration
	US Department of Labor
	200 Constitution Ave., NW
	Washington DC  20210

	OSHA 2207-91			Construction Industry
				
	PCA		Portland Cement Association
		5420 Old Orchard Road
				Skokie, IL  60077

	PCI		Prestressed Concrete Institute
	175 West Jackson Blvd, Suite 1859
	Chicago, IL  60604

	MNL 116-85			Manual for Quality Control for Plants and Production of Precast and Prestressed Concrete Products

	PS		Product Standards
	US Department of Commerce
				Government Printing Office
	Washington, DC  20402

	PS 1-83				U.S. Product Standard for Construction and Industrial Plywood
	PS 51				Voluntary Product Standard
	PS1					Veneer Grade & Glue Bond Performance, Exterior Type

	RCSHSB	Red Cedar Shingle and Handsplit Shake Bureau
				515‑116th Avenue, N.E., Suite 275
			Bellevue, WA  98004

	REA		Rural Electrification Administration
	US Department of Agriculture
				14th & Independence Avenue, S.W.
				Washington, DC  20250

	REA 50 17 (DT-5B)		Wood Crossarms, Transmission Timbers and Pole Keys
	REA 50 18 (DT-5C)		Wood Poles, Stubs, and Anchor Logs
	REA 50 24 (DT-19)		Quality control and Inspection of Timber Products
	REA Bulletin 43-5		List of Materials Suitable for Use on Systems of REA Electrification Borrowers

	RFCI	Resilient Floor Covering Institute
		966 Hungerford Dr., Suite 12-B
		Rockville, MD 20850

	SAE		SAE International
	400 Commonwealth Dr.
	Warrendale PA  15096

	SAE J 429-83			Mechanical and Material Requirements for Externally Threaded Fasteners
	SAE J 1349-90			Engine Power Test Code, Net Power Rating (R1995)

	SDI		Steel Deck Institute
				P.O. Box 9506 
	Canton, OH  44711-9506

	SDI		Steel Door Institute
	30200 Detroit Road 
				Cleveland, OH  44145-1967
 
	SDI 107-84			Hardware on Steel Doors (Reinforcement-Application)
	SDI 100-91			Recommended Specifications Standard Steel Doors and Frames
	SDI 111-85			Recommended Standard Details Steel Doors and Frames

	SIGMA	Sealed Insulating Glass Manufacturers' Association
				401 N Michigan Ave.
			Chicago, IL  60611

	SJI		Steel Joist Institute
				1205  48th Avenue North, Suite A
				Myrtle Beach, SC  29577

	SMACNA	Sheet Metal and Air Conditioning Contractors' National Association, Inc.
	4201 Lafayette Center Drive
	Chantilly, VA  22021

	SMACNA-85			HVAC Duct Construction Standards - Metal and Flexible
	SMACNA-93			Architectural Sheet Metal Manual

	SPI		Society of the Plastics Industry, Inc.
	1275 K Street N.W., Suite 400
	Washington, DC  20005

	SPIB
	SPIB 1991			Grading Rules

	SSPC	Steel Structures Painting Council
				4516 Henry St., Suite 301
				Pittsburgh, PA  15213

	SSPC-PA 1-91			Paint Applications: Shop, field, and Maintenance Painting
	SSPC-Paint 9-91		No. 9 white or Colored Vinyl Paint
	SSPC-PS 10.01-82		Painting System Specification No. 10.01 Hot-Applied Coal Tar Enamel Painting System
	SSPC SP 3-89			Surface Preparation No. 3 Power Tool Cleaning
	SSPC SP 6-91			Surface Preparation No. 6 Commercial Blast Cleaning

	STI
	STI-P3-90			Specification and Manual for External Corrosion Protection of Underground Steel Storage Tanks

	SUI
SUI Standard Specifications for Open Web Steel Joists J-Series and H-Series

	TCA		Tile Council of America, Inc.
		P.O. Box 326
				Princeton, NJ  08542-0326

	TCA A 118.1-92		Dry-Set Portland Cement Mortar
	TCA A 137.1-88		Ceramic Tile

	TPI		Truss Plate Institute Inc.
	583 D'Onofrio Drive, Suite 200
	Madison, WI  53719

	UFAS	Uniform Accessibility Standards
				Architectural and Transportation Barriers Compliance Board
				1331 "F" Street NW Suite 1000
				Washington, D.C.  20004

	UL		Underwriters' Laboratories, Inc.
				333 Pfingston Road
				Northbrook, IL  60062

	UL-842-93			Valves for Flammable Fluids
	UL Feb 1995			Recognized Component Directory (Volume 1)
	UL 10-B-86			UL Standard for Safety Fire Tests of Door Assemblies Seventh Edition
	UL 47-87				Semi-Automatic Fire Hose Storage Devices
	UL 55 A-83			UL Standard for Safety Materials for Built Up Roof Coverings
	UL 58-86				Steel Underground Tanks for Flammable and Combustible Liquids
	UL 69-87				Safety Electric Fence Controllers
	UL 70-79				Septic Tanks, Bituminous Coated Metal
	UL 109-78			Tube Fittings for Flammable and Combustible Fluids, Refrigeration Service, and Marine Use
	UL 142-87			Steel Aboveground Tanks for Flammable and Combustible Liquids
	UL 154-84			Carbon-Dioxide Fire Extinguishers
	UL 181-81			Factory-Made Air Ducts and Connectors
	UL 198 B-88			Class H Fuses, Fourth Edition
	UL 198 C-86			High-Interrupting-Capacity Fuses, Current-Limiting Types, Fifth Edition
	UL 198 E-88			Class R Fuses, Fourth Edition
	UL 198 F-88			Plug Fuses, Fourth Edition
	UL 203-89			Pipe Hanger Equipment for Fire Protection Service
	UL 213-78			Rubber Gasketed Fittings for Fire Protection Service
	UL 219-83			Lined Fire Hose for Interior Standpipes
	UL 246-79			Hydrants for Fire Protection Service (1/14/87)
	UL 262-88			Gate Valves for Fire Protection Service
	UL 263-92			UL Standard for Safety Fire Tests of Building Construction and Materials
	UL 268-81			Smoke Detectors for Fire Protective Signaling Systems Second Edition; July 20, 1987 Bulletin
	UL 299-82			Dry-Chemical Fire Extinguishers
	UL 312-88			Check Valves for Fire Protection Service
	UL 399-87			Drinking Water Coolers
	UL 401-86			Portable Spray Hose Nozzles for Fire Protection Service
	UL 405-79			Fire Department Connections
	UL 484-82			Room Air Conditioners
	UL 555-79			Fire Dampers and Ceiling Dampers
	UL 555 S-83			Leakage Rated Dampers for Use in Smoke Control Systems
	UL 559-85			Heat Pumps
	UL 580-88			Tests for Wind Uplift Resistance of Roof Assemblies
	UL 651-89			Schedule 40 and 80 Rigid PVC Conduit
	UL 668-89			Hose Valves for Fire Protection Service
	UL 674-89			Electric Motors and Generators for Use in Hazardous (Classified) Locations
	UL 723-83			Test for Surface Burning Characteristics of Building Materials
	UL 753-89			Alarm Accessories for Automatic Water Supply Control Valves for Fire Protection Service
	UL 789-87			Indicator Posts for Fire Protection Service
	UL 790-83			Safety Tests for Fire Resistence of Roof Covering Materials
	UL 900-87			Test Performance of Air Filter Units
	UL 969-89			UL Standard for Safety Marking and Labeling Systems Third Edition
	UL 992-71			Outline of Investigation for the Test for the Flame Propogation Classification of Flooring and Floor Covering Materials
	UL 1004-89			Electric Motors

	UMC		UMC-1994		Uniform Mechanical Guide

	UPC		UPC-1988		Uniform Plumbing Guide

	USFS	USFS Spark Arrester Guide 1992

	USDA	U.S. Department of Agriculture
			Independence Ave. between 12th St. and 14th St., SW
		Washington, DC 20250

	WA		Wallcoverings Assoc.
		401 N. Michigan Ave.
		Chicago, IL 60611-4267

	WCLIB	West Coast Lumber Inspection Bureau
				P.O. Box  23145
			Portland, OR  97225

	WCLB				Grade Stamps for West Coast Lumber

	WCLB No. 16-89		REV Standard Grading Rules for West Coast Lumber
	WCLB No. 17-91 REV-93	Standard Grading and Dressing Rules

	WRI		Wire Reinforcement Institute, Inc.
	1760 Reston Parkway, Suite 403
				Reston, VA  22090

	WWPA	Western Wood Products Association
				522 SW 5th Avenue, Yeon Bldg
				Portland, OR  97204-2122

	WWPA	Woven Wire Products Assoc.
		2515 N. Nordica Ave.
		Chicago, IL 60635

B.	Referenced Codes with Abbreviations and Acronyms:  Wherever the following acronyms are used in these specifications or on the drawings, they are to be construed the same as the respective expressions represented.  Copies of the referenced codes referred to may be procured by the Contractor from the following:

	LSC		Life Safety Code
				National Fire Protection Association
			1 Batterymarch Park
				Quincy, MA  02269

	NEC		National Electrical Code
			National Fire Protection Association
				1 Batterymarch Park
				Quincy, MA  02269

	NESC	National Electrical Safety Code (ANSI)
	American National Standards Institute
	1430 Broadway
	New York, NY  10018

	NFGC	National Fuel Gas Code
				American Gas Association
				8501 East Pleasant Valley Road
				Cleveland, OH  44131

	UBC		Uniform Building Code
				International Conference of Building Officials
				5360 South Workman Mill Road
				Whittier, CA  90601

	UCBC	Uniform Code for Building Conservation
	International Conference of Building Officials
	5360 South Workman Mill Road
	Whittier, CA  90601

	UMC		Uniform Mechanical Code
				International Association of Plumbing and Mechanical Officials
				5032 Alhambra Avenue
			Los Angeles, CA  90032‑3490

	UPC		Uniform Plumbing Code
				International Association of Plumbing and Mechanical Officials
				5032 Alhambra Avenue
				Los Angeles, CA  90032‑3490

	USEC	Uniform Solar Energy Code
				International Association of Plumbing and Mechanical Officials
		5032 Alhambra Avenue
				Los Angeles, CA  90032‑3490

1.3	DEFINITIONS

A.	Approvals:  Approval of the submittals is an indication that the Contractor's submittals have been reviewed and that there are no objections, except as noted.  Approval of deviations shall apply only to those deviations or omissions from the requirements of the drawings and specifications brought to the Contracting Officer's attention in writing.  After approval of an item, submit a substitute for approval when the approved item cannot be purchased or delivered in time to avoid delay in completion of the project.

1.4	SUBMITTALS

A.	Scope:  Submittals include design computations, shop drawings, manufacturers' literature, as‑built drawings, samples, and maintenance manuals.

*******************************************************************************
Insert number of days to be allowed for review.  Normally 10 days is sufficient.
*******************************************************************************

B.	Requirements:  Refer to specifications for submittals required.  Allow at least [    ] working days for review.  Submittals shall be delivered to [                                                 .]

C.	Identification of Submittals:  Completely identify each submittal by showing at least the following information:
1.	Name and address of submitter, plus name and telephone number of the individual to contact for further information.
2.	Name of project as it appears in these specifications.
3.	Contract number, drawing number, and specification section number to which the submittal applies.
4.	Whether this is an original submittal or resubmittal.
5.	Each item shall clearly note the manufacturer's name and address, trade name, product, lot, style, color, catalog designation or model number, and locations of use.

1.5	CERTIFICATES OF CONFORMANCE

A.	Requirements:  The Contracting Officer may permit use, prior to sampling and testing, of materials when accompanied by Certificates of Conformance.  Materials used on the basis of a Certificate of Conformance may be sampled and tested.  Installation of materials on the basis of Certificates of Conformance shall not relieve the Contractor of responsibility for incorporating materials which conform to the requirements of the drawings and specifications.  Material not conforming to those requirements will be subject to rejection, whether in place or not.  

B.	Format:  The Certificate of Conformance provided by the supplier shall:
1.	State that the named product conforms to the Contract requirements.
2.	Either be accompanied with a certified copy of the test results, or certify that such test results are on file with the manufacturer and will be furnished to the Contracting Officer upon request.
3.	Provide the name and address of the manufacturer, the testing agency, and the date of tests.
4.	Set forth the means of identification which will permit field determination of the product delivered as being the product covered by the certification.

1.6	QUALITY ASSURANCE

A.	Codes and Standards:  The work shall comply with codes and standards applicable to each type of work and as listed in the individual sections of these specifications.  This Contract incorporates materials, applications, and tests by reference, with the same force and effect as when they were given in full text.

B.	Conflict:  Where a conflict occurs between reference documents and project specifications, the project specifications shall govern.

C.	Measurements:  Where approved manufacturer's diagrams and shop drawings give specific measurements or rough‑in dimensions for equipment, these dimensions shall take precedence over dimensions indicated on the drawings.

D.	Equipment:  Prior to ordering equipment, verify dimensions and functions of equipment proposed for use [including the electrical service requirements].  [Be certain the equipment is compatible with the structural and architectural features of the work, avoids conflicts with equipment of other crafts, and that it will fit in the space provided.]

1.7	DELIVERY, STORAGE, AND HANDLING

A.	Delivery:  Protect products incorporated into the work from damage while in transit to the site.  Products must be delivered in original unopened containers with manufacturer's name, brand designation, and contents legibly indicated.  [The containers shall bear the referenced specification number, type, and class as applicable.]

B.	Storage:  Provide temporary storage facilities for products.  Storage shall comply with the manufacturer's instructions.  The storage area shall permit access for inspection and handling.

C.	Handling:  Load and unload products protecting them from damage. 

1.8	PROJECT/SITE CONDITIONS

*******************************************************************************
INSERT FIRE PLAN AS APPROPRIATE.  INSERT SPECIFIC REQUIREMENTS NOT COVERED BY FAR CLAUSE 52.236‑10.
*******************************************************************************

A.	Access to the Work:  [                                      .]

*******************************************************************************
INSERT SPECIFIC REQUIREMENTS NOT COVERED BY FAR CLAUSES 52.236‑9 AND 52.236‑10.
*******************************************************************************

B.	Environmental Considerations:  [                               .]
1.9	SEQUENCING AND SCHEDULING

A.	Work Schedule:  The schedule shall be submitted at the pre‑work conference.  When requested, submit an updated schedule within 3 calendar days.  As a minimum, the estimated start and completion dates shall be shown in the estimate.

PART 2:  PRODUCTS

	(There are no applicable requirements.)

PART 3:  EXECUTION

3.1	PROJECT MEETINGS

A.	Pre‑Work Conference:
1.	Will be held prior to the start of work.  The Contractor will be notified in advance of meeting time, date and place.  The purpose will be to review required work, project drawings and specifications, construction schedules, payroll and payments, and administrative provisions of the Contract.
2.	The Contractor, subcontractors and the persons responsible for coordination of the work shall be present at the meeting.
3.	Be prepared to summarize and explain procedures planned for the project [and present the submittals requested in the specifications].

B.	Progress Meetings:
1.	To be held at the project site, or as determined by the Contracting Officer.
2.	May be called by either the Contracting Officer or the Contractor.  Request shall state who should attend and include an agenda.

C.	Final Inspection:
1.	To be held at the project site, or as determined by the Contracting Officer.
2.	Notify the Contracting Officer in writing at least [  ] working days before the completion date so the Government can schedule final inspection.
3.	The superintendent shall be present during this inspection.

3.2	PREPARATION

*******************************************************************************
DESCRIBE PRECISELY WHAT WILL BE STAKED AND WHAT ELEVATIONS WILL BE FURNISHED BY THE GOVERNMENT, WHEN SUCH ITEMS ARE NOT SHOWN ON THE DRAWINGS OR COVERED BY FAR CLAUSE 52.236‑17.
*******************************************************************************

A.	Work Layout:  [The Government will set [          ] to give the Contractor measurements, lines and grades necessary for the work executed under the Contract.]  [Baseline monuments or benchmarks disturbed or removed during construction shall be reset by the Contractor at the Contractor's expense.]

B.	Work Limits and Control Points:  Will be [staked] [and] [established] by the Contracting Officer.

3.3	PROJECT MONUMENT

A.	Requirements:  Install a Government‑furnished project monument at the location designated by the Contracting Officer.  The installation shall be as detailed on the drawings.

3.4	SALVAGEABLE ITEMS

A.	Requirements:  Salvageable items consisting of [     ] shall become the property of the [Contractor.]  [Government.]  [Remove and store items designated as salvage for the Government at the locations approved in writing by the Contracting Officer.]  [Government property shall be left on the site at locations designated by the Contracting Officer.]  [Government property shall be delivered to [          .]]  [Replace or reimburse the Government for items designated as salvage for the Government that are lost or destroyed during demolition work.]  [Items which have become the property of the Contractor shall be removed from the work site.]  

3.5	DISPOSAL OF DEBRIS

A.	Requirements:  Items or debris not designated as salvage for the Government shall become the property of the Contractor.  [Disposal of materials in a legal manner and payment of fees required is the Contractor's responsibility.]  [Items or debris may be hauled to the site indicated on the drawings.]  [Sale of material onsite is not allowed unless authorized in writing by the Contracting Officer.]  [When hazardous materials are encountered during demolition operations, comply with applicable federal, state, and local regulations, laws, and ordinances concerning removal, handling, and protection against exposure or environmental pollution.]  [Burning of removed materials is not permitted on the work site.]

3.6	PROJECT IDENTIFICATION

A.	Requirements:  Furnish and install a project sign that shall be located at the main construction entrance to the site.  The size, mounting, construction, paint colors and lettering shall be as detailed on the drawings.

3.7	AS‑BUILT DRAWINGS

A.	General Requirements:  A complete set of full-sized prints, furnished by the Contracting Officer for this purpose only, shall be kept at the site.  As the job progresses, continuously maintain as-built drawings of the work.  The changes shall be noted legibly in red pencil or red ink.  These drawings shall be submitted to the Contracting Officer prior to final inspection.  [Should final inspection reveal changes in the project not so noted on the as‑built drawings, record these changes on the as‑built drawings within 5 working days of final inspection and deliver completed as‑built drawings to the Contracting Officer.]

B.	Installation Changes:  Records shall be maintained of actual installations where at variance with the work shown, where changed, or where not otherwise located by dimension, elevation or other reference on the Contract drawings.  Actual locations and elevations of equipment and components (such as pipe, conduits and ducts) occurring within concealed areas shall be recorded by actual dimensions referenced from readily accessible and permanent structures or monuments.

3.8	WARRANTY

A.	Requirements:  Materials and equipment furnished under this Contract shall be covered by the most favorable commercial warranties given to customers for such materials or equipment.  The rights or remedies provided herein are in addition to and do not limit rights afforded to the Government by other clauses of this Contract.  With respect to warranties, expressed or implied, from manufacturers or suppliers for materials or equipment furnished under the Contract the Contractor shall:
1.	Obtain warranties that would be given in normal commercial practices.
2.	Require warranties to be executed, in writing, for the benefit of the Government.
3.	Submit warranties to the Contracting Officer prior to the final inspection.

3.9	TRAINING OF GOVERNMENT EMPLOYEES

*******************************************************************************
INSERT SYSTEM REQUIRING TRAINING AND HOURS OF TRAINING REQUIRED.
*******************************************************************************

A.	Requirements:  Prior to final acceptance, provide instruction for employees designated by the Contracting Officer in the operation and maintenance of each system and its equipment.  The instructor's expertise shall be appropriate to the particular system involved.  Instructions by a factory-trained representative approved by the Contracting Officer shall be provided for systems.  Prior to the start of training, the instructors shall submit an outline of the proposed training (including hours of training planned) and copies of training materials to be distributed to the trainees for approval by the Contracting Officer.  Minimal training periods shall be as follows:

System			Hours of Training

PART 4:  MEASUREMENT AND PAYMENT

4.1	METHOD OF MEASUREMENT

*******************************************************************************
SELECT "THE CONTRACT" PHRASE WHEN A "LUMP SUM" CONTRACT.
*******************************************************************************

A.	Units:  [There will be no separate measurement for individual items of work done under this Contract.]  [The work described in this section will not be measured for payment.]

4.2	BASIS OF PAYMENT

*******************************************************************************
SELECT PAYMENT PHRASE WHICH INDICATES PAY ITEM WHEN A "LUMP SUM" CONTRACT.
*******************************************************************************

A.	Payment:  [No direct payment for the work described under this section will be made.  Consideration for this item shall be included in the bid price for other items of the Contract.]  [Payment will be made at the Contract price, as indicated in the Bid Schedule, and will include full compensation for the work described in the Contract.  Payment will be made under:]
Pay Item		Pay Unit

99999(01)  [                ]	Lump Sum

END OF SECTION

SECTION 01009 REMOVE THIS PAGE

GENERAL INFORMATION AND REQUIREMENTS
11/01
Project Name (ftr B)