D EPICS Alarm Handler

Geoff Savage

D Analog I/O Alarms

• Alarm limits

HIHI

HIGH LOW LOLO

• Severity

MAJOR - attention and dangerous

MINOR - attention not dangerous

NO_ALARM - turn off alarms

D Alarm Limits

record(ai,"RM1/AD00") { field(DESC, "Rack Monitor RM1/AD00") field(DTYP, "Raw Soft Channel") field(INP, "RM1.AD00 NPP NMS") field(SCAN, "1 second") field(LINR, "NO CONVERSION") field(ASLO, "4.885E-3") field(AOFF, "0.0") field(HIHI, "9") field(HHSV, "MAJOR") field(HIGH, "6") field(HSV, "MINOR") field(LOW, "-6") field(LSV, "MINOR") field(LOLO, "-9") field(LLSV, "MAJOR") }

HIHI=9V

HIGH = 6V

LOW= -6V

LOLO= -9V

D Alarm Handler

• Channel access client

• Registers for events

Configuration file

• Hierarchical display

D No Alarms

D Alarms