PHENIX Collaboration OFFLINE Computing System

PEP Message Passing Example

No. From To Message Action by Receiver 1 Dop Ctr Idle Controller locates idle Input 2 Ctr Inp Process Input read and prepares data strucures for one event 3 Inp Ctr Done + DSpointer

Controller prefpares message for Dop 4 Ctr Dop Process + DSpointer

Dop changes state and prepares message for Input 5 Dop Inp Deliver + DSpointer

Insert event in PVM buffer and submit it 6 Inp Dop DS buffer Dop unpacks event 7 Inp Ctr Idle Update proxy state 8 Dop Ctr Processing Update proxy state