E949: K^+ !π^+νν

Alberta/BNL/FNAL/Fukui/IHEP/INR/KEK Kyoto/UNM/Osaka/TRIUMF/Yeshiva

Sensitivity Improvement compared to E787 (1995):

ffl Increased spill length (�1:56) ffl Lower Momentum (�1:38) ffl Increased efficiency (trigger,DAQ,analysis) (�3:2)

{ Increase acceptance below K_{ß2} peak [�2] { Re-optimize analysis for higher rates [�2]

ffl Total gain of �14 (per hour of running)