a = -1.2�65 mmDC pads (50x50)Guard RingPoly ResistorsBias Line(metalized)AC pads (150x60)metal jumpersimplanted n+ strips (10x72380)5353 mm 4850 mmScribeLine50mm150mmLayer 4, Z-side