History of Hybrid/Module 49^{CERN hybrid dataFNAL hybrid data}FNAL module data

Channel/Strip

0 20 40 60 80 100 120

Pedestal [FADC Counts]

0

10

20

30

40

50

60 Chip 0x40 Pedestals and Noise

Noise [FADC Counts]

0 1 2 3 4 5 6 7 8 9

Chip 0x40

Channel/Strip

0 20 40 60 80 100 120

Pedestal [FADC Counts]

0

10

20

30

40

50

60

Chip 0x42 Pedestals and Noise

Noise [FADC Counts]

0 1 2 3 4 5 6 7 8

Chip 0x42

Channel/Strip

0 20 40 60 80 100 120

Pedestal [FADC Counts]

0 10 20 30 40 50 60

Chip 0x48 Pedestals and Noise

Noise [FADC Counts]

0 1 2 3 4 5 6 7 8

Chip 0x48

Channel/Strip

0 20 40 60 80 100 120

Pedestal [FADC Counts]

0 10 20 30 40 50 60 70

Chip 0x4a Pedestals and Noise

Noise [FADC Counts]

0

2

4

6

8

10

Chip 0x4a