* * * * * * * * 

READ AND REMOVE THIS PAGE BEFORE PLACING
THE SPECIFICATION SECTION IN THE CONTRACT

* * * * * * * *

DIVISION 8:  DOORS AND WINDOWS

SECTION 08708 ‑ FINISH HARDWARE

USE:	Furnishing and installing finish hardware for doors listed in Door Schedule.  

NOTES TO SPECIFIER:

	A.	Options within paragraphs are identified by enclosure in brackets; blank spaces enclosed by brackets [_____] provide for information to be inserted, as appropriate, to individual projects.

	B.	TO AVOID CONFLICTING REQUIREMENTS AND COSTLY MISTAKES, the specifier must edit (delete, substitute or add to the text).  The remaining paragraphs must be renumbered.

	C.	DELETE FOR FINAL COPY: Notes to the Specifier, located between lines of asterisks; all [brackets], underlining, boldface, and italics, within the paragraphs; and this page.  (Open Reveal Codes [alt F3] to do this accurately.)

	D.	To Edit “(Footer B)”: (Corel 8).  ENTIRE FOOTER SHOULD BE BOLDED.  Click in the footer and delete the “Project Name (ftr B)” text and replace it with the Name of the Project (upper and lower case).  Replace date with current MM/YY (WITHOUT BRACKETS).

	E.	The Guide Specifications are intended to be continuously reviewed and revised.  User’s technical comments are appreciated.  Also, other related or similar specification that are written “from scratch” that could benefit others, or other questions can be sent to NSTC A/E Group, ST 110, or call (303) 987-6868.

DRAWING DATA REQUIRED: 

REQUIRED SPEC MODIFICATIONS:

GENERAL NOTES

A.	Whenever entire articles, paragraphs, or subparagraphs are not applicable, the articles, paragraphs, or subparagraphs should be deleted; when necessary, reletter or renumber articles, paragraphs, or subparagraphs.

B.	THIS GUIDE IS NOT INTENDED AS A SUBSTITUTE FOR READING THE ENTIRE SECTION.

TECHNICAL NOTES

A.	1.1B:  Select or add applicable specification sections.  Do not list specification sections from Division 8.

B.	1.2:  Select or add applicable references.

	C.	1.4A:  Select applicable phrase.

D.	1.4B:  Insert number of copies of the manufacturer's descriptive data required.  Normally 5 copies are required.  Distribution after review is normally 1 copy to the CO, 3 copies to the Contractor, and 1 copy to the project file.

E.	1.4C:  Insert number of copies of installation instructions required.  Normally 5 copies are required.  Distribution after review is normally 1 copy to the CO, 5 copies to the Contractor, and 1 copy to the project file.

	F.	1.4D:  Insert number of copies of the manufacturer's operating and maintenance instructions required.  Normally 5 copies are required.  Distribution after review is normally 1 copy to the CO, 3 copies to the Contractor, and 1 copy to the project file.

G.	1.4E:  Insert number of copies of hardware schedule required.  Normally 5 copies are required.  Distribution after review is normally 1 copy to the CO, 3 copies to the Contractor, and 1 copy to the project file.

H.	4.1 and 4.2:  When a "lump sum" Contract is used, delete the title PART 4:  MEASUREMENT AND PAYMENT, and both articles from this specification section.  Measurement and payment will be addressed in Part 4 of Section 01010.

REVISIONS OF THIS SECTION:
CSI format, editorial changes: 12/01
Metric:  
Technical Update: 01/94

SECTION 08708

FINISH HARDWARE
PART 1:  GENERAL

1.1  SUMMARY:

	A.	Section Includes:  Furnishing and installing finish hardware on doors as noted in the Door Schedule.

1.2  REFERENCES:

	A.  American National Standards Institute:
	ANSI A 156.1-88	Butts and Hinges
		ANSI A 156.2-89	Bored and Preassembled Locks and Latches
		ANSI A 156.3-89	Exit Devices and Directory of Certified Exit Devices
		ANSI A 156.4-86	Door Controls - Closers
		ANSI A 156.5-84	Auxiliary Locks and Associated Products
		ANSI A 156.6-86	Architectural Door Trim
		ANSI A 156.7-88	Template Hinge Dimensions
		ANSI A 156.8-88	Door Controls - Overhead Holders
	ANSI A 156.14-91	Sliding and Folding Door Hardware
		ANSI A 156.15-86	Closer Holder Release Devices
		ANSI A 156.16-89	Auxilliary Hardware
		ANSI A 156.18-87	Materials and Finishes
	ANSI A 156.21-89	Thresholds

	B.  Door and Hardware Institute:
	DHI				Recommended Locations for Builder's Hardware for Standard Steel Doors and Frames

	C.  International Conference of Building Officials (ICBO):
	UBC‑1994     		Uniform Building Code

	D.  National Fire Protection Association:
	NFPA 101‑94   	Code for Safety to Life from Fire in Buildings and Structures

	E.  Underwriters' Laboratories, Inc.:	
	UL  969‑89 		UL Standard for Safety Marking and Labeling Systems Third Edition

1.3  SYSTEM DESCRIPTION:

	A.	Performance Requirements:  Doors, when latched, shall fit snugly against silencers.  There shall be no movement of the door possible when door is latched; however, there shall also be no extra force required to latch the door.

1.4  SUBMITTALS:

	A.	General:  Submittals shall be according to [Section 01009 - General Information and Requirements.] [and] [Section 01300 ‑ Submittals.] [and] [Section 01365 - Certificates of Conformance.] 

	B.	Manufacturer's Literature:  Submit [__] copies of the manufacturer's descriptive data for the finish hardware to be used on this project.

	C.	Installation Instructions:  Submit [__] copies of the manufacturer's installation instructions for the finish hardware to be used on this project.

	D.	Operating and Maintenance Instructions:  Submit [     ] copies of manufacturer's operating and maintenance instructions for finish hardware to be used on this project.  

	E.	Hardware Schedule:  Submit [     ] copies of the schedule covering hardware for all personnel doors.  Coordinate hardware with doors, frames, and related work to ensure proper size, weight, hand function, and finish.  Organize schedule into "sets" indicating every item required for each door and frame.  Furnish approved hardware template to each fabricator of doors and frames requiring factory preparation for hardware installation.  Include the following:
		1.  Name and manufacturer for each item.
		2.  Type, style, function, size, and finish for each item.
		3.  Hardware location cross‑referenced to floor plans.
		4.  Explanation of schedule abbreviations, symbols, and codes.
		5.  Door and frame sizes, and materials.
		6.  Keying information.

1.5  QUALITY ASSURANCE:

	A.	Hardware Consultant:  The Contractor shall have a hardware supplier who has an employee who is a member of the American Society of Hardware Consultants with the technical experience to correctly interpret these Contract documents and efficiently service the hardware portion of this Contract.  This representative shall be available, subject to call by the Contracting Officer.  [This representative shall make a personal inspection of the hardware after application and before final inspection, to see that the hardware is properly installed and in good working order.  In case of faulty installation, he shall inform the Contractor and the Contracting Officer, and suggest proper corrections.]

	B.	Labeling Requirements:  Provide UL label on exit devices required on fire‑rated doors.

	C.	Product Uniformity:  The warranty for all components and type of hardware (butts, locksets, closers, and other items necessary to complete the intended application) shall be covered by a single manufacturer.

	D.	Failure Criteria:  Not limited to the following:
	1.  Units coming loose from their mounts.    
	2.  Units becoming non‑functional.
   	3.  Units' finish becoming tarnished through normal use.

1.6  SEQUENCING AND SCHEDULING:

	A.	Readiness:  Doors shall have been previously primed and shall be ready for application of hardware prior to application of finish coats.
		1.	Do not install hardware until areas routed or drilled for hardware have been painted.  Do not install hardware until complete door has been painted, including tops and bottoms.

1.7  MAINTENANCE:

	A.	Specialized Maintenance Tool Set:  Furnish a complete set which will be required for future adjustment, maintenance, removal, and replacement of hardware.

PART 2:  PRODUCTS

2.1  MATERIALS:

	A.	Door Hardware:  Shall comply with the followings standards:
		1. 	Butts and Hinges					ANSI A 156.1	
		2. 	Locks and Trim					ANSI A 156.2	
	3. 	Exit Devices						ANSI A 156.3		
	4. 	Closers							ANSI A 156.4		
		5. 	Auxiliary Locks					ANSI A 156.5		
	6. 	Architectural Door Trim				ANSI A 156.6		
	7. 	Template Hinge Dimensions			ANSI A 156.7	
	8. 	Overhead Holders					ANSI A 156.8		
	9. 	Closer Holder Release Devices		ANSI A 156.15		

10.	ab	Auxiliary Hardware					ANSI A 156.16	
11.	ab	Materials and Finishes				ANSI A 156.18	
12.	ab	Sliding and Folding Door Hardware	ANSI A 156.14	
13.	ab	Thresholds						ANSI A 156.21

	B.	Fastenings:  Finish hardware shall be furnished with necessary screws, bolts or other fastenings of suitable size and type to anchor the hardware in position for heavy use and long life, and shall harmonize with the hardware as to material and finish.  These fastenings shall be furnished where necessary with expansion shields, sex bolts, toggle bolts, or other approved anchors according to the material to which it is applied and according to the manufacturer's written instructions.

	C.	Keys:  Provide two keys for each lock furnished.  Die stamp each key with numbers of lock change and set symbol number or letter.  Keys shall be turned in to the Contracting Officer, who will issue a receipt for them.

	D.	Keying:  Locks shall be keyed alike in groups, master‑keyed and grand master‑keyed, as approved by the local governing authority.  Furnish five master keys for each set and five grand master keys direct by registered mail from lock manufacturer to the Contracting Officer properly marked for easy identification.

E.	Key Security:  For security purposes, keying must be done by the lock manufacturer and permanent records maintained by this manufacturer.  Keying chart from manufacturer shall be made available to the Government.  

PART 3:  EXECUTION

3.1  PREPARATION:

	A.	General:  Mortised items shall be fitted and then removed and placed in their original packages until painters have completed their work.

	B.	Blocking:  Provide solid blocking for wall stops.

3.2  INSTALLATION:

	A.	General:  Install each hardware item in compliance with the manufacturer's instructions.  Wherever cutting and fitting are required to install hardware on surfaces which will be painted or finished at a later time, install each item completely and then remove and store in a secure place.  After completion of the finishes, reinstall each item.  Do not install surface‑mounted items until finishes have been completed on the substrate.

	B.	Location:  Install the required hardware on the appropriate door according to the approved hardware schedule.

	C.	Cylinder Cores:  Remove construction cores from cylinders and replace with permanent cores in the presence of the Contracting Officer.  Demonstrate that tagged keys operate respective locks.  Deliver tagged keys to the Contracting Officer upon acceptance of each core cylinder installation.

	D.	Installation:  Manuals accompanying the hardware shall be consulted and their instructions strictly adhered to.
	1.	Mounting Heights:  Mount units at heights identified by the Door and Hardware Institute, except as otherwise indicated.
		2.	Install each hardware item in compliance with the manufacturer's instructions.  Wherever cutting and fitting are required to install hardware on surfaces which will be painted or finished at a later time, install each item completely and then remove and store in a secure place.  After completion of the finishes, reinstall each item.  Do not install surface-mounted items until finishes have been completed on the substrate.

	E.	Silencers:  Door frames shall receive rubber door silencers; single doors shall receive three per door; double doors shall receive two per opening.  
		1.	Doors, when latched, shall fit snugly against silencers.  There shall be no movement of the door possible when door is latched; however, there shall also be no extra force required to latch the door.
		2.	Apply single door silencers to jamb stop strip and apply double door silencers to header stop strip near the center of opening.

	F.	Fasteners:  Use fastening devices as needed to securely anchor hardware according to manufacturer's published templates.  Self‑tapping sheet metal screws are not acceptable.  Closers and exit devices on wood doors shall be through‑bolted.

303  ADJUSTING:

	A.	General:  Wherever hardware installation is made more than one month prior to acceptance or occupancy, make a final check and adjustment of hardware items during the week prior to acceptance or occupancy.  Clean and lubricate operating items as necessary to restore proper function and finish of hardware and doors.  Adjust door-control devices to compensate for final operation of heating and ventilating equipment.  Adjust and check each operating item of hardware and each door to insure proper operation or function of every unit.  Replace units which cannot be adjusted to operate freely and smoothly.

3.4  DEMONSTRATION:

	A.	Requirements:  Instruct designated Government personnel in proper adjustment and maintenance of hardware and hardware finishes.

PART 4:  MEASUREMENT AND PAYMENT

4.1  METHOD OF MEASUREMENT:

	A.	Units:  The work described in this section will not be measured for payment.

4.2  BASIS OF PAYMENT:

	A.	Payment:  No direct payment for the work described under this section will be made.  The Contractor shall include consideration for this item in the bid price for other items of the Contract.

END OF SECTION

FINISH HARDWARE
[12/01]
Project Name (ftr B)