VME SLAVE INTER- FACE

Trigger Logic

CLOCK & CONTROL FANOUT

Flat Cables to 8 Preamp/ Digitizer Card

Shift Register Interface PLDs Xilink & DAQ Pipline

Line Xceivers

Level 2 Trigger bit 32 ch/flat cable

256 ch/board

( 6 CES/CWIR 1 CPR & 1 CCR)