E-787 TN 314 June 6, 2000

Experiment 787 Technical Note No. 314

Trigger Definitions — 1995–98 S. Kettell, P. Meyers, T. Nakano

The definitions of the various triggers used in 1995–1998. This version revised 6-June-2000. This file now supercedes /e787d/e787/tr2/doc/trigger.definitions on bnlku7.

Trigger TB AO PS Ref Description

pnn(1) 4s0 A01 0-0 TB-17 KB · IC · DC · T•2 · (6_{ct} + 7_{ct}) · (19_{ct} + 20_{ct} + 21_{ct}) · BV + EC · (L0rr1(1) · US + L0rr1(2) · DS) · HEX · L1.n pnn(2) 2s0 A02 0-1 T2-141 KB · IC · DC · T•2 · 3_{ct} · 4_{ct} · 5_{ct} · 6_{ct} · (13_{ct} + · · · + 18_{ct}) · (19 + 20 + 21) ·

BV + EC · L0rr2(1) · HEX · L1.n

Kpi2(1) 4s2 A09 2-0 TB-17 KB · T•2 · (6_{ct} + 7_{ct}) · (19_{ct} + 20_{ct} + 21_{ct}) · TBPS Kpi2(2) 4s3 A06 1-1 TB-17 KB · IC · DC · T•2 · (6_{ct} + 7_{ct}) · (19_{ct} + 20_{ct} + 21_{ct}) · HEX · TBPS · L1.n Kmu2(1) 4s4 A10 2-1 TB-17 KB · T•2 · (6_{ct} + 7_{ct}) · (19_{ct} + 20_{ct} + 21_{ct}) · TBPS Kmu2(2) 4s5 A11 2-2 TB-17 KB · DC · T•2 · (6_{ct} + 7_{ct}) · 21_{ct} · BV · TBPS 3gamma 5s3 A15 0-3 TB-30 KB · DC · T•2 · (3_{ct} + 4_{ct}) · (7_{ct} + 8_{ct}) · (9 + · · · + 21) · EC · HEX · NG3 3gamma(95) (6s1)(A14)(3-2) T2-143 KB · IC · DC · T•2 · (6_{ct} + 7_{ct}) · (11 + · · · + 20) · (19_{ct} + 20_{ct} + 21_{ct}) ·

EC · HEX · NG3

1gamma 6s1 A08 1-3 T3-104 KB · IC · DC · T•2 · (6_{ct} + 7_{ct}) · (19_{ct} + 20_{ct} + 21_{ct}) · HEX · EC · BV · NG2 · L1.n Kmu2g 5s0 (A14)(3-2) T2-148 KB · DC · T•2 · (6_{ct} · 7_{ct} · · · · · 16_{ct}) · HEX · EC · BVh · 21 · NG2 CEX 5s1 A16 3-3 TB-23 KB · DC · 2( T•2 ) · (6_{ct} + 7_{ct}) · BV + EC + πB · (19_{ct} + 20_{ct} + 21_{ct}) prompt 5s2 A03 0-2 TB-30 KB · C_π · T•2 · (6_{ct} + 7_{ct}) · (19_{ct} + 20_{ct} + 21_{ct}) · BV + EC · HEX · L0rr1(4) · L1.n Kpi2(3) 6s0 A07 1-2 T2-142 KB · IC · DC · T•2 · (6_{ct} + 7_{ct}) · (19_{ct} + 20_{ct} + 21_{ct}) · BV · HEX · L0rr1(3) · L1.n minbias 6s2 A14 3-2 TB-20 KB · IC · DC · T•2 pnn1L0 4s0 A12 2-3 TB-17 KB · IC · DC · T•2 · (6_{ct} + 7_{ct}) · (19_{ct} + 20_{ct} + 21_{ct}) · BV + EC · (L0rr1(1) · US + L0rr1(2) · DS) · HEX pnn1L0o 4s1 A13 3-0 TB-17 KB · IC · DC · T•2 · (6_{ct} + 7_{ct}) · (19_{ct} + 20_{ct} + 21_{ct}) · BV + EC · TBPS piscat 2s2 B01 4-1 TB-16 πB · DC · IC · T•2 · (6_{ct} + 7_{ct}) · (20 + 21) · BV + EC · HEX KB — D02 4-0 KB eckmu2 — D03 4-2 KB · (EC + CO)Sum · ( T•2 + BV + RS + prompt) Xe — D04 — Xe Ref PMT pibeam — D06 3-1 πB cosmic — D10 — T•2 · IC · spill or T•2 · IC or T•2 · (>1 non-adj IC) pulser — D11 4-3 Prescaler EOS — D12 — end-of-spill gate generator YAlO — D13 — EC Xtal OR random — D14 — BVsum

Description of elements:

KB Beam kaon C_K · B4 · TTsum · spill

πB Beam pion C_π · B4 · TTsum · spill

IC I counter hit
T•2 Concidence of 1st and 2nd layer of RS in the same sector and IC
DC Delayed Coincidence (IC timing - KB timing > 2 ns)
EC Endcap Veto (upstream and downstream)
BV Barrel Veto discriminated analog sum
BVh Barrel Veto (integrated analog sum), high threshold
6 Hit in 6 layer of RS
6_{ct} Hit in 6 layer of RS, associated with a T•2 (“charged track”)
HEX 1 or 2 adjacent hit hextants
L0rr1(i) pnn(1) Refined Range using MLU mask, bit i
L0rr2(i) pnn(2) Refined Range using MLU mask, bit i
US, DS L0z sign bit: upstream, downstream
NG3 Number of photon clusters must be greater than 2
NG2 Number of photon clusters must be greater than or equal to 2
NTG Number of hit target elements
TBPS Trigger board by-16 prescaler; bypassable using EXTCON 24=H
RS OR of 6 hextant discriminators
prompt used to veto prompt IC-KB coincidence
L1.n L1.1 and/or L1.2
L1.1 TD area vs. height cut; select pion
L1.2 FERA energy cut in stopping HEX and Lay(n+1) and/or bad SCF and/or HEX afterburner

Notes:

— TB = trigger board and channel. Each board is numbered, channel: 0–5. — AO = and-or board channel = Lev 0 trigger bit: 0–15; or BD board channel — PS = prescaler board: 0–4 starting at right, and channel: 0–3. — the IC requirement was added to T•2 in 1996. — L0rr2 mask was all “pass” until 6/96; then cut NTG=15 only. — ( ) around TB-AO-PS means that slot is now used for something else. — pmm trigger has never been used in Trigger 2.

References:

— TB = TB2A logbook — Tn = Trigger 2 main logbook, volume n