TITLEDRAWINGNUMBERDATEDRAWNBYSCALE

Do Not Scale This DrawingCBH24 Feb 99DSP-008-BModifiedRingDetails1" = 3/8"Tolerances +/- (unless specified) x/x .x .xx .xxx angular1/64" .1" .01" .005" 1degSouthern California Integrated GPS Network Southern California Earthquake CenterLos Angeles, California 90089-0742http://www.scign.org/SCIGNRadomeDrawings

ModifiedRingDetails

AntennaDimensions(assumed range ofmanufacturer’sspecificationschoke R: 7.067"-7.085"flange R: 7.468"-7.505"flange dpth: 0.120"-0.140")Short Dome10-24 x 1" Torx HeadSS Flat Washer(11/16" OD.w/ 13/64" ID)ModifiedRingBase

TristarH-series insert1024X375C

Drill .252" D(+.003"/-.000")1� taperx .5" dp.Drill #11 (.191" D)thrucountersink 3/4" Dx .078" dp.