34 Pin Header

14 Pin HeaderWSTREQ

EDGE REGISTERD1-16WAK

TTL-ECL

ECL-TTL

TTL-NIM

4 Pin HeaderPASSRENEOED1-16MC10124MC10124MC10124-5.2V2K5656-1.2VRENPASSWST,REQ-5.2V470470CROS - DYC+ ADAPTER- 2V56D1-16-5.2V330180WST,REQPASS5656-1.2VMC10125MC10125MC10125RENDYC+MC10125MC10124470470-5.2V NOTES:1. CROS Adapter doesn’t use WAK as handshake signal 2. Pins polarity of REN has been changed on DYC+ output connector.<=1mCROS-DYC+ Communication. Status of October, 14