TITLEDRAWINGNUMBERDATEDRAWNBYSCALE

Do Not Scale This DrawingCBH25 Feb 99DSP-005BaseRing1" = 2.5"Tolerances +/- (unless specified) x/x .x .xx .xxx angular1/64" .1" .01" .005" 1deg

7.528"+.015-.015

8.145"+.015-.015 30�

.425"+.000-.010

9/16"7.085" R

1/8" RThese crush ribs are added8 places, (not whererunners come in)

Southern California Integrated GPS Network Southern California Earthquake CenterLos Angeles, California 90089-0742http://www.scign.org/SCIGNRadomeDrawingsDrill ’H’ thru(.266" D) 12 places@ 30� centerline of bolt holes(different from base plate)primaryoutside radiusat flange

8.003"+.015-.015outside radius, at centerline of bolt holes

7.100"+.020-.010Rinner radius of crush ribsat upper end

1�face anglesfrom underside of ring

Refer to Base Platefor furtherinformation

8.011"+.015-.015

90�15�Drill 3/16" D. thru(for pop rivets)4 places @ 90�.583" up from flange