PHENIX Note #255 addendum

A Comparison of Bicron BCF99-29A and BCF99-29AA WLS Fibers (addendum)

Sean P. Stoll PHENIX EMCal Collaboration Brookhaven National Laboratory

April 16, 1997

The light output of the production runs of wls fibers has been measured using the same method

(see Figure 1) described in the accompanying note. Fibers from the batches/runs #9990,

#11052, and #11097 were measured as standards with each group of measurements.

Quality Control/ Light Output Testing of Fiber Production Runs measurement date production date fiber type # measured average output relative to 9990

10-4-96 7-10-95 9990 T-4 BCF 99 29A 6 698 1.0

10-1-96 11052 T-1 29AA 6 716 + 3 %

12-18-96 7-10-95 9990 T-4 29A 2 689 - 1 %

10-1-96 11052 T-1 29AA 2 724 + 4 %

7-6-95 9951 T-3 29A 2 654 - 6 %

10-17-96 11080 T-3 29A 2 759 + 9 %

11-4-96 11097 T-3 29A 2 782 + 12 %

11-5-96 11098 T-3 29A 4 815 + 17 %

11-7-96 11099 T-3 29A 2 841 + 20 %

11-8-96 11100 T-3 29A 2 806 + 15 %

11-11-96 11101 T-3 29A 1 819 + 17 %

11-12-96 11102 T-3 29A 1 676 - 3 %

11-14-96 11103 T-3 29A 1 962 + 38 %

11-15-96 11104 T-1 29A 1 756 + 8 %

11-18-96 11105 T-3 29A 1 768 + 10 %

11-19-96 11106 T-3 29A 1 782 + 12 %

1-22-97 7-10-95 9990 T-4 29A 2 685 - 2 %

10-1-96 11052 T-1 29AA 4 729 + 4 %

7-6-95 9951 T-3 29A 2 585 - 16%

1-21-97 11151 T-3 29AA 8 513 - 27 %

2-18-97 7-6-95 9951 T-3 29A 1 168 - 12 %

7-10-95 9990 T-4 29A 6 192 1.0

10-1-96 11052 T-3 29AA 8 187 - 3 %

11-4-96 11097 T-3 29A 4 225 + 17 %

1-29-97 11158 T-1 29AA 6 192 1.0

* 1-29-97 11160 T-3 29AA 4 183 - 5 %

* 1-23-97 11162 T-S 29AA 6 183 - 5 %

1-29-97 11164 T-3 29AA 6 204 + 6 %

* 2-11-97 11172 T-3 29AA 4 215 + 12 %

* 2-12-97 11173 T-3 29AA 4 232 + 21 %

Quality Control/ Light Output Testing of Fiber Production Runs (continued)

measurement date production date fiber type # measured average output relative to 9990 3-18-97 7-6-95 9951 T-3 29A 1 104 - 18 % 7-10-95 9990 T-4 29A 4 127 1.00 10-1-96 11052 T-3 29AA 4 134 + 6 % 11-4-96 11097 T-3 29A 4 156 + 23 %

1-23-97 11158 T-1 29AA 6 150 + 18 % 11159 T-1 29AA 1 140 + 10 % 11160 T-3 29AA 5 144 + 13 % 11161 T-3 29AA 1 119 - 6 % 11162 T-5 29AA 1 142 + 12 % 11163 T-5 29AA 1 134 + 6 % 11164 T-3 29AA 2 144 + 13 % 11165 T-3 29AA 1 130 + 2 % 11167 T-1 29AA 1 140 + 10 % 11168 T-1 29AA 1 140 + 10 % 11169 T-5 29AA 1 135 + 6 % 11170 T-5 29AA 1 143 + 13 % 11171 T-3 29AA 1 173 + 36 % 11172 T-3 29AA 1 125 + 2 % 11173 T-3 29AA 1 152 + 20 %

Quality Control/ Light Output Testing of Fiber Production Runs (continued) measurement date production date fiber type # measured average output relative to

9990

4-10-97 7-10-95 9990 T-4 29A 6 154 1.00

4-11-97 10-1-96 11052 T-3 29AA 12 175 + 14 %

4-16-97 11-6-96 11097 T-3 29A 6 172 + 12 %

4-11-97 2-14-97 11174 T-1 29AA 3 195 + 27 %

2-21-97 11179 T-3 29AA 3 195 + 27 %

2-24-97 11180 T-3 29AA 6 187 + 11 %

2-25-97 11181 T-3 29AA 3 172 + 12 %

2-26-97 11182 T-3 29AA 3 182 + 19 %

2-27-97 11183 T-3 29AA 3 170 + 11 %

2-28-97 11184 T-3 29AA 3 195 + 27 %

3-24-97 11186 T-1 29AA 3 188 + 22 %

3-24-97 11187 T-1 29AA 3 178 + 16 %

3-24-97 11188 T-2 29AA 3 180 + 17 %

3-24-97 11189 T-2 29AA 3 170 + 11 %

3-24-97 11190 T-3 29AA 3 174 + 13 %

3-24-97 11191 T-3 29AA 3 176 + 15 %

4-14-97 3-25-97 11192 T-1 29AA 3 201 + 31 %

3-26-97 11193 T-1 29AA 3 197 + 28 %

3-25-97 11194 T-2 29AA 3 185 + 21 %

3-25-97 11195 T-3 29AA 3 172 + 12 %

3-26-97 11196 T-1 29AA 3 206 + 34 %

3-26-97 11197 T-1 29AA 3 180 + 17 %

3-26-97 11198 T-2 29AA 3 166 + 8 %

3-26-97 11199 T-2 29AA 3 195 + 27 %

3-26-97 11200 T-3 29AA 3 204 + 33 %

3-26-97 11201 T-3 29AA 3 186 + 21 %

3-26-97 11202 T-2 29AA 3 167 + 9 %

3-26-97 11203 T-3 29AA 3 188 + 22 %

5-27-97 4-1-97 11204 29AA 2 184 + 19 %

4-2-97 11205 29AA 2 196 + 27 %

4-1-97 11206 29AA 2 186 + 21 %

4-2-97 11207 29AA 2 181 + 18 %

4-1-97 11208 29AA 2 170 + 10 %

4-2-97 11209 29AA 2 169 + 10 %

4-3-97 11210 29AA 2 183 + 19 %

4-3-97 11212 29AA 4 196 + 27 %

4-3-97 11214 29AA 3 214 + 39 %

preform # Bicron meas. (rel to 11052)

BNL meas. (rel to 11052) 11158 + 3 % 11159 + 7 % 11160 + 3 % - 2 % 11161 + 3 % 11162 + 11 % - 2 % 11163 + 4 % 11164 + 7 % + 9 % 11165 - 7 % 11167 + 35 % 11168 + 33 % 11169 + 39 % 11170 + 25 % 11171 + 40 % 11172 + 42 % + 15 % 11173 + 5 % + 24 %

6