Table 1: T–counter efficiencies. Runs 44561–44580

T–counter N total N ineff. ϵ σ_ϵ 1 840 51 0.939 0.008 2 825 51 0.938 0.008 3 734 48 0.935 0.009 4 809 42 0.948 0.008 5 833 44 0.947 0.008 6^∗ 762 318 0.583 0.017 7 767 64 0.917 0.010 8 787 56 0.929 0.009 9 874 45 0.948 0.007 10 757 42 0.945 0.008 11^∗ 810 222 0.726 0.016 12 757 55 0.927 0.009 13 813 51 0.937 0.009 14 822 40 0.951 0.008 15 809 38 0.953 0.007 16 776 47 0.939 0.009 17 787 56 0.928 0.009 18 864 47 0.946 0.008 19 779 65 0.917 0.010 20 837 73 0.912 0.010 21 878 77 0.912 0.010 22 855 81 0.905 0.010 23 778 64 0.918 0.010 24 797 68 0.915 0.010

∗Known to be bad after intallation (broken fiber tailes)

Table 2: T–counter efficiencies. Runs 48991–49930

T–counter N total N ineff. ϵ σ_ϵ 1 379 35 0.908 0.015 2 375 31 0.917 0.014 3 375 43 0.885 0.016 4 382 51 0.867 0.017 5 383 49 0.872 0.017 6^∗ 336 42 0.875 0.018 7 319 68 0.824 0.019 8 357 45 0.874 0.018 9 411 42 0.898 0.015 10 366 29 0.921 0.014 11^∗ 365 32 0.912 0.015 12 307 54 0.850 0.019 13 374 49 0.869 0.017 14 330 30 0.909 0.016 15 366 51 0.861 0.018 16 339 25 0.926 0.014 17 357 39 0.891 0.017 18 388 48 0.876 0.017 19 334 37 0.889 0.017 20 318 40 0.888 0.017 21 389 44 0.887 0.016 22 381 58 0.848 0.018 23 359 42 0.883 0.017 24 347 44 0.873 0.018

∗Fixed by applying “or”–logic between T-counters ends

Figure 1: Efficiency distribution from Downstream to Upstream ends along Z axis for all T–counters. 1 horizontal axis tick is a number of T-counter. Length between two nearby ticks is the T-counter length which was scanned in 10 points with 5 cm step from -25 cm to 25 cm.

Figure 2: Angular (the angle at which width of T–counter is viewed from UTC) efficiency distribution. 1 horizontal axis tick is a number of T-counter. Length between two nearby ticks is a T-counter UTC angle from -0.13 to 0.13 rad. Efficiency was calculated in 10 points transverse each T–counter.

Figure 3: Angular events distribution summed over all T–counters. It shows that the most numbers of inefficient events are located near sector crossings in T–layer.

Figure 4: From Fig 1 7th T–counter shows low efficiency in Runs 48991–49930. Anyway, ADC signals of this counter seems to be OK.