10 T Super FOFO

Note This example cools to about the same minimum emittance as the standard 15 T alternating solenoid example, but uses only 10 T instead of 15 T. It also has less loss and seems altogether less sensitive.

But less of the length is full of rf, and as a result the rate of cooling as a function of distance is less.

len1 dl rad dr I/A m m m m A/mm^2 0.028 0.179 0.071 0.179 4 141.92 0.286 0.143 0.286 0.179 4 -132.22 0.507 0.179 0.071 0.179 4 141.92 0.714 0.000 0.071 0.071 1 0.00

Hydrogen 5 cm Al Window: 50 micron 3 cm rad Gap 20 cm 3 RF pillbox cavities

lengths 7.1 cm freq 805 MHz grad 36 MV/m windows 50 micron Be 5cm rad gap Al window

Note: The window thicknesses are arbitary radii (cm)

length (m)

0.00 0.25 0.50 0.75 1.00 1.25 0

10

20

30

40

+0 −141

+-132

−141 −0 +141

−-132

+141

Super FOFO 5 cm (79 fo1)

len (m) axial and dipole B (T)

0.0 0.5 1.0 1.5 2.0

-20

0

20 n/n = 990 / 1000

Super FOFO 5 cm (79 fo1)

len (m) rms rad (cm)

0 5 10 15 20 25 0.0

2.5

5.0

7.5

10.0

Super FOFO 5 cm (79 fo1) n/n = 990 / 1000

len (m) rms theta (mrad)

0 5 10 15 20 25 0

250

500

750

1000

Super FOFO 5 cm (79 fo1) n/n = 990 / 1000

rms corr momentum (%)

length (m)

0 5 10 15 20 25 0.0

2.5

5.0

7.5

10.0

•••••••••••••••••••••••••••••••••••••••••••••••••••••••••••••••••••••••••••••••• •••••••••••••••••••••••••••••••••••••••••••••••••••••••••••••••••••••••••••••••• rms (dash=rmcube) ct (cm)

length (cm)

Super FOFO 5 cm (79 fo1)

0 5 10 15 20 25 0

1

2

3

4

5 ct (cm)

length (m)

Super FOFO 5 cm (79 fo1)

0 5 10 15 20 25 30 -5

0

5

10

15

20

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

+

•

•

Super FOFO 5 cm (79 fo1)

n/n = 990 / 1000

len (m) rms emit norm x,y (ß mm mrad)

0 5 10 15 20 25 0

250

500

750

1000

• • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • •

∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘ ∘

Super FOFO 5 cm (79 fo1) n/n = 990 / 1000

long emit (pi mm)

length (m)

0 5 10 15 20 25

0.0 10^0

1.0 10^3

2.0 10^3

3.0 10^3

4.0 10^3

5.0 10^3

•••••••••••••••••••••••••••••••••••••••••••••••••••• •••••••••••••••••••••••••••••••• •••••••••••••••••••••••••••••••••••••••••••••••••••••••• ••••••••••••••••••••

Super FOFO 5 cm (79 fo1)

n/n = 990 / 1000

emit6 (10�^{12} (ß m)^3)

length (m)

0 5 10 15 20 25 0

500

1000

1500

2000

•••••••••••••••••••• ••••••••••••••••••• ••••••••••••••••••••• •••••••••••••••••••••••••••••••• •••••••••••••••••••• •••••••••••••••••••••••••••••••••••••••••••••••• loss %

length (m)

Super FOFO 5 cm (79 fo1) n/n = 990 / 1000

0 5 10 15 20 25

0.00

0.25

0.50

0.75

1.00

Super FOFO 5 cm (79 fo1) n/n = 990 / 1000

len (m) ave(blue) ref(red) mom (MeV/c)

0 5 10 15 20 25

180

190

200

210