Appendix_A_MCM_Channels.xls CFT Trigger Asymetric 10:39 AM on 11/25/98

LHB RHB Layer 68 Layer 68 Cassette Module MCM Cassette Module MCM A 32 A 32 32 32 32 32 1 64 68 0 1 64 68 0 32 32 32 36 B 32 B 48 0 0 16 12 2 64 2 64 48 4 48 0 C 48 C 48 0 44 0 48 68 1 68 1 16 24 0 8 D 64 D 48 48 40 48 40 3 64 68 2 3 64 68 2 16 28 16 28 E 64 E 64 48 36 48 36 4 64 68 3 4 64 68 3 16 32 16 32 F 64 F 80 48 32 64 48 5 64 68 4 5 64 68 4 16 36 0 20 G 80 G 80 6 64 64 44 6 64 64 60

0 16 7 64 68 5 7 64 68 5 64 24 48 8 H 96 H 80 32 72 32 72 8 64 72 6 8 64 72 6 32 32 PS 32 PS 32 0 64 0 64 64 7 64 7

The number of channels from layers B, D, F and H is exchanged between the LH and RH boards on a cassette to make the smalles cassette connector 16 channels. The bias splits at the D layer on the LHB and at the B layer on the RHB. The thresholds for both split in the D layer.

Figure A 1

Fred Borcherding_1

Appendix_A_MCM_Channels.xls CFT Stereo Asymetric 10:39 AM on 11/25/98

LHB RHB Layer 68 Layer 68 Cassette Module MCM Cassette Module MCM 1 - 32 32 ’1 - 32 32 32 32 32 32 1 64 68 0 1 64 68 0 32 32 32 36 33 - 64 32 33 - 80 48 0 0 16 12 2 64 2 64 48 4 48 0 65 - 112 48 81 - 128 48 0 44 0 48 68 1 68 1 16 24 0 8 113 - 176 64 129 - 176 48 48 40 48 40 3 64 68 2 3 64 68 2 16 28 16 28 177 - 240 64 177 - 240 64 48 36 48 36 4 64 68 3 4 64 68 3 16 32 16 32 241 - 256 241 - 256 1 - 48 64 1 - 64 80 48 32 64 48 5 64 68 4 5 64 68 4 16 36 0 20 49 - 128 80 65 - 144 80 6 64 64 44 6 64 64 60

0 16 7 64 68 5 7 64 68 5 64 24 48 8 129 - 224 96 145 - 224 80 32 72 32 72 8 64 72 6 8 64 72 6 32 32 225 - 256 32 225 - 256 32 0 32 0 32 32 7 32 7

The channel layout for the CFT Stereo Boards using the same board layout as the CFT Axial Trigger boards. The same board is used for the stereo. When it is stuffed the charge division for the 32 formerly PS channels is modified to non-charge division.

Figure A 2

Fred Borcherding_2

Appendix_A_MCM_Channels.xls FPS Trigger 10:39 AM on 11/25/98

Layer Cassette Module MCM L1 - U TH-1 The FPS has four thresholds 1 50 50 0.0 and four possible bias values 50 50 101 The Forward layers, L1 and L2 have NO charge splitting.

51 51 2 51 51 0.1 MCM # m.n means HDI # m and MCM/SVX # n

L2 - V

3 53 50 0.2 53 50 101 48 51 4 63 51 0.3 15

L3 - U TH-2 TH-3

5 64 67 0.4 67 1.4 64 67 135 56 68 6 63 68 0.5 68 1.5 7

L4 - V

7 64 67 0.6 67 1.6 64 67 135 64 68 8 64 68 0.7 68 1.7

472 Figure A 3

Fred Borcherding_3

Appendix_A_MCM_Channels.xls CPS Stereo 10:39 AM on 11/25/98

Layer

Cassette Module MCM MCM

TH-1 TH-3

The CPS Stereo has four

1 64 64 0.0 64 1.0 thresholds and four possible

64 64 bias values. 128 64 64

2 64 64 0.1 64 1.1 MCM # m.n means

HDI # m and MCM/SVX # n

3 64 64 0.2 64 1.2

64 64 128 64 64

4 64 64 0.3 64 1.3

TH-2 TH-4

5 64 64 0.4 64 1.4

64 64 128 64 64

6 64 64 0.5 64 1.5

7 64 64 0.6 64 1.6

64 64 128 64 64

8 64 64 0.7 64 1.7

512 Figure A 4

Fred Borcherding^4