TITLEDRAWINGNUMBERDATEDRAWNBYSCALE

Do Not Scale This DrawingCBH23 Feb 99DSP-007Fit Details1" = 3/8"Tolerances +/- (unless specified) x/x .x .xx .xxx angular1/64" .1" .01" .005" 1degSouthern California Integrated GPS Network Southern California Earthquake CenterLos Angeles, California 90089-0742http://www.scign.org/SCIGNRadomeDrawings

Tall Dome FitShort Dome Fit

.183"

.496"

.093"

.459"

.469"

8.178" R8.086" R7.528" R8.011" R8.066" R8.145" R

8.058" R8.078" R

.463"

.488"

.608"

.112"

.183"7.085" R7.100" R7.528" R8.011" R8.032" R8.145" R8.003" R8.024" R

8.174" R8.161" Rthickness 0.137"

.589"

8.259" R8.244" Rthickness 0.166" base platetall domeringshort dome