|  |
| --- |
| [MMI codes: support calling line identification presentation (+CLIP)](https://jirapdi.tid.es/browse/OWD-28089) |

|  |  |
| --- | --- |
|  **Description**   |   |

|  |
| --- |
| As a user I want to be able to know calling line identification presentation (+CLIP) status through MMI code |

|  |  |
| --- | --- |
| **Acceptance Criteria:** | * Query the current CLIP status entering through dialer ""\*#30#"" code:
	+ 1 for CLIP provisioned
	+ 0 for CLIP not provisioned
	+ 2 for unknown
* In case of 1, make a call, the called party receives the calling party's address information
* In case of 2, make a call, the called party doesn't receive the calling party's address information
 |