Punch list:

**(Priority I)**

* Finish all trim. (Cabinet crown, toe kick, center island & electrical outlet, countertop attachment.)
* Crown molding, (Type/Style needs to be verified by client.)
* Tile back-splash installation (Provided the client has purchased tiles….)
* Final electric[[1]](#footnote-1). (Momentum Electrical)

**(Priority II)**

* Dishwasher install and hook up (need to have replacement sink from client)

**(Priority III)**

* Paint & touch-up as and where needed.

**(Choice Priority)**

* Install crown molding over cabinet
* Install baseboard[[2]](#footnote-2) where needed in kitchen and on pony wall and adjacent wall stub.

\*Knobs on door frame edge, upper or lower corner as applicable, approximately 1 1/8" in from (centered) door frame edge. Handles in center of drawer center pane.

1. Install provided light-switches, outlets and plates. [↑](#footnote-ref-1)
2. Standard type big-box store (Home Despot) baseboard: LWM623 9/16 in. x 3-1/4 in. MDF Base Moulding [↑](#footnote-ref-2)