|  |
| --- |
| [MMI codes: support calling line identification presentation (+CLIP)](https://jirapdi.tid.es/browse/OWD-28089) |

|  |  |
| --- | --- |
| **Description** |  |

|  |
| --- |
| As a user I want to be able to know calling line identification presentation (+CLIP) status through MMI code |

|  |  |
| --- | --- |
| **Acceptance Criteria:** | * Query the current CLIP status entering through dialer ""\*#30#"" code:   + 1 for CLIP provisioned   + 0 for CLIP not provisioned   + 2 for unknown * In case of 1, make a call, the called party receives the calling party's address information * In case of 2, make a call, the called party doesn't receive the calling party's address information |