

Test weight  
= 10% content





**Incline Pendulum Steelyard Co2 cylinder weight monitoring device**

In the event of gas loss, the liquid level will be reduced lowering the cylinders  
centre of gravity urging the cylinder closer to the vertical and activating the limit switch

Hinged support for lifting cylinder into position

10% loss liquid level

Full liquid level

Co2 Cylinder suspended   
2⁰ off vertical

Limit switch