 Two Engine NP

Single Engine NP

Copilot

Flaps 5, Set Speed

Flaps 5, Set Speed

Flaps 1, Set Speed

Flaps 1, Set Speed

 Airplane

Deployed…Reversers Normal….60kts…Autobrake Disarm

When Cleared for Approach

LNAV/LOC

VNAV Cruise Page (alt matches & < 240kts)

VNAV

Altitude MCP (mins to next 100 Ft)

Missed Approach Altitude Set

Landing Checklist Complete

@ 300 Ft Below Missed Approach Altitude, Set Missed Approach

Altitude

@ 300 Ft Below Missed Approach Altitude

Set Missed Approach Altitude

Gear Down, Flaps 15, Set Speed, Landing Checklist

Flaps 30/40, Set speed, Complete Landing Checklist

Final Approach Course

Gear Down, Flaps 15, Set Speed, Landing Checklist to Flaps

**35**

**17**

Landing/Go Around

Landing/Go Around

@100 above

Approaching minimums

500 Ft

800 Ft

Minimums

1000 Ft

Missed approach altitude set

Landing Checklist Complete (2 engine & SE)

Cleared to Land (2 engine & SE)