1. Tracking for Virtual Set with Blui.i and encoded Vinten head

GATEWAY

RS232 or RS422 data converter for Virtual

Z-MODULE

Interface to Blue.i and measuring of height

HEAD ENCODING MODULE

Interface to encoded heads and lenses

Virtual Set PC

(RS232 or RS422)

Genlock

Blui.i Navigator

Encoded Head

Lens Encoders

(mechanical or serial)

PSU (12-32 Volt)

With Terminator

1. Tracking for Virtual Set with Blui.i and encoded head (Mo-Sys Bus + Vinten direct)

Encoded Head

Virtual Set PC

(RS232 or RS422)

Lens Encoders

(mechanical or serial)

Blui.i Navigator

Genlock

Vinten Encoding Box

Z-MODULE

Interface to Blue.i and measuring of height

GATEWAY

RS232 or RS422 data converter for Virtual

PSU (12-32 Volt)

With Terminator

1. Tracking for Virtual Set with Blui.i and e-Crane

Virtual Set PC

(RS232 or RS422)

Pan/Tilt

joy stick

Genlock

Lens Encoders

(mechanical or serial)

e-Crane Turn/Jib encoders

Blui.i Navigator

GATEWAY

RS232 or RS422 data converter for Virtual

OPERATING CONSOLE

REM 15 Remote Head

LENS ENCODING MODULE

E-CRANE MODULE

BLUE.I INTERFACE MODULE

Lens

Lens Controler

PSU (12-32 Volt)

With Terminator

1. Tracking for Virtual Set with Blui.i and e-Crane (mechanical cable version)

E-Crane Head

Virtual Set PC

(RS232 or RS422)

LENS eNCODER

Genlock

e-Crane Turn/Jib encoders

Blui.i Navigator

GATEWAY

RS232 or RS422 data converter for Virtual

HEAD/LENS ENCODING MODULE

E-CRANE MODULE

BLUE.I INTERFACE MODULE

Lens Controler

Lens

PSU (12-32 Volt)

With Terminator