1DISTRIBUTION FILES STRUCTURE02/02/99dist_strfmt.rtfStructure: sla02** Structure DATAMAJOR2, 6 tags, length=488: TPSTRUCT -> TIMEPN Array[1] RPSTRUCT -> RANGEPN Array[1] BPSTRUCT -> BOUNCPN Array[1] PAPSTRUCT -> POSSATTPN Array[1] EPSTRUCT -> ENGPN Array[1] WAVGRPSTRUCT -> FWAV Array[1]Structure: sla02.tp** Structure TIMEPN, 4 tags, length=32: MES DOUBLE LASTIMEDOUBLE SHUT_DIFFDOUBLE MES_CORRDOUBLEStructure: sla02.rp** Structure RANGEPN, 1 tags, length=8: RANGE_CORR DOUBLEStructure: sla02.bp** Structure BOUNCPN, 8 tags, length=64: LATDOUBLE LONDOUBLE ELLIP_HTDOUBLE SURFACE_1DOUBLE SURFACE_2DOUBLE SURFACE_3DOUBLE GEOIDDOUBLE ORTHO_HTDOUBLEStructure: sla02.pap** Structure POSSATTPN, 6 tags, length=48: SATHTDOUBLE ECFX_SHOTDOUBLE ECFY_SHOTDOUBLE ECFZ_SHOTDOUBLE AZIMUTHDOUBLE AOFFNADIRDOUBLE

2Structure: sla02.ep** Structure ENGPN, 12 tags, length=200: XMIT_ENBYTE Array[1] RECEIVE_ENBYTE Array[3] THRESHBYTE Array[3] CHANNELBYTE Array[1] WAVE_OFFSETBYTE Array[1] VGABYTE Array[1] DIGI_ATTENDOUBLE SCALE_FACTORDOUBLE PWIDTHBYTE Array[1] AVERAGEBYTE Array[1] BIN_SIZEDOUBLE WAVEFORMBYTE Array[150]********************************************************************************Waveform Parameters Structure:Structure: sla02.wavgrp** Structure FWAV, 5 tags, length=136: BL STRUCT -> BASLIN Array[1] WFSTRUCT -> WVFRM Array[1] ENSTRUCT -> ENVRN Array[1] CLSTRUCT -> CLASS Array[1] GMSTRUCT -> GMOD Array[1]Structure: sla02.wavgrp.bl** Structure BASLIN, 3 tags, length=12: NPOINTSINT MEANFLOAT SIGFLOATStructure: sla02.wavgrp.wf** Structure WVFRM, 8 tags, length=40: STARTINT NPOINTSINT MAXFLOAT WIDTHFLOAT AMPLITUDEFLOAT AREAFLOAT MMNTSTRUCT -> WMOM Array[1] NMAXFLOAT

3Structure: sla02.wavgrp.wf.mmnt** Structure WMOM, 4 tags, length=16: MEANFLOAT SIGFLOAT SKEWFLOAT KURTFLOATStructure: sla02.wavgrp.en** Structure ENVRN, 6 tags, length=24: DEMFLOAT NDVI1FLOAT NDVI2FLOAT LANDCOVERINT SLOPEFLOAT ROUGHNESSFLOATStructure: sla02.wavgrp.cl** Structure CLASS, 7 tags, length=24: RTYPINT STYPINT DTYPINT RMSFLOAT ASPECTFLOAT LP_CENTROIDFLOAT WV_CENTROIDFLOATStructure: sla02.wavgrp.gm** Structure GMOD, 6 tags, length=32: CFFLAGINT G0FLOAT G1FLOAT G2FLOAT CHISQDOUBLE NITRINT