Part Information | Outline Drawing | Introduction | Specifications | Ordering Information

Part Information:

Part Number: 425-3006-026 Description: .025" Loose pair Twist ’N’ Flat , 30 awg stranded, PVC, 26 conductors

Family: Internal Twisted Pair

Add to Information Request

Outline Drawing

Introduction

For internal single-ended or differential SCSI applications requiring twisted pairs, Spectra-Strip now offers mass termination on .025" centers with its new .025" Twist ’n’ Flat®. Unique in the industry, this is the only cable to offer programmable twist length sections (up to a maximum of 10) and loose, unbonded twisted pairs for a maximum in cable flexibility and improved airflow within the cabinet. Compared with traditional hand lamination methods, .025" Twist ’n’ Flat® affords considerable end product cost savings.

Benefits UL CSA Certified Offers reduced total assembly costs over current labor-intensive discrete or hand-lamination methods Up to ten twist length combinations are available Loose pairs between IDC flats allows increased airflow around the assembly Terminates to industry standard .025" IDC connectors Double-sided lamination provides excellent conductor strain relief

Specifications

Physical

Conductors 30 AWG 7/38 Strand, Tinned Copper

Color 1st Pair Red/Gray Followed by Blue Gray and Repeat

Insulation .006 PVC

Laminate Polyester

Temperature Rating 80°C

UL Style #20744 CSA AWM FT-1

Electrical

Impedance 90 + / - 6 ohms, single ended 122 + / - 10 ohms, differential

Capacitance 16.8 pf/ft Nom, single ended @ 1 MHz 12.0 pf/ft Nom, differentially @ 1 MHz

Propagation Delay 1.5 ns/ft Nom

Voltage Rating 150 volts

Current Rating 0.75 amp

DC Resistance 95 ohm/1,000’

Crosstalk see chart

Ordering Information

Width "A" Span "B"

Part Number No. Cond No. Pairs

Inches (mm) Inches (mm)

425-3006-010 10 5 .257 (6,53) .225 ± .010 (5,72 ± 0,25) 425-3006-014 14 7 .357 (9,07) .325 ± .010 (8,26 ± 0,25) 425-3006-016 16 8 .407 (10,34) .375 ± .010 (9,53 ± 0,25) 425-3006-020 20 10 .507 (12,88) .475 ± .010 (12,07 ± 0,25) 425-3006-026 26 13 .657 (16,69) .625 ± .010 (15,88 ± 0,25) 425-3006-034 34 17 .857 (21,77) .825 ± .010 (20,96 ± 0,25) 425-3006-036 36 18 .907 (23,04) .875 ± .010 (22,23 ± 0,25) 425-3006-040 40 20 1.007 (25,58) .975 ± .010 (24,77 ± 0,25) 425-3006-050 50 25 1.257 (31,93) 1.225 ± .010 (31,12 ± 0,25) 425-3006-060 60 30 1.507 (38,28) 1.475 ± .010 (37,47 ± 0,25) 425-3006-064 64 32 1.607 (40,82) 1.575 ± .010 (40,01 ± 0,25) 425-3006-068 68 34 1.707 (43,36) 1.675 ± .010 (42,55 ± 0,25) 425-3006-080 80 40 2.007 (50,98) 1.975 ± .010 (50,17 ± 0,25) 425-3006-100 100 50 2.507 (63,68) 2.475 ± .010 (62,87 ± 0,25)